{"text_format":"3","workbook":"xls","n_sheets":6,"sheets":["2级单相智能电能表","1级三相智能电能表","0.5S级三相智能电能表","0.2S级三相智能电能表","集中器、采集器","专变采集终端"],"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"2级单相智能电能表","index":0,"n_rows":389,"n_cols":9,"rows_kept":389,"merged":[[0,0,0,8],[1,0,1,8],[3,0,23,0],[24,0,64,0],[65,0,70,0],[71,0,76,0],[77,0,85,0],[86,0,94,0],[98,0,114,0],[115,0,120,0],[122,0,125,0],[126,0,128,0],[129,0,131,0],[132,0,134,0],[135,0,137,0],[138,0,145,0],[146,0,147,0],[155,0,160,0],[162,0,163,0],[164,0,174,0],[175,0,183,0],[184,0,206,0],[207,0,209,0],[210,0,212,0],[213,0,214,0],[215,0,216,0],[217,0,218,0],[219,0,220,0],[221,0,224,0],[225,0,233,0],[234,0,239,0],[240,0,362,0],[365,0,367,0],[368,0,378,0],[379,0,380,0],[381,0,388,0]],"flags":["formulas_cached_only"]}
["国家电网公司2017年第一次电能表及用电信息采集设备招标活动\n货物需求一览表\n(2级单相智能电能表)"]
["分标编号:0711-17OTL03922000-1"]
["包号","项目单位","项目名称","招标货物","物资描述","单位","行数量","交货日期","交货地点"]
["包01GW1","上海市电力公司","国网上海公司2017年第一次电能表（含用电信息采集）项目","单相计量故障识别模块","现场作业终端外设-采集故障识别模块:无,计量故障识别模块:单相,超高频RFID模块:无,蓝牙打印模块:无","个","150","2018-04-30","买方指定仓库车板交货"]
[null,"上海市电力公司","国网上海公司2017年第一次电能表（含用电信息采集）项目","2级单相费控智能电能表（模块-远程-开关内置）","单相智能电能表-准确度等级:2级,费控方式:远程,负荷开关:内置,通信模块接口:有,电压规格:220V,电流规格:5A","只","250000","2018-04-30","买方指定仓库车板交货"]
[null,"上海市电力公司","国网上海公司2017年第一次电能表（含用电信息采集）项目","采集故障识别模块","现场作业终端外设-采集故障识别模块:有,计量故障识别模块:无,超高频RFID模块:无,蓝牙打印模块:无","个","150","2018-04-30","买方指定仓库车板交货"]
[null,"上海市电力公司","国网上海公司2017年第一次电能表（含用电信息采集）项目","计量现场作业终端与外设收纳箱","现场作业终端与外设收纳箱-存放外设个数:3","个","150","2018-04-30","买方指定仓库车板交货"]
[null,"上海市电力公司","国网上海公司2017年第一次电能表（含用电信息采集）项目","超高频RFID模块","现场作业终端外设-采集故障识别模块:无,计量故障识别模块:无,超高频RFID模块:有,蓝牙打印模块:无","个","10","2018-04-30","买方指定仓库车板交货"]
[null,"天津市电力公司","","2级单相表本地通信单元（窄带）","通信单元-通信单元类别:本地,适用终端/表类型:2级单相表,通信方式:窄带载波,频率范围/中心频率:421kHz,调制方式:BFSK","只","880","2017-12-31","买方指定仓库地面交货"]
[null,"冀北电力有限公司","","计量现场作业终端","现场作业终端-屏幕尺寸范围:≤4.0英寸,购电卡接口:有","台","881","2017-12-31","买方指定仓库地面交货"]
[null,"冀北电力有限公司","","三相计量故障识别模块","现场作业终端外设-采集故障识别模块:无,计量故障识别模块:三相,超高频RFID模块:无,蓝牙打印模块:无","个","87","2017-12-31","买方指定仓库地面交货"]
[null,"冀北电力有限公司","","计量现场作业终端与外设收纳箱","现场作业终端与外设收纳箱-存放外设个数:4","个","68","2017-12-31","买方指定仓库地面交货"]
[null,"冀北电力有限公司","","采集故障识别模块","现场作业终端外设-采集故障识别模块:有,计量故障识别模块:无,超高频RFID模块:无,蓝牙打印模块:无","个","88","2017-12-31","买方指定仓库地面交货"]
[null,"湖南省电力公司","","三相计量故障识别模块","现场作业终端外设-采集故障识别模块:无,计量故障识别模块:三相,超高频RFID模块:无,蓝牙打印模块:无","个","200","2018-05-31","买方指定仓库车板交货"]
[null,"湖南省电力公司","","单相计量故障识别模块","现场作业终端外设-采集故障识别模块:无,计量故障识别模块:单相,超高频RFID模块:无,蓝牙打印模块:无","个","1200","2018-05-31","买方指定仓库车板交货"]
[null,"西藏电力有限公司","国网西藏电力有限公司各供电公司营销专项、电网基建/户表","2级单相费控智能电能表（模块-远程-开关内置）","单相智能电能表-准确度等级:2级,费控方式:远程,负荷开关:内置,通信模块接口:有,电压规格:220V,电流规格:5A","只","20545","2017-06-30","买方指定仓库地面交货"]
[null,"湖南省电力公司","","采集故障识别模块","现场作业终端外设-采集故障识别模块:有,计量故障识别模块:无,超高频RFID模块:无,蓝牙打印模块:无","个","1400","2018-05-31","买方指定仓库车板交货"]
[null,"天津市电力公司","","2级单相费控智能电能表（模块-远程-开关内置）","单相智能电能表-准确度等级:2级,费控方式:远程,负荷开关:内置,通信模块接口:有,电压规格:220V,电流规格:5A","只","2000","2017-12-31","买方指定仓库地面交货"]
[null,"天津市电力公司","","2级单相表本地通信单元（窄带）","通信单元-通信单元类别:本地,适用终端/表类型:2级单相表,通信方式:窄带载波,频率范围/中心频率:其他,调制方式:其他","只","420","2017-12-31","买方指定仓库地面交货"]
[null,"天津市电力公司","","2级单相表本地通信单元（窄带）","通信单元-通信单元类别:本地,适用终端/表类型:2级单相表,通信方式:窄带载波,频率范围/中心频率:270kHz,调制方式:BFSK","只","700","2017-12-31","买方指定仓库地面交货"]
[null,"冀北电力有限公司","","单相计量故障识别模块","现场作业终端外设-采集故障识别模块:无,计量故障识别模块:单相,超高频RFID模块:无,蓝牙打印模块:无","个","88","2017-12-31","买方指定仓库地面交货"]
[null,"西藏电力有限公司","国网西藏电力有限公司各供电公司营销专项、电网基建/户表","2级单相表本地通信单元（微功率）","通信单元-通信单元类别:本地,适用终端/表类型:2级单相表,通信方式:微功率,频率范围/中心频率:470～510MHz,调制方式:GFSK","只","5000","2017-07-30","买方指定仓库地面交货"]
[null,"西藏电力有限公司","国网西藏电力有限公司各供电公司营销专项、电网基建/户表","2级单相表本地通信单元（窄带）","通信单元-通信单元类别:本地,适用终端/表类型:2级单相表,通信方式:窄带载波,频率范围/中心频率:421kHz,调制方式:BFSK","只","29301","2017-07-30","买方指定仓库地面交货"]
[null,"上海市电力公司","国网上海公司2017年第一次电能表（含用电信息采集）项目","计量现场作业终端","现场作业终端-屏幕尺寸范围:≤4.0英寸,购电卡接口:无","台","150","2018-04-30","买方指定仓库车板交货"]
["包01GW2","内蒙古东部电力有限公司","","2级单相表本地通信单元（窄带）","通信单元-通信单元类别:本地,适用终端/表类型:2级单相表,通信方式:窄带载波,频率范围/中心频率:421kHz,调制方式:BFSK","只","500","2017-12-31","买方指定仓库地面交货"]
[null,"内蒙古东部电力有限公司","","2级单相表本地通信单元（宽带）","通信单元-通信单元类别:本地,适用终端/表类型:2级单相表,通信方式:宽带载波,频率范围/中心频率:2～12MHz,调制方式:OFDM","只","6000","2017-12-31","买方指定仓库地面交货"]
[null,"内蒙古东部电力有限公司","","2级单相表本地通信单元（窄带）","通信单元-通信单元类别:本地,适用终端/表类型:2级单相表,通信方式:窄带载波,频率范围/中心频率:其他,调制方式:其他","只","4855","2017-12-31","买方指定仓库地面交货"]
[null,"内蒙古东部电力有限公司","","2级单相表本地通信单元（窄带）","通信单元-通信单元类别:本地,适用终端/表类型:2级单相表,通信方式:窄带载波,频率范围/中心频率:421kHz,调制方式:BFSK","只","3100","2017-12-31","买方指定仓库地面交货"]
[null,"内蒙古东部电力有限公司","","2级单相表本地通信单元（窄带）","通信单元-通信单元类别:本地,适用终端/表类型:2级单相表,通信方式:窄带载波,频率范围/中心频率:270kHz,调制方式:BFSK","只","400","2017-12-31","买方指定仓库地面交货"]
[null,"内蒙古东部电力有限公司","","2级单相表本地通信单元（窄带）","通信单元-通信单元类别:本地,适用终端/表类型:2级单相表,通信方式:窄带载波,频率范围/中心频率:270kHz,调制方式:BFSK","只","1208","2017-12-31","买方指定仓库地面交货"]
[null,"内蒙古东部电力有限公司","","2级单相表本地通信单元（窄带）","通信单元-通信单元类别:本地,适用终端/表类型:2级单相表,通信方式:窄带载波,频率范围/中心频率:421kHz,调制方式:BFSK","只","1188","2017-12-31","买方指定仓库地面交货"]
[null,"内蒙古东部电力有限公司","","2级单相表本地通信单元（窄带）","通信单元-通信单元类别:本地,适用终端/表类型:2级单相表,通信方式:窄带载波,频率范围/中心频率:270kHz,调制方式:BFSK","只","500","2017-12-31","买方指定仓库地面交货"]
[null,"内蒙古东部电力有限公司","","2级单相表本地通信单元（窄带）","通信单元-通信单元类别:本地,适用终端/表类型:2级单相表,通信方式:窄带载波,频率范围/中心频率:421kHz,调制方式:BFSK","只","500","2017-12-31","买方指定仓库地面交货"]
[null,"内蒙古东部电力有限公司","","2级单相表本地通信单元（窄带）","通信单元-通信单元类别:本地,适用终端/表类型:2级单相表,通信方式:窄带载波,频率范围/中心频率:300kHz,调制方式:BPSK","只","22820","2017-12-31","买方指定仓库地面交货"]
[null,"内蒙古东部电力有限公司","","2级单相表本地通信单元（窄带）","通信单元-通信单元类别:本地,适用终端/表类型:2级单相表,通信方式:窄带载波,频率范围/中心频率:421kHz,调制方式:BFSK","只","700","2017-12-31","买方指定仓库地面交货"]
[null,"黑龙江省电力有限公司","","计量现场作业终端","现场作业终端-屏幕尺寸范围:≥7.0英寸,购电卡接口:无","台","1200","2018-04-20","买方指定仓库地面交货"]
[null,"黑龙江省电力有限公司","","2级单相表本地通信单元（窄带）","通信单元-通信单元类别:本地,适用终端/表类型:2级单相表,通信方式:窄带载波,频率范围/中心频率:421kHz,调制方式:BFSK","只","129392","2018-04-20","买方指定仓库地面交货"]
[null,"黑龙江省电力有限公司","","2级单相表本地通信单元（窄带）","通信单元-通信单元类别:本地,适用终端/表类型:2级单相表,通信方式:窄带载波,频率范围/中心频率:270kHz,调制方式:BFSK","只","13821","2018-04-20","买方指定仓库地面交货"]
[null,"黑龙江省电力有限公司","","2级单相表本地通信单元（宽带）","通信单元-通信单元类别:本地,适用终端/表类型:2级单相表,通信方式:宽带载波,频率范围/中心频率:2～12MHz,调制方式:OFDM","只","5701","2018-04-20","买方指定仓库地面交货"]
[null,"黑龙江省电力有限公司","","2级单相费控智能电能表（模块-远程-开关内置）","单相智能电能表-准确度等级:2级,费控方式:远程,负荷开关:内置,通信模块接口:有,电压规格:220V,电流规格:5A","只","150000","2018-04-20","买方指定仓库地面交货"]
[null,"黑龙江省电力有限公司","","采集故障识别模块","现场作业终端外设-采集故障识别模块:有,计量故障识别模块:无,超高频RFID模块:无,蓝牙打印模块:无","个","120","2018-04-20","买方指定仓库地面交货"]
[null,"内蒙古东部电力有限公司","","2级单相费控智能电能表（模块-远程-开关内置）","单相智能电能表-准确度等级:2级,费控方式:远程,负荷开关:内置,通信模块接口:有,电压规格:220V,电流规格:5A","只","150","2017-12-31","买方指定仓库地面交货"]
[null,"内蒙古东部电力有限公司","","2级单相费控智能电能表（模块-远程-开关内置）","单相智能电能表-准确度等级:2级,费控方式:远程,负荷开关:内置,通信模块接口:有,电压规格:220V,电流规格:5A","只","51954","2017-12-31","买方指定仓库地面交货"]
[null,"内蒙古东部电力有限公司","","2级单相费控智能电能表（模块-远程-开关内置）","单相智能电能表-准确度等级:2级,费控方式:远程,负荷开关:内置,通信模块接口:有,电压规格:220V,电流规格:5A","只","299","2017-12-31","买方指定仓库地面交货"]
[null,"内蒙古东部电力有限公司","","2级单相费控智能电能表（模块-远程-开关内置）","单相智能电能表-准确度等级:2级,费控方式:远程,负荷开关:内置,通信模块接口:有,电压规格:220V,电流规格:5A","只","1010","2017-12-31","买方指定仓库地面交货"]
[null,"内蒙古东部电力有限公司","","2级单相费控智能电能表（模块-远程-开关内置）","单相智能电能表-准确度等级:2级,费控方式:远程,负荷开关:内置,通信模块接口:有,电压规格:220V,电流规格:5A","只","94608","2017-12-31","买方指定仓库地面交货"]
[null,"内蒙古东部电力有限公司","","2级单相费控智能电能表（模块-远程-开关内置）","单相智能电能表-准确度等级:2级,费控方式:远程,负荷开关:内置,通信模块接口:有,电压规格:220V,电流规格:5A","只","6000","2017-12-31","买方指定仓库地面交货"]
[null,"内蒙古东部电力有限公司","","2级单相费控智能电能表（模块-远程-开关内置）","单相智能电能表-准确度等级:2级,费控方式:远程,负荷开关:内置,通信模块接口:有,电压规格:220V,电流规格:5A","只","2000","2017-12-31","买方指定仓库地面交货"]
[null,"内蒙古东部电力有限公司","","2级单相费控智能电能表（模块-远程-开关内置）","单相智能电能表-准确度等级:2级,费控方式:远程,负荷开关:内置,通信模块接口:有,电压规格:220V,电流规格:5A","只","100","2017-12-31","买方指定仓库地面交货"]
[null,"内蒙古东部电力有限公司","","2级单相费控智能电能表（模块-远程-开关内置）","单相智能电能表-准确度等级:2级,费控方式:远程,负荷开关:内置,通信模块接口:有,电压规格:220V,电流规格:5A","只","1131","2017-12-31","买方指定仓库地面交货"]
[null,"内蒙古东部电力有限公司","","2级单相表本地通信单元（窄带）","通信单元-通信单元类别:本地,适用终端/表类型:2级单相表,通信方式:窄带载波,频率范围/中心频率:421kHz,调制方式:BFSK","只","1060","2017-12-31","买方指定仓库地面交货"]
[null,"内蒙古东部电力有限公司","","2级单相表本地通信单元（窄带）","通信单元-通信单元类别:本地,适用终端/表类型:2级单相表,通信方式:窄带载波,频率范围/中心频率:其他,调制方式:其他","只","8698","2017-12-31","买方指定仓库地面交货"]
[null,"内蒙古东部电力有限公司","","2级单相表本地通信单元（宽带）","通信单元-通信单元类别:本地,适用终端/表类型:2级单相表,通信方式:宽带载波,频率范围/中心频率:2～12MHz,调制方式:OFDM","只","5775","2017-12-31","买方指定仓库地面交货"]
[null,"内蒙古东部电力有限公司","","2级单相表本地通信单元（窄带）","通信单元-通信单元类别:本地,适用终端/表类型:2级单相表,通信方式:窄带载波,频率范围/中心频率:其他,调制方式:其他","只","79","2017-12-31","买方指定仓库地面交货"]
[null,"内蒙古东部电力有限公司","","2级单相表本地通信单元（窄带）","通信单元-通信单元类别:本地,适用终端/表类型:2级单相表,通信方式:窄带载波,频率范围/中心频率:421kHz,调制方式:BFSK","只","500","2017-12-31","买方指定仓库地面交货"]
[null,"内蒙古东部电力有限公司","","2级单相表本地通信单元（窄带）","通信单元-通信单元类别:本地,适用终端/表类型:2级单相表,通信方式:窄带载波,频率范围/中心频率:421kHz,调制方式:BFSK","只","1000","2017-12-31","买方指定仓库地面交货"]
[null,"内蒙古东部电力有限公司","","2级单相表本地通信单元（窄带）","通信单元-通信单元类别:本地,适用终端/表类型:2级单相表,通信方式:窄带载波,频率范围/中心频率:270kHz,调制方式:BFSK","只","200","2017-12-31","买方指定仓库地面交货"]
[null,"内蒙古东部电力有限公司","","2级单相表本地通信单元（宽带）","通信单元-通信单元类别:本地,适用终端/表类型:2级单相表,通信方式:宽带载波,频率范围/中心频率:2～12MHz,调制方式:OFDM","只","3000","2017-12-31","买方指定仓库地面交货"]
[null,"内蒙古东部电力有限公司","","2级单相表本地通信单元（宽带）","通信单元-通信单元类别:本地,适用终端/表类型:2级单相表,通信方式:宽带载波,频率范围/中心频率:2～12MHz,调制方式:OFDM","只","82924","2017-12-31","买方指定仓库地面交货"]
[null,"内蒙古东部电力有限公司","","2级单相表本地通信单元（窄带）","通信单元-通信单元类别:本地,适用终端/表类型:2级单相表,通信方式:窄带载波,频率范围/中心频率:421kHz,调制方式:BFSK","只","12881","2017-12-31","买方指定仓库地面交货"]
[null,"内蒙古东部电力有限公司","","2级单相表本地通信单元（窄带）","通信单元-通信单元类别:本地,适用终端/表类型:2级单相表,通信方式:窄带载波,频率范围/中心频率:270kHz,调制方式:BFSK","只","2398","2017-12-31","买方指定仓库地面交货"]
[null,"内蒙古东部电力有限公司","","2级单相表本地通信单元（窄带）","通信单元-通信单元类别:本地,适用终端/表类型:2级单相表,通信方式:窄带载波,频率范围/中心频率:132kHz,调制方式:BPSK","只","1137","2017-12-31","买方指定仓库地面交货"]
[null,"内蒙古东部电力有限公司","","2级单相表本地通信单元（宽带）","通信单元-通信单元类别:本地,适用终端/表类型:2级单相表,通信方式:宽带载波,频率范围/中心频率:2～12MHz,调制方式:OFDM","只","1333","2017-12-31","买方指定仓库地面交货"]
[null,"内蒙古东部电力有限公司","","2级单相表本地通信单元（窄带）","通信单元-通信单元类别:本地,适用终端/表类型:2级单相表,通信方式:窄带载波,频率范围/中心频率:421kHz,调制方式:BFSK","只","150","2017-12-31","买方指定仓库地面交货"]
[null,"内蒙古东部电力有限公司","","2级单相表本地通信单元（宽带）","通信单元-通信单元类别:本地,适用终端/表类型:2级单相表,通信方式:宽带载波,频率范围/中心频率:2～12MHz,调制方式:OFDM","只","200","2017-12-31","买方指定仓库地面交货"]
["包01FJ2","福建省电力有限公司","国网福建省电力有限公司采购","2级单相费控智能电能表（模块-远程-开关内置）","单相智能电能表-准确度等级:2级,费控方式:远程,负荷开关:内置,通信模块接口:有,电压规格:220V,电流规格:5A","只","350000","2018-06-30","买方指定仓库地面交货"]
[null,"福建省电力有限公司","国网福建省电力有限公司采购","2级单相表本地通信单元（窄带）","通信单元-通信单元类别:本地,适用终端/表类型:2级单相表,通信方式:窄带载波,频率范围/中心频率:132kHz,调制方式:BPSK","只","4861","2018-06-30","买方指定仓库地面交货"]
[null,"福建省电力有限公司","国网福建省电力有限公司采购","2级单相表本地通信单元（宽带）","通信单元-通信单元类别:本地,适用终端/表类型:2级单相表,通信方式:宽带载波,频率范围/中心频率:2～12MHz,调制方式:OFDM","只","48612","2018-06-30","买方指定仓库地面交货"]
[null,"福建省电力有限公司","国网福建省电力有限公司采购","2级单相表本地通信单元（窄带）","通信单元-通信单元类别:本地,适用终端/表类型:2级单相表,通信方式:窄带载波,频率范围/中心频率:421kHz,调制方式:BFSK","只","9722","2018-06-30","买方指定仓库地面交货"]
[null,"福建省电力有限公司","国网福建省电力有限公司采购","2级单相表本地通信单元（窄带）","通信单元-通信单元类别:本地,适用终端/表类型:2级单相表,通信方式:窄带载波,频率范围/中心频率:其他,调制方式:其他","只","43750","2018-06-30","买方指定仓库地面交货"]
[null,"福建省电力有限公司","国网福建省电力有限公司采购","2级单相表本地通信单元（窄带）","通信单元-通信单元类别:本地,适用终端/表类型:2级单相表,通信方式:窄带载波,频率范围/中心频率:270kHz,调制方式:BFSK","只","243055","2018-06-30","买方指定仓库地面交货"]
["包01FJ3","福建省电力有限公司","国网福建省电力有限公司采购","2级单相费控智能电能表（模块-远程-开关内置）","单相智能电能表-准确度等级:2级,费控方式:远程,负荷开关:内置,通信模块接口:有,电压规格:220V,电流规格:5A","只","280000","2018-06-30","买方指定仓库地面交货"]
[null,"福建省电力有限公司","国网福建省电力有限公司采购","2级单相表本地通信单元（窄带）","通信单元-通信单元类别:本地,适用终端/表类型:2级单相表,通信方式:窄带载波,频率范围/中心频率:270kHz,调制方式:BFSK","只","194445","2018-06-30","买方指定仓库地面交货"]
[null,"福建省电力有限公司","国网福建省电力有限公司采购","2级单相表本地通信单元（宽带）","通信单元-通信单元类别:本地,适用终端/表类型:2级单相表,通信方式:宽带载波,频率范围/中心频率:2～12MHz,调制方式:OFDM","只","38888","2018-06-30","买方指定仓库地面交货"]
[null,"福建省电力有限公司","国网福建省电力有限公司采购","2级单相表本地通信单元（窄带）","通信单元-通信单元类别:本地,适用终端/表类型:2级单相表,通信方式:窄带载波,频率范围/中心频率:其他,调制方式:其他","只","35000","2018-06-30","买方指定仓库地面交货"]
[null,"福建省电力有限公司","国网福建省电力有限公司采购","2级单相表本地通信单元（窄带）","通信单元-通信单元类别:本地,适用终端/表类型:2级单相表,通信方式:窄带载波,频率范围/中心频率:421kHz,调制方式:BFSK","只","7778","2018-06-30","买方指定仓库地面交货"]
[null,"福建省电力有限公司","国网福建省电力有限公司采购","2级单相表本地通信单元（窄带）","通信单元-通信单元类别:本地,适用终端/表类型:2级单相表,通信方式:窄带载波,频率范围/中心频率:132kHz,调制方式:BPSK","只","3889","2018-06-30","买方指定仓库地面交货"]
["包01HB1","湖北省电力公司","","超高频RFID模块","现场作业终端外设-采集故障识别模块:无,计量故障识别模块:无,超高频RFID模块:有,蓝牙打印模块:无","个","15","2017-07-31","买方指定仓库地面交货"]
[null,"湖北省电力公司","","单相计量故障识别模块","现场作业终端外设-采集故障识别模块:无,计量故障识别模块:单相,超高频RFID模块:无,蓝牙打印模块:无","个","15","2017-07-31","买方指定仓库地面交货"]
[null,"湖北省电力公司","","计量现场作业终端","现场作业终端-屏幕尺寸范围:(4.0～7.0)英寸,购电卡接口:无","台","15","2017-07-31","买方指定仓库地面交货"]
[null,"湖北省电力公司","","计量现场作业终端","现场作业终端-屏幕尺寸范围:≥7.0英寸,购电卡接口:无","台","15","2017-07-31","买方指定仓库地面交货"]
[null,"湖北省电力公司","","现场打印模块","现场作业终端外设-采集故障识别模块:无,计量故障识别模块:无,超高频RFID模块:无,蓝牙打印模块:有","个","15","2017-07-31","买方指定仓库地面交货"]
[null,"湖北省电力公司","","采集故障识别模块","现场作业终端外设-采集故障识别模块:有,计量故障识别模块:无,超高频RFID模块:无,蓝牙打印模块:无","个","15","2017-07-31","买方指定仓库地面交货"]
[null,"湖北省电力公司","","2级单相费控智能电能表（模块-远程-开关内置）","单相智能电能表-准确度等级:2级,费控方式:远程,负荷开关:内置,通信模块接口:有,电压规格:220V,电流规格:5A","只","500000","2017-07-31","买方指定仓库地面交货"]
[null,"湖北省电力公司","","计量现场作业终端","现场作业终端-屏幕尺寸范围:≤4.0英寸,购电卡接口:无","台","15","2017-07-31","买方指定仓库地面交货"]
[null,"湖北省电力公司","","三相计量故障识别模块","现场作业终端外设-采集故障识别模块:无,计量故障识别模块:三相,超高频RFID模块:无,蓝牙打印模块:无","个","15","2017-07-31","买方指定仓库地面交货"]
["包01HB2","湖北省电力公司","","计量现场作业终端","现场作业终端-屏幕尺寸范围:≥7.0英寸,购电卡接口:无","台","15","2017-07-31","买方指定仓库地面交货"]
[null,"湖北省电力公司","","三相计量故障识别模块","现场作业终端外设-采集故障识别模块:无,计量故障识别模块:三相,超高频RFID模块:无,蓝牙打印模块:无","个","15","2017-07-31","买方指定仓库地面交货"]
[null,"湖北省电力公司","","超高频RFID模块","现场作业终端外设-采集故障识别模块:无,计量故障识别模块:无,超高频RFID模块:有,蓝牙打印模块:无","个","15","2017-07-31","买方指定仓库地面交货"]
[null,"湖北省电力公司","","单相计量故障识别模块","现场作业终端外设-采集故障识别模块:无,计量故障识别模块:单相,超高频RFID模块:无,蓝牙打印模块:无","个","15","2017-07-31","买方指定仓库地面交货"]
[null,"湖北省电力公司","","计量现场作业终端","现场作业终端-屏幕尺寸范围:(4.0～7.0)英寸,购电卡接口:无","台","15","2017-07-31","买方指定仓库地面交货"]
[null,"湖北省电力公司","","计量现场作业终端","现场作业终端-屏幕尺寸范围:≤4.0英寸,购电卡接口:无","台","15","2017-07-31","买方指定仓库地面交货"]
[null,"湖北省电力公司","","2级单相费控智能电能表（模块-远程-开关内置）","单相智能电能表-准确度等级:2级,费控方式:远程,负荷开关:内置,通信模块接口:有,电压规格:220V,电流规格:5A","只","450000","2017-07-31","买方指定仓库地面交货"]
[null,"湖北省电力公司","","现场打印模块","现场作业终端外设-采集故障识别模块:无,计量故障识别模块:无,超高频RFID模块:无,蓝牙打印模块:有","个","15","2017-07-31","买方指定仓库地面交货"]
[null,"湖北省电力公司","","采集故障识别模块","现场作业终端外设-采集故障识别模块:有,计量故障识别模块:无,超高频RFID模块:无,蓝牙打印模块:无","个","15","2017-07-31","买方指定仓库地面交货"]
["包01HB3","湖北省电力公司","","2级单相费控智能电能表（模块-远程-开关内置）","单相智能电能表-准确度等级:2级,费控方式:远程,负荷开关:内置,通信模块接口:有,电压规格:220V,电流规格:5A","只","450000","2017-07-31","买方指定仓库地面交货"]
["包01HB4","湖北省电力公司","","2级单相费控智能电能表（模块-远程-开关内置）","单相智能电能表-准确度等级:2级,费控方式:远程,负荷开关:内置,通信模块接口:有,电压规格:220V,电流规格:5A","只","350000","2017-07-31","买方指定仓库地面交货"]
["包01HB5","湖北省电力公司","","2级单相费控智能电能表（模块-远程-开关内置）","单相智能电能表-准确度等级:2级,费控方式:远程,负荷开关:内置,通信模块接口:有,电压规格:220V,电流规格:5A","只","250000","2017-07-31","买方指定仓库地面交货"]
["包01MD1","内蒙古东部电力有限公司","","2级单相费控智能电能表（模块-远程-开关内置）","单相智能电能表-准确度等级:2级,费控方式:远程,负荷开关:内置,通信模块接口:有,电压规格:220V,电流规格:5A","只","5500","2017-12-31","买方指定仓库地面交货"]
[null,"内蒙古东部电力有限公司","","2级单相费控智能电能表（模块-远程-开关内置）","单相智能电能表-准确度等级:2级,费控方式:远程,负荷开关:内置,通信模块接口:有,电压规格:220V,电流规格:5A","只","79","2017-12-31","买方指定仓库地面交货"]
[null,"内蒙古东部电力有限公司","","2级单相费控智能电能表（模块-远程-开关内置）","单相智能电能表-准确度等级:2级,费控方式:远程,负荷开关:内置,通信模块接口:有,电压规格:220V,电流规格:5A","只","11981","2017-12-31","买方指定仓库地面交货"]
[null,"内蒙古东部电力有限公司","","2级单相费控智能电能表（模块-远程-开关内置）","单相智能电能表-准确度等级:2级,费控方式:远程,负荷开关:内置,通信模块接口:有,电压规格:220V,电流规格:5A","只","1333","2017-12-31","买方指定仓库地面交货"]
[null,"内蒙古东部电力有限公司","","2级单相表本地通信单元（宽带）","通信单元-通信单元类别:本地,适用终端/表类型:2级单相表,通信方式:宽带载波,频率范围/中心频率:2～12MHz,调制方式:OFDM","只","216440","2017-12-31","买方指定仓库地面交货"]
[null,"内蒙古东部电力有限公司","","2级单相表本地通信单元（宽带）","通信单元-通信单元类别:本地,适用终端/表类型:2级单相表,通信方式:宽带载波,频率范围/中心频率:2～12MHz,调制方式:OFDM","只","220211","2017-12-31","买方指定仓库地面交货"]
[null,"内蒙古东部电力有限公司","","2级单相表本地通信单元（宽带）","通信单元-通信单元类别:本地,适用终端/表类型:2级单相表,通信方式:宽带载波,频率范围/中心频率:2～12MHz,调制方式:OFDM","只","11981","2017-12-31","买方指定仓库地面交货"]
[null,"内蒙古东部电力有限公司","","采集故障识别模块","现场作业终端外设-采集故障识别模块:有,计量故障识别模块:无,超高频RFID模块:无,蓝牙打印模块:无","个","200","2017-12-31","买方指定仓库地面交货"]
[null,"内蒙古东部电力有限公司","","计量现场作业终端","现场作业终端-屏幕尺寸范围:≥7.0英寸,购电卡接口:无","台","200","2017-12-31","买方指定仓库地面交货"]
[null,"内蒙古东部电力有限公司","","计量现场作业终端","现场作业终端-屏幕尺寸范围:≥7.0英寸,购电卡接口:无","台","160","2017-12-31","买方指定仓库地面交货"]
[null,"内蒙古东部电力有限公司","","采集故障识别模块","现场作业终端外设-采集故障识别模块:有,计量故障识别模块:无,超高频RFID模块:无,蓝牙打印模块:无","个","160","2017-12-31","买方指定仓库地面交货"]
[null,"内蒙古东部电力有限公司","","计量现场作业终端","现场作业终端-屏幕尺寸范围:≥7.0英寸,购电卡接口:无","台","107","2017-12-31","买方指定仓库地面交货"]
[null,"内蒙古东部电力有限公司","","采集故障识别模块","现场作业终端外设-采集故障识别模块:有,计量故障识别模块:无,超高频RFID模块:无,蓝牙打印模块:无","个","107","2017-12-31","买方指定仓库地面交货"]
[null,"内蒙古东部电力有限公司","","计量现场作业终端","现场作业终端-屏幕尺寸范围:≥7.0英寸,购电卡接口:无","台","313","2017-12-31","买方指定仓库地面交货"]
[null,"内蒙古东部电力有限公司","","采集故障识别模块","现场作业终端外设-采集故障识别模块:有,计量故障识别模块:无,超高频RFID模块:无,蓝牙打印模块:无","个","313","2017-12-31","买方指定仓库地面交货"]
[null,"内蒙古东部电力有限公司","","2级单相费控智能电能表（模块-远程-开关内置）","单相智能电能表-准确度等级:2级,费控方式:远程,负荷开关:内置,通信模块接口:有,电压规格:220V,电流规格:5A","只","191004","2017-12-31","买方指定仓库地面交货"]
[null,"内蒙古东部电力有限公司","","2级单相费控智能电能表（模块-远程-开关内置）","单相智能电能表-准确度等级:2级,费控方式:远程,负荷开关:内置,通信模块接口:有,电压规格:220V,电流规格:5A","只","210757","2017-12-31","买方指定仓库地面交货"]
["包01MD2","内蒙古东部电力有限公司","","2级单相表本地通信单元（宽带）","通信单元-通信单元类别:本地,适用终端/表类型:2级单相表,通信方式:宽带载波,频率范围/中心频率:2～12MHz,调制方式:OFDM","只","100","2017-12-31","买方指定仓库地面交货"]
[null,"内蒙古东部电力有限公司","","2级单相表本地通信单元（宽带）","通信单元-通信单元类别:本地,适用终端/表类型:2级单相表,通信方式:宽带载波,频率范围/中心频率:2～12MHz,调制方式:OFDM","只","500","2017-12-31","买方指定仓库地面交货"]
[null,"内蒙古东部电力有限公司","","2级单相费控智能电能表（模块-远程-开关内置）","单相智能电能表-准确度等级:2级,费控方式:远程,负荷开关:内置,通信模块接口:有,电压规格:220V,电流规格:5A","只","340452","2017-12-31","买方指定仓库地面交货"]
[null,"内蒙古东部电力有限公司","","2级单相表本地通信单元（宽带）","通信单元-通信单元类别:本地,适用终端/表类型:2级单相表,通信方式:宽带载波,频率范围/中心频率:2～12MHz,调制方式:OFDM","只","54552","2017-12-31","买方指定仓库地面交货"]
[null,"内蒙古东部电力有限公司","","2级单相表本地通信单元（宽带）","通信单元-通信单元类别:本地,适用终端/表类型:2级单相表,通信方式:宽带载波,频率范围/中心频率:2～12MHz,调制方式:OFDM","只","168956","2017-12-31","买方指定仓库地面交货"]
[null,"内蒙古东部电力有限公司","","2级单相表本地通信单元（窄带）","通信单元-通信单元类别:本地,适用终端/表类型:2级单相表,通信方式:窄带载波,频率范围/中心频率:421kHz,调制方式:BFSK","只","136061","2017-12-31","买方指定仓库地面交货"]
["包01SH1","上海市电力公司","国网上海公司2017年第一次电能表（含用电信息采集）项目","2级单相费控智能电能表（模块-远程-开关内置）","单相智能电能表-准确度等级:2级,费控方式:远程,负荷开关:内置,通信模块接口:有,电压规格:220V,电流规格:5A","只","350000","2018-04-30","买方指定仓库车板交货"]
["包01SX1","山西省电力公司","","采集故障识别模块","现场作业终端外设-采集故障识别模块:有,计量故障识别模块:无,超高频RFID模块:无,蓝牙打印模块:无","个","982","2018-04-30","买方指定仓库地面交货"]
[null,"山西省电力公司","","2级单相费控智能电能表（模块-远程-开关内置）","单相智能电能表-准确度等级:2级,费控方式:远程,负荷开关:内置,通信模块接口:有,电压规格:220V,电流规格:5A","只","356002","2018-04-30","买方指定仓库地面交货"]
[null,"山西省电力公司","","计量现场作业终端","现场作业终端-屏幕尺寸范围:≤4.0英寸,购电卡接口:无","台","982","2018-04-30","买方指定仓库地面交货"]
[null,"山西省电力公司","","计量现场作业终端与外设收纳箱","现场作业终端与外设收纳箱-存放外设个数:1","个","982","2018-04-30","买方指定仓库地面交货"]
["包03GW1","西藏电力有限公司","国网西藏电力有限公司各供电公司营销专项、电网基建/户表","2级单相表本地通信单元（窄带）","通信单元-通信单元类别:本地,适用终端/表类型:2级单相表,通信方式:窄带载波,频率范围/中心频率:421kHz,调制方式:BFSK","只","238","2017-07-30","买方指定仓库地面交货"]
[null,"西藏电力有限公司","国网西藏电力有限公司各供电公司营销专项、电网基建/户表","2级单相费控智能电能表（模块-远程-开关外置）","单相智能电能表-准确度等级:2级,费控方式:远程,负荷开关:外置,通信模块接口:有,电压规格:220V,电流规格:10A","只","238","2017-06-30","买方指定仓库地面交货"]
[null,"江苏省电力公司","","2级单相费控智能电能表（远程-开关内置）","单相智能电能表-准确度等级:2级,费控方式:远程,负荷开关:内置,通信模块接口:无,电压规格:220V,电流规格:5A","只","250000","2018-04-15","买方指定仓库地面交货"]
["包03JS1","江苏省电力公司","","2级单相费控智能电能表（远程-开关内置）","单相智能电能表-准确度等级:2级,费控方式:远程,负荷开关:内置,通信模块接口:无,电压规格:220V,电流规格:5A","只","230000","2018-04-15","买方指定仓库地面交货"]
[null,"江苏省电力公司","","2级单相费控智能电能表（远程-开关内置）","单相智能电能表-准确度等级:2级,费控方式:远程,负荷开关:内置,通信模块接口:无,电压规格:220V,电流规格:5A","只","270000","2018-04-15","买方指定仓库地面交货"]
[null,"江苏省电力公司","","计量现场作业终端","现场作业终端-屏幕尺寸范围:(4.0～7.0)英寸,购电卡接口:无","台","1000","2018-04-15","买方指定仓库地面交货"]
["包03JS2","江苏省电力公司","","2级单相费控智能电能表（远程-开关内置）","单相智能电能表-准确度等级:2级,费控方式:远程,负荷开关:内置,通信模块接口:无,电压规格:220V,电流规格:5A","只","210000","2018-04-15","买方指定仓库地面交货"]
[null,"江苏省电力公司","","计量现场作业终端","现场作业终端-屏幕尺寸范围:≤4.0英寸,购电卡接口:无","台","800","2018-04-15","买方指定仓库地面交货"]
[null,"江苏省电力公司","","2级单相费控智能电能表（远程-开关内置）","单相智能电能表-准确度等级:2级,费控方式:远程,负荷开关:内置,通信模块接口:无,电压规格:220V,电流规格:5A","只","240000","2018-04-15","买方指定仓库地面交货"]
["包03JS3","江苏省电力公司","","2级单相费控智能电能表（远程-开关内置）","单相智能电能表-准确度等级:2级,费控方式:远程,负荷开关:内置,通信模块接口:无,电压规格:220V,电流规格:5A","只","190000","2018-04-15","买方指定仓库地面交货"]
[null,"江苏省电力公司","","2级单相费控智能电能表（远程-开关内置）","单相智能电能表-准确度等级:2级,费控方式:远程,负荷开关:内置,通信模块接口:无,电压规格:220V,电流规格:5A","只","180000","2018-04-15","买方指定仓库地面交货"]
[null,"江苏省电力公司","","计量现场作业终端","现场作业终端-屏幕尺寸范围:≤4.0英寸,购电卡接口:无","台","700","2018-04-15","买方指定仓库地面交货"]
["包03JS4","江苏省电力公司","","超高频RFID模块","现场作业终端外设-采集故障识别模块:无,计量故障识别模块:无,超高频RFID模块:有,蓝牙打印模块:无","个","80","2018-04-15","买方指定仓库地面交货"]
[null,"江苏省电力公司","","计量现场作业终端与外设收纳箱","现场作业终端与外设收纳箱-存放外设个数:4","个","150","2018-04-15","买方指定仓库地面交货"]
[null,"江苏省电力公司","","采集故障识别模块","现场作业终端外设-采集故障识别模块:有,计量故障识别模块:无,超高频RFID模块:无,蓝牙打印模块:无","个","150","2018-04-15","买方指定仓库地面交货"]
[null,"江苏省电力公司","","三相计量故障识别模块","现场作业终端外设-采集故障识别模块:无,计量故障识别模块:三相,超高频RFID模块:无,蓝牙打印模块:无","个","80","2018-04-15","买方指定仓库地面交货"]
[null,"江苏省电力公司","","单相计量故障识别模块","现场作业终端外设-采集故障识别模块:无,计量故障识别模块:单相,超高频RFID模块:无,蓝牙打印模块:无","个","80","2018-04-15","买方指定仓库地面交货"]
[null,"江苏省电力公司","","现场打印模块","现场作业终端外设-采集故障识别模块:无,计量故障识别模块:无,超高频RFID模块:无,蓝牙打印模块:有","个","15","2018-04-15","买方指定仓库地面交货"]
[null,"江苏省电力公司","","2级单相费控智能电能表（远程-开关内置）","单相智能电能表-准确度等级:2级,费控方式:远程,负荷开关:内置,通信模块接口:无,电压规格:220V,电流规格:5A","只","200000","2018-04-15","买方指定仓库地面交货"]
[null,"江苏省电力公司","","2级单相费控智能电能表（远程-开关内置）","单相智能电能表-准确度等级:2级,费控方式:远程,负荷开关:内置,通信模块接口:无,电压规格:220V,电流规格:5A","只","150000","2018-04-15","买方指定仓库地面交货"]
["包03JS5","江苏省电力公司","","2级单相费控智能电能表（远程-开关内置）","单相智能电能表-准确度等级:2级,费控方式:远程,负荷开关:内置,通信模块接口:无,电压规格:220V,电流规格:5A","只","100000","2018-04-15","买方指定仓库地面交货"]
[null,"江苏省电力公司","","2级单相费控智能电能表（远程-开关内置）","单相智能电能表-准确度等级:2级,费控方式:远程,负荷开关:内置,通信模块接口:无,电压规格:220V,电流规格:5A","只","220000","2018-04-15","买方指定仓库地面交货"]
["包03JS6","江苏省电力公司","","2级单相费控智能电能表（远程-开关内置）","单相智能电能表-准确度等级:2级,费控方式:远程,负荷开关:内置,通信模块接口:无,电压规格:220V,电流规格:5A","只","260000","2018-04-15","买方指定仓库地面交货"]
["包03ZJ1","浙江省电力公司","","2级单相费控智能电能表（远程-开关内置）","单相智能电能表-准确度等级:2级,费控方式:远程,负荷开关:内置,通信模块接口:无,电压规格:220V,电流规格:5A","只","500000","2019-03-31","买方指定仓库地面交货"]
["包03ZJ2","浙江省电力公司","","2级单相费控智能电能表（远程-开关内置）","单相智能电能表-准确度等级:2级,费控方式:远程,负荷开关:内置,通信模块接口:无,电压规格:220V,电流规格:5A","只","495000","2019-03-31","买方指定仓库地面交货"]
["包03ZJ3","浙江省电力公司","","2级单相费控智能电能表（远程-开关内置）","单相智能电能表-准确度等级:2级,费控方式:远程,负荷开关:内置,通信模块接口:无,电压规格:220V,电流规格:5A","只","450000","2019-03-31","买方指定仓库地面交货"]
["包03ZJ4","浙江省电力公司","","2级单相费控智能电能表（远程-开关内置）","单相智能电能表-准确度等级:2级,费控方式:远程,负荷开关:内置,通信模块接口:无,电压规格:220V,电流规格:5A","只","355000","2019-03-31","买方指定仓库地面交货"]
["包03ZJ5","浙江省电力公司","","2级单相费控智能电能表（远程-开关内置）","单相智能电能表-准确度等级:2级,费控方式:远程,负荷开关:内置,通信模块接口:无,电压规格:220V,电流规格:5A","只","350000","2019-03-31","买方指定仓库地面交货"]
["包03ZJ6","浙江省电力公司","","2级单相费控智能电能表（远程-开关内置）","单相智能电能表-准确度等级:2级,费控方式:远程,负荷开关:内置,通信模块接口:无,电压规格:220V,电流规格:5A","只","345000","2019-03-31","买方指定仓库地面交货"]
["包01FJ1","福建省电力有限公司","国网福建省电力有限公司采购","2级单相表本地通信单元（窄带）","通信单元-通信单元类别:本地,适用终端/表类型:2级单相表,通信方式:窄带载波,频率范围/中心频率:421kHz,调制方式:BFSK","只","12500","2018-06-30","买方指定仓库地面交货"]
[null,"福建省电力有限公司","国网福建省电力有限公司采购","2级单相表本地通信单元（宽带）","通信单元-通信单元类别:本地,适用终端/表类型:2级单相表,通信方式:宽带载波,频率范围/中心频率:2～12MHz,调制方式:OFDM","只","62500","2018-06-30","买方指定仓库地面交货"]
[null,"福建省电力有限公司","国网福建省电力有限公司采购","2级单相表本地通信单元（窄带）","通信单元-通信单元类别:本地,适用终端/表类型:2级单相表,通信方式:窄带载波,频率范围/中心频率:其他,调制方式:其他","只","56250","2018-06-30","买方指定仓库地面交货"]
[null,"福建省电力有限公司","国网福建省电力有限公司采购","2级单相表本地通信单元（窄带）","通信单元-通信单元类别:本地,适用终端/表类型:2级单相表,通信方式:窄带载波,频率范围/中心频率:132kHz,调制方式:BPSK","只","8553","2018-06-30","买方指定仓库地面交货"]
[null,"福建省电力有限公司","国网福建省电力有限公司采购","2级单相费控智能电能表（模块-远程-开关内置）","单相智能电能表-准确度等级:2级,费控方式:远程,负荷开关:内置,通信模块接口:有,电压规格:220V,电流规格:5A","只","450000","2018-06-30","买方指定仓库地面交货"]
[null,"福建省电力有限公司","国网福建省电力有限公司采购","2级单相表本地通信单元（窄带）","通信单元-通信单元类别:本地,适用终端/表类型:2级单相表,通信方式:窄带载波,频率范围/中心频率:270kHz,调制方式:BFSK","只","318655","2018-06-30","买方指定仓库地面交货"]
["包03ZJ7","浙江省电力公司","","2级单相费控智能电能表（远程-开关内置）","单相智能电能表-准确度等级:2级,费控方式:远程,负荷开关:内置,通信模块接口:无,电压规格:220V,电流规格:5A","只","340000","2019-03-31","买方指定仓库地面交货"]
["包03ZJ8","浙江省电力公司","","2级单相费控智能电能表（远程-开关外置）","单相智能电能表-准确度等级:2级,费控方式:远程,负荷开关:外置,通信模块接口:无,电压规格:220V,电流规格:10A","只","3900","2019-03-31","买方指定仓库地面交货"]
[null,"浙江省电力公司","","2级单相费控智能电能表（远程-开关内置）","单相智能电能表-准确度等级:2级,费控方式:远程,负荷开关:内置,通信模块接口:无,电压规格:220V,电流规格:5A","只","335000","2019-03-31","买方指定仓库地面交货"]
["包05TJ1","天津市电力公司","","2级单相表本地通信单元（宽带）","通信单元-通信单元类别:本地,适用终端/表类型:2级单相表,通信方式:宽带载波,频率范围/中心频率:2～12MHz,调制方式:OFDM","只","110000","2017-12-31","买方指定仓库地面交货"]
[null,"天津市电力公司","","单相计量故障识别模块","现场作业终端外设-采集故障识别模块:无,计量故障识别模块:单相,超高频RFID模块:无,蓝牙打印模块:无","个","10","2017-12-31","买方指定仓库地面交货"]
[null,"天津市电力公司","","三相计量故障识别模块","现场作业终端外设-采集故障识别模块:无,计量故障识别模块:三相,超高频RFID模块:无,蓝牙打印模块:无","个","10","2017-12-31","买方指定仓库地面交货"]
[null,"天津市电力公司","","2级单相费控智能电能表（模块-CPU卡-开关内置）","单相智能电能表-准确度等级:2级,费控方式:本地,负荷开关:内置,通信模块接口:有,电压规格:220V,电流规格:5A","只","442000","2017-12-31","买方指定仓库地面交货"]
[null,"天津市电力公司","","2级单相表本地通信单元（窄带）","通信单元-通信单元类别:本地,适用终端/表类型:2级单相表,通信方式:窄带载波,频率范围/中心频率:132kHz,调制方式:BPSK","只","4000","2017-12-31","买方指定仓库地面交货"]
[null,"天津市电力公司","","计量现场作业终端","现场作业终端-屏幕尺寸范围:(4.0～7.0)英寸,购电卡接口:有","台","100","2017-12-31","买方指定仓库地面交货"]
[null,"天津市电力公司","","2级单相表本地通信单元（窄带）","通信单元-通信单元类别:本地,适用终端/表类型:2级单相表,通信方式:窄带载波,频率范围/中心频率:421kHz,调制方式:BFSK","只","72000","2017-12-31","买方指定仓库地面交货"]
[null,"天津市电力公司","","2级单相表本地通信单元（窄带）","通信单元-通信单元类别:本地,适用终端/表类型:2级单相表,通信方式:窄带载波,频率范围/中心频率:270kHz,调制方式:BFSK","只","144000","2017-12-31","买方指定仓库地面交货"]
[null,"天津市电力公司","","2级单相表本地通信单元（窄带）","通信单元-通信单元类别:本地,适用终端/表类型:2级单相表,通信方式:窄带载波,频率范围/中心频率:其他,调制方式:其他","只","10000","2017-12-31","买方指定仓库地面交货"]
[null,"天津市电力公司","","采集故障识别模块","现场作业终端外设-采集故障识别模块:有,计量故障识别模块:无,超高频RFID模块:无,蓝牙打印模块:无","个","60","2017-12-31","买方指定仓库地面交货"]
[null,"天津市电力公司","","2级单相表本地通信单元（窄带）","通信单元-通信单元类别:本地,适用终端/表类型:2级单相表,通信方式:窄带载波,频率范围/中心频率:其他,调制方式:其他","只","102000","2017-12-31","买方指定仓库地面交货"]
["包37GW1","河南省电力公司","","2级单相费控智能电能表（模块-远程-开关内置-电池可换）","单相智能电能表-准确度等级:2级,费控方式:远程/电池可换,负荷开关:内置,通信模块接口:有,电压规格:220V,电流规格:5A","只","480000","2018-04-10","买方指定仓库地面交货"]
[null,"新疆电力公司","国家电网公司2017年第一次电能表（含用电信息采集）","2级单相表本地通信单元（窄带）","通信单元-通信单元类别:本地,适用终端/表类型:2级单相表,通信方式:窄带载波,频率范围/中心频率:132kHz,调制方式:BPSK","只","550","2017-10-30","买方指定仓库车板交货"]
[null,"新疆电力公司","国家电网公司2017年第一次电能表（含用电信息采集）","2级单相表本地通信单元（窄带）","通信单元-通信单元类别:本地,适用终端/表类型:2级单相表,通信方式:窄带载波,频率范围/中心频率:270kHz,调制方式:BFSK","只","2200","2017-10-30","买方指定仓库车板交货"]
[null,"新疆电力公司","国家电网公司2017年第一次电能表（含用电信息采集）","2级单相表本地通信单元（窄带）","通信单元-通信单元类别:本地,适用终端/表类型:2级单相表,通信方式:窄带载波,频率范围/中心频率:421kHz,调制方式:BFSK","只","2750","2017-10-30","买方指定仓库车板交货"]
[null,"河南省电力公司","","2级单相表本地通信单元（窄带）","通信单元-通信单元类别:本地,适用终端/表类型:2级单相表,通信方式:窄带载波,频率范围/中心频率:421kHz,调制方式:BFSK","只","229548","2018-04-10","买方指定仓库地面交货"]
[null,"河南省电力公司","","2级单相表本地通信单元（窄带）","通信单元-通信单元类别:本地,适用终端/表类型:2级单相表,通信方式:窄带载波,频率范围/中心频率:270kHz,调制方式:BFSK","只","31020","2018-04-10","买方指定仓库地面交货"]
[null,"河南省电力公司","","2级单相表本地通信单元（窄带）","通信单元-通信单元类别:本地,适用终端/表类型:2级单相表,通信方式:窄带载波,频率范围/中心频率:132kHz,调制方式:BPSK","只","148896","2018-04-10","买方指定仓库地面交货"]
[null,"河南省电力公司","","2级单相表本地通信单元（窄带）","通信单元-通信单元类别:本地,适用终端/表类型:2级单相表,通信方式:窄带载波,频率范围/中心频率:其他,调制方式:其他","只","118536","2018-04-10","买方指定仓库地面交货"]
[null,"新疆电力公司","国家电网公司2017年第一次电能表（含用电信息采集）","2级单相费控智能电能表（模块-远程-开关内置-电池可换）","单相智能电能表-准确度等级:2级,费控方式:远程/电池可换,负荷开关:内置,通信模块接口:有,电压规格:220V,电流规格:5A","只","5000","2017-10-30","买方指定仓库车板交货"]
["包37GW2","青海省电力公司","","2级单相费控智能电能表（模块-远程-开关内置-电池可换）","单相智能电能表-准确度等级:2级,费控方式:远程/电池可换,负荷开关:内置,通信模块接口:有,电压规格:220V,电流规格:5A","只","3000","2018-05-31","买方指定仓库地面交货"]
[null,"青海省电力公司","","2级单相费控智能电能表（模块-远程-开关内置-电池可换）","单相智能电能表-准确度等级:2级,费控方式:远程/电池可换,负荷开关:内置,通信模块接口:有,电压规格:220V,电流规格:5A","只","2000","2018-05-31","买方指定仓库地面交货"]
[null,"青海省电力公司","","2级单相表本地通信单元（窄带）","通信单元-通信单元类别:本地,适用终端/表类型:2级单相表,通信方式:窄带载波,频率范围/中心频率:421kHz,调制方式:BFSK","只","3000","2018-05-31","买方指定仓库地面交货"]
[null,"青海省电力公司","","2级单相表本地通信单元（窄带）","通信单元-通信单元类别:本地,适用终端/表类型:2级单相表,通信方式:窄带载波,频率范围/中心频率:270kHz,调制方式:BFSK","只","1000","2018-05-31","买方指定仓库地面交货"]
[null,"青海省电力公司","","2级单相表本地通信单元（窄带）","通信单元-通信单元类别:本地,适用终端/表类型:2级单相表,通信方式:窄带载波,频率范围/中心频率:421kHz,调制方式:BFSK","只","1000","2018-05-31","买方指定仓库地面交货"]
[null,"青海省电力公司","","2级单相表本地通信单元（窄带）","通信单元-通信单元类别:本地,适用终端/表类型:2级单相表,通信方式:窄带载波,频率范围/中心频率:132kHz,调制方式:BPSK","只","4000","2018-05-31","买方指定仓库地面交货"]
[null,"青海省电力公司","","2级单相表本地通信单元（窄带）","通信单元-通信单元类别:本地,适用终端/表类型:2级单相表,通信方式:窄带载波,频率范围/中心频率:270kHz,调制方式:BFSK","只","4000","2018-05-31","买方指定仓库地面交货"]
[null,"山东电力集团公司","","2级单相费控智能电能表（模块-远程-开关内置-电池可换）","单相智能电能表-准确度等级:2级,费控方式:远程/电池可换,负荷开关:内置,通信模块接口:有,电压规格:220V,电流规格:5A","只","266100","2018-06-30","买方指定仓库地面交货"]
[null,"青海省电力公司","","2级单相费控智能电能表（模块-远程-开关内置-电池可换）","单相智能电能表-准确度等级:2级,费控方式:远程/电池可换,负荷开关:内置,通信模块接口:有,电压规格:220V,电流规格:5A","只","7000","2018-05-31","买方指定仓库地面交货"]
[null,"青海省电力公司","","2级单相表本地通信单元（窄带）","通信单元-通信单元类别:本地,适用终端/表类型:2级单相表,通信方式:窄带载波,频率范围/中心频率:421kHz,调制方式:BFSK","只","2000","2018-05-31","买方指定仓库地面交货"]
[null,"青海省电力公司","","2级单相费控智能电能表（模块-远程-开关内置-电池可换）","单相智能电能表-准确度等级:2级,费控方式:远程/电池可换,负荷开关:内置,通信模块接口:有,电压规格:220V,电流规格:5A","只","8000","2018-05-31","买方指定仓库地面交货"]
[null,"青海省电力公司","","2级单相表本地通信单元（窄带）","通信单元-通信单元类别:本地,适用终端/表类型:2级单相表,通信方式:窄带载波,频率范围/中心频率:132kHz,调制方式:BPSK","只","8000","2018-05-31","买方指定仓库地面交货"]
[null,"青海省电力公司","","2级单相表本地通信单元（窄带）","通信单元-通信单元类别:本地,适用终端/表类型:2级单相表,通信方式:窄带载波,频率范围/中心频率:421kHz,调制方式:BFSK","只","1000","2018-05-31","买方指定仓库地面交货"]
[null,"青海省电力公司","","2级单相表本地通信单元（窄带）","通信单元-通信单元类别:本地,适用终端/表类型:2级单相表,通信方式:窄带载波,频率范围/中心频率:270kHz,调制方式:BFSK","只","1000","2018-05-31","买方指定仓库地面交货"]
[null,"青海省电力公司","","2级单相表本地通信单元（窄带）","通信单元-通信单元类别:本地,适用终端/表类型:2级单相表,通信方式:窄带载波,频率范围/中心频率:270kHz,调制方式:BFSK","只","1000","2018-05-31","买方指定仓库地面交货"]
[null,"青海省电力公司","","2级单相费控智能电能表（模块-远程-开关内置-电池可换）","单相智能电能表-准确度等级:2级,费控方式:远程/电池可换,负荷开关:内置,通信模块接口:有,电压规格:220V,电流规格:5A","只","14000","2018-05-31","买方指定仓库地面交货"]
[null,"青海省电力公司","","2级单相表本地通信单元（窄带）","通信单元-通信单元类别:本地,适用终端/表类型:2级单相表,通信方式:窄带载波,频率范围/中心频率:421kHz,调制方式:BFSK","只","13000","2018-05-31","买方指定仓库地面交货"]
[null,"青海省电力公司","","2级单相表本地通信单元（窄带）","通信单元-通信单元类别:本地,适用终端/表类型:2级单相表,通信方式:窄带载波,频率范围/中心频率:132kHz,调制方式:BPSK","只","3000","2018-05-31","买方指定仓库地面交货"]
[null,"青海省电力公司","","2级单相表本地通信单元（窄带）","通信单元-通信单元类别:本地,适用终端/表类型:2级单相表,通信方式:窄带载波,频率范围/中心频率:270kHz,调制方式:BFSK","只","2000","2018-05-31","买方指定仓库地面交货"]
[null,"青海省电力公司","","2级单相费控智能电能表（模块-远程-开关内置-电池可换）","单相智能电能表-准确度等级:2级,费控方式:远程/电池可换,负荷开关:内置,通信模块接口:有,电压规格:220V,电流规格:5A","只","6000","2018-05-31","买方指定仓库地面交货"]
[null,"青海省电力公司","","2级单相表本地通信单元（窄带）","通信单元-通信单元类别:本地,适用终端/表类型:2级单相表,通信方式:窄带载波,频率范围/中心频率:132kHz,调制方式:BPSK","只","5000","2018-05-31","买方指定仓库地面交货"]
[null,"青海省电力公司","","2级单相表本地通信单元（窄带）","通信单元-通信单元类别:本地,适用终端/表类型:2级单相表,通信方式:窄带载波,频率范围/中心频率:270kHz,调制方式:BFSK","只","1000","2018-05-31","买方指定仓库地面交货"]
[null,"青海省电力公司","","2级单相费控智能电能表（模块-远程-开关内置-电池可换）","单相智能电能表-准确度等级:2级,费控方式:远程/电池可换,负荷开关:内置,通信模块接口:有,电压规格:220V,电流规格:5A","只","10000","2018-05-31","买方指定仓库地面交货"]
["包37AH1","安徽省电力公司","","2级单相费控智能电能表（模块-远程-开关内置-电池可换）","单相智能电能表-准确度等级:2级,费控方式:远程/电池可换,负荷开关:内置,通信模块接口:有,电压规格:220V,电流规格:5A","只","355000","2017-07-10","买方指定仓库地面交货"]
[null,"安徽省电力公司","","2级单相表本地通信单元（窄带）","通信单元-通信单元类别:本地,适用终端/表类型:2级单相表,通信方式:窄带载波,频率范围/中心频率:其他,调制方式:其他","只","6600","2017-07-10","买方指定仓库地面交货"]
[null,"安徽省电力公司","","2级单相表本地通信单元（窄带）","通信单元-通信单元类别:本地,适用终端/表类型:2级单相表,通信方式:窄带载波,频率范围/中心频率:421kHz,调制方式:BFSK","只","358400","2017-07-10","买方指定仓库地面交货"]
["包37AH2","安徽省电力公司","","2级单相费控智能电能表（模块-远程-开关内置-电池可换）","单相智能电能表-准确度等级:2级,费控方式:远程/电池可换,负荷开关:内置,通信模块接口:有,电压规格:220V,电流规格:5A","只","280000","2017-07-10","买方指定仓库地面交货"]
[null,"安徽省电力公司","","2级单相表本地通信单元（窄带）","通信单元-通信单元类别:本地,适用终端/表类型:2级单相表,通信方式:窄带载波,频率范围/中心频率:132kHz,调制方式:BPSK","只","103500","2017-07-10","买方指定仓库地面交货"]
[null,"安徽省电力公司","","2级单相表本地通信单元（窄带）","通信单元-通信单元类别:本地,适用终端/表类型:2级单相表,通信方式:窄带载波,频率范围/中心频率:421kHz,调制方式:BFSK","只","176500","2017-07-10","买方指定仓库地面交货"]
["包37FJ1","福建省电力有限公司","国网福建省电力有限公司采购","2级单相费控智能电能表（模块-远程-开关内置-电池可换）","单相智能电能表-准确度等级:2级,费控方式:远程/电池可换,负荷开关:内置,通信模块接口:有,电压规格:220V,电流规格:5A","只","300000","2018-06-30","买方指定仓库地面交货"]
[null,"福建省电力有限公司","国网福建省电力有限公司采购","2级单相表本地通信单元（宽带）","通信单元-通信单元类别:本地,适用终端/表类型:2级单相表,通信方式:宽带载波,频率范围/中心频率:2～12MHz,调制方式:OFDM","只","300000","2018-06-30","买方指定仓库地面交货"]
["包37HA1","河南省电力公司","","2级单相表本地通信单元（微功率）","通信单元-通信单元类别:本地,适用终端/表类型:2级单相表,通信方式:微功率,频率范围/中心频率:470～510MHz,调制方式:GFSK","只","495000","2018-04-10","买方指定仓库地面交货"]
[null,"河南省电力公司","","2级单相费控智能电能表（模块-远程-开关内置-电池可换）","单相智能电能表-准确度等级:2级,费控方式:远程/电池可换,负荷开关:内置,通信模块接口:有,电压规格:220V,电流规格:5A","只","450000","2018-04-10","买方指定仓库地面交货"]
["包37HA2","河南省电力公司","","2级单相费控智能电能表（模块-远程-开关内置-电池可换）","单相智能电能表-准确度等级:2级,费控方式:远程/电池可换,负荷开关:内置,通信模块接口:有,电压规格:220V,电流规格:5A","只","350000","2018-04-10","买方指定仓库地面交货"]
[null,"河南省电力公司","","2级单相表本地通信单元（宽带）","通信单元-通信单元类别:本地,适用终端/表类型:2级单相表,通信方式:宽带载波,频率范围/中心频率:2～12MHz,调制方式:OFDM","只","385000","2018-04-10","买方指定仓库地面交货"]
["包37HA3","河南省电力公司","","2级单相表本地通信单元（宽带）","通信单元-通信单元类别:本地,适用终端/表类型:2级单相表,通信方式:宽带载波,频率范围/中心频率:2～12MHz,调制方式:OFDM","只","385000","2018-04-10","买方指定仓库地面交货"]
[null,"河南省电力公司","","2级单相费控智能电能表（模块-远程-开关内置-电池可换）","单相智能电能表-准确度等级:2级,费控方式:远程/电池可换,负荷开关:内置,通信模块接口:有,电压规格:220V,电流规格:5A","只","350000","2018-04-10","买方指定仓库地面交货"]
["包37HA4","河南省电力公司","","2级单相费控智能电能表（模块-远程-开关内置-电池可换）","单相智能电能表-准确度等级:2级,费控方式:远程/电池可换,负荷开关:内置,通信模块接口:有,电压规格:220V,电流规格:5A","只","250000","2018-04-10","买方指定仓库地面交货"]
[null,"河南省电力公司","","2级单相表本地通信单元（宽带）","通信单元-通信单元类别:本地,适用终端/表类型:2级单相表,通信方式:宽带载波,频率范围/中心频率:2～12MHz,调制方式:OFDM","只","57200","2018-04-10","买方指定仓库地面交货"]
[null,"河南省电力公司","","2级单相表本地通信单元（窄带）","通信单元-通信单元类别:本地,适用终端/表类型:2级单相表,通信方式:窄带载波,频率范围/中心频率:其他,调制方式:其他","只","92400","2018-04-10","买方指定仓库地面交货"]
[null,"河南省电力公司","","2级单相表本地通信单元（微功率）","通信单元-通信单元类别:本地,适用终端/表类型:2级单相表,通信方式:微功率,频率范围/中心频率:470～510MHz,调制方式:GFSK","只","125400","2018-04-10","买方指定仓库地面交货"]
["包37HE1","河北省电力公司","","2级单相费控智能电能表（模块-远程-开关内置-电池可换）","单相智能电能表-准确度等级:2级,费控方式:远程/电池可换,负荷开关:内置,通信模块接口:有,电压规格:220V,电流规格:5A","只","408000","2018-03-31","买方指定仓库地面交货"]
[null,"河北省电力公司","","现场打印模块","现场作业终端外设-采集故障识别模块:无,计量故障识别模块:无,超高频RFID模块:无,蓝牙打印模块:有","个","208","2018-03-31","买方指定仓库地面交货"]
[null,"河北省电力公司","","超高频RFID模块","现场作业终端外设-采集故障识别模块:无,计量故障识别模块:无,超高频RFID模块:有,蓝牙打印模块:无","个","208","2018-03-31","买方指定仓库地面交货"]
[null,"河北省电力公司","","单相计量故障识别模块","现场作业终端外设-采集故障识别模块:无,计量故障识别模块:单相,超高频RFID模块:无,蓝牙打印模块:无","个","208","2018-03-31","买方指定仓库地面交货"]
[null,"河北省电力公司","","三相计量故障识别模块","现场作业终端外设-采集故障识别模块:无,计量故障识别模块:三相,超高频RFID模块:无,蓝牙打印模块:无","个","208","2018-03-31","买方指定仓库地面交货"]
[null,"河北省电力公司","","采集故障识别模块","现场作业终端外设-采集故障识别模块:有,计量故障识别模块:无,超高频RFID模块:无,蓝牙打印模块:无","个","208","2018-03-31","买方指定仓库地面交货"]
[null,"河北省电力公司","","2级单相表本地通信单元（窄带）","通信单元-通信单元类别:本地,适用终端/表类型:2级单相表,通信方式:窄带载波,频率范围/中心频率:132kHz,调制方式:BPSK","只","408000","2018-03-31","买方指定仓库地面交货"]
[null,"河北省电力公司","","计量现场作业终端","现场作业终端-屏幕尺寸范围:(4.0～7.0)英寸,购电卡接口:有","台","2638","2018-03-31","买方指定仓库地面交货"]
[null,"河北省电力公司","","计量现场作业终端与外设收纳箱","现场作业终端与外设收纳箱-存放外设个数:4","个","104","2018-03-31","买方指定仓库地面交货"]
["包37HE2","河北省电力公司","","2级单相费控智能电能表（模块-远程-开关内置-电池可换）","单相智能电能表-准确度等级:2级,费控方式:远程/电池可换,负荷开关:内置,通信模块接口:有,电压规格:220V,电流规格:5A","只","443000","2018-03-31","买方指定仓库地面交货"]
[null,"河北省电力公司","","2级单相表本地通信单元（窄带）","通信单元-通信单元类别:本地,适用终端/表类型:2级单相表,通信方式:窄带载波,频率范围/中心频率:300kHz,调制方式:QPSK","只","11000","2018-03-31","买方指定仓库地面交货"]
[null,"河北省电力公司","","2级单相表本地通信单元（窄带）","通信单元-通信单元类别:本地,适用终端/表类型:2级单相表,通信方式:窄带载波,频率范围/中心频率:421kHz,调制方式:BFSK","只","62000","2018-03-31","买方指定仓库地面交货"]
[null,"河北省电力公司","","2级单相表本地通信单元（窄带）","通信单元-通信单元类别:本地,适用终端/表类型:2级单相表,通信方式:窄带载波,频率范围/中心频率:270kHz,调制方式:BFSK","只","40000","2018-03-31","买方指定仓库地面交货"]
[null,"河北省电力公司","","2级单相表本地通信单元（微功率）","通信单元-通信单元类别:本地,适用终端/表类型:2级单相表,通信方式:微功率,频率范围/中心频率:470～510MHz,调制方式:GFSK","只","37000","2018-03-31","买方指定仓库地面交货"]
[null,"河北省电力公司","","2级单相表本地通信单元（窄带）","通信单元-通信单元类别:本地,适用终端/表类型:2级单相表,通信方式:窄带载波,频率范围/中心频率:300kHz,调制方式:BPSK","只","293000","2018-03-31","买方指定仓库地面交货"]
["包37LN1","辽宁省电力有限公司","","现场打印模块","现场作业终端外设-采集故障识别模块:无,计量故障识别模块:无,超高频RFID模块:无,蓝牙打印模块:有","个","15","2017-08-20","买方指定仓库地面交货"]
[null,"辽宁省电力有限公司","","采集故障识别模块","现场作业终端外设-采集故障识别模块:有,计量故障识别模块:无,超高频RFID模块:无,蓝牙打印模块:无","个","15","2017-08-22","买方指定仓库地面交货"]
[null,"辽宁省电力有限公司","","单相计量故障识别模块","现场作业终端外设-采集故障识别模块:无,计量故障识别模块:单相,超高频RFID模块:无,蓝牙打印模块:无","个","15","2017-08-22","买方指定仓库地面交货"]
[null,"辽宁省电力有限公司","","三相计量故障识别模块","现场作业终端外设-采集故障识别模块:无,计量故障识别模块:三相,超高频RFID模块:无,蓝牙打印模块:无","个","36","2017-08-31","买方指定仓库地面交货"]
[null,"辽宁省电力有限公司","","计量现场作业终端与外设收纳箱","现场作业终端与外设收纳箱-存放外设个数:4","个","36","2017-08-31","买方指定仓库地面交货"]
[null,"辽宁省电力有限公司","","计量现场作业终端","现场作业终端-屏幕尺寸范围:(4.0～7.0)英寸,购电卡接口:有","台","15","2017-07-24","买方指定仓库地面交货"]
[null,"辽宁省电力有限公司","","现场打印模块","现场作业终端外设-采集故障识别模块:无,计量故障识别模块:无,超高频RFID模块:无,蓝牙打印模块:有","个","15","2017-07-24","买方指定仓库地面交货"]
[null,"辽宁省电力有限公司","","2级单相费控智能电能表（模块-远程-开关内置-电池可换）","单相智能电能表-准确度等级:2级,费控方式:远程/电池可换,负荷开关:内置,通信模块接口:有,电压规格:220V,电流规格:5A","只","10000","2017-08-22","买方指定仓库地面交货"]
[null,"辽宁省电力有限公司","","2级单相费控智能电能表（模块-远程-开关内置-电池可换）","单相智能电能表-准确度等级:2级,费控方式:远程/电池可换,负荷开关:内置,通信模块接口:有,电压规格:220V,电流规格:5A","只","70500","2017-07-25","买方指定仓库地面交货"]
[null,"辽宁省电力有限公司","","2级单相费控智能电能表（模块-远程-开关内置-电池可换）","单相智能电能表-准确度等级:2级,费控方式:远程/电池可换,负荷开关:内置,通信模块接口:有,电压规格:220V,电流规格:5A","只","31000","2017-09-21","买方指定仓库地面交货"]
[null,"辽宁省电力有限公司","","2级单相费控智能电能表（模块-远程-开关内置-电池可换）","单相智能电能表-准确度等级:2级,费控方式:远程/电池可换,负荷开关:内置,通信模块接口:有,电压规格:220V,电流规格:5A","只","20000","2017-07-20","买方指定仓库地面交货"]
[null,"辽宁省电力有限公司","","2级单相费控智能电能表（模块-远程-开关内置-电池可换）","单相智能电能表-准确度等级:2级,费控方式:远程/电池可换,负荷开关:内置,通信模块接口:有,电压规格:220V,电流规格:5A","只","15000","2017-09-15","买方指定仓库地面交货"]
[null,"辽宁省电力有限公司","","2级单相费控智能电能表（模块-远程-开关内置-电池可换）","单相智能电能表-准确度等级:2级,费控方式:远程/电池可换,负荷开关:内置,通信模块接口:有,电压规格:220V,电流规格:5A","只","21000","2017-08-20","买方指定仓库地面交货"]
[null,"辽宁省电力有限公司","","2级单相表本地通信单元（窄带）","通信单元-通信单元类别:本地,适用终端/表类型:2级单相表,通信方式:窄带载波,频率范围/中心频率:270kHz,调制方式:BFSK","只","5000","2017-08-22","买方指定仓库地面交货"]
[null,"辽宁省电力有限公司","","2级单相表本地通信单元（窄带）","通信单元-通信单元类别:本地,适用终端/表类型:2级单相表,通信方式:窄带载波,频率范围/中心频率:270kHz,调制方式:BFSK","只","15000","2017-09-15","买方指定仓库地面交货"]
[null,"辽宁省电力有限公司","","2级单相表本地通信单元（窄带）","通信单元-通信单元类别:本地,适用终端/表类型:2级单相表,通信方式:窄带载波,频率范围/中心频率:421kHz,调制方式:BFSK","只","10000","2017-09-18","买方指定仓库地面交货"]
[null,"辽宁省电力有限公司","","2级单相表本地通信单元（窄带）","通信单元-通信单元类别:本地,适用终端/表类型:2级单相表,通信方式:窄带载波,频率范围/中心频率:270kHz,调制方式:BFSK","只","30075","2017-09-18","买方指定仓库地面交货"]
[null,"辽宁省电力有限公司","","2级单相表本地通信单元（窄带）","通信单元-通信单元类别:本地,适用终端/表类型:2级单相表,通信方式:窄带载波,频率范围/中心频率:270kHz,调制方式:BFSK","只","15000","2017-08-20","买方指定仓库地面交货"]
[null,"辽宁省电力有限公司","","2级单相表本地通信单元（窄带）","通信单元-通信单元类别:本地,适用终端/表类型:2级单相表,通信方式:窄带载波,频率范围/中心频率:其他,调制方式:其他","只","6500","2017-08-20","买方指定仓库地面交货"]
[null,"辽宁省电力有限公司","","现场打印模块","现场作业终端外设-采集故障识别模块:无,计量故障识别模块:无,超高频RFID模块:无,蓝牙打印模块:有","个","32","2017-08-25","买方指定仓库地面交货"]
[null,"辽宁省电力有限公司","","超高频RFID模块","现场作业终端外设-采集故障识别模块:无,计量故障识别模块:无,超高频RFID模块:有,蓝牙打印模块:无","个","28","2017-07-25","买方指定仓库地面交货"]
[null,"辽宁省电力有限公司","","现场打印模块","现场作业终端外设-采集故障识别模块:无,计量故障识别模块:无,超高频RFID模块:无,蓝牙打印模块:有","个","12","2017-07-20","买方指定仓库地面交货"]
[null,"辽宁省电力有限公司","","计量现场作业终端","现场作业终端-屏幕尺寸范围:≥7.0英寸,购电卡接口:有","台","15","2017-09-15","买方指定仓库地面交货"]
[null,"辽宁省电力有限公司","","单相计量故障识别模块","现场作业终端外设-采集故障识别模块:无,计量故障识别模块:单相,超高频RFID模块:无,蓝牙打印模块:无","个","15","2017-09-15","买方指定仓库地面交货"]
[null,"辽宁省电力有限公司","","三相计量故障识别模块","现场作业终端外设-采集故障识别模块:无,计量故障识别模块:三相,超高频RFID模块:无,蓝牙打印模块:无","个","15","2017-09-15","买方指定仓库地面交货"]
[null,"辽宁省电力有限公司","","现场打印模块","现场作业终端外设-采集故障识别模块:无,计量故障识别模块:无,超高频RFID模块:无,蓝牙打印模块:有","个","15","2017-09-15","买方指定仓库地面交货"]
[null,"辽宁省电力有限公司","","超高频RFID模块","现场作业终端外设-采集故障识别模块:无,计量故障识别模块:无,超高频RFID模块:有,蓝牙打印模块:无","个","15","2017-09-15","买方指定仓库地面交货"]
[null,"辽宁省电力有限公司","","计量现场作业终端与外设收纳箱","现场作业终端与外设收纳箱-存放外设个数:4","个","15","2017-09-15","买方指定仓库地面交货"]
[null,"辽宁省电力有限公司","","采集故障识别模块","现场作业终端外设-采集故障识别模块:有,计量故障识别模块:无,超高频RFID模块:无,蓝牙打印模块:无","个","12","2017-08-20","买方指定仓库地面交货"]
[null,"辽宁省电力有限公司","","单相计量故障识别模块","现场作业终端外设-采集故障识别模块:无,计量故障识别模块:单相,超高频RFID模块:无,蓝牙打印模块:无","个","12","2017-08-20","买方指定仓库地面交货"]
[null,"辽宁省电力有限公司","","计量现场作业终端","现场作业终端-屏幕尺寸范围:(4.0～7.0)英寸,购电卡接口:有","台","15","2017-09-23","买方指定仓库地面交货"]
[null,"辽宁省电力有限公司","","采集故障识别模块","现场作业终端外设-采集故障识别模块:有,计量故障识别模块:无,超高频RFID模块:无,蓝牙打印模块:无","个","15","2017-09-23","买方指定仓库地面交货"]
[null,"辽宁省电力有限公司","","单相计量故障识别模块","现场作业终端外设-采集故障识别模块:无,计量故障识别模块:单相,超高频RFID模块:无,蓝牙打印模块:无","个","15","2017-09-23","买方指定仓库地面交货"]
[null,"辽宁省电力有限公司","","计量现场作业终端与外设收纳箱","现场作业终端与外设收纳箱-存放外设个数:4","个","15","2017-07-20","买方指定仓库地面交货"]
[null,"辽宁省电力有限公司","","超高频RFID模块","现场作业终端外设-采集故障识别模块:无,计量故障识别模块:无,超高频RFID模块:有,蓝牙打印模块:无","个","15","2017-07-20","买方指定仓库地面交货"]
[null,"辽宁省电力有限公司","","现场打印模块","现场作业终端外设-采集故障识别模块:无,计量故障识别模块:无,超高频RFID模块:无,蓝牙打印模块:有","个","15","2017-07-20","买方指定仓库地面交货"]
[null,"辽宁省电力有限公司","","2级单相表本地通信单元（宽带）","通信单元-通信单元类别:本地,适用终端/表类型:2级单相表,通信方式:宽带载波,频率范围/中心频率:2～12MHz,调制方式:OFDM","只","73450","2017-08-31","买方指定仓库地面交货"]
[null,"辽宁省电力有限公司","","2级单相表本地通信单元（窄带）","通信单元-通信单元类别:本地,适用终端/表类型:2级单相表,通信方式:窄带载波,频率范围/中心频率:421kHz,调制方式:BFSK","只","12000","2017-08-20","买方指定仓库地面交货"]
[null,"辽宁省电力有限公司","","2级单相表本地通信单元（窄带）","通信单元-通信单元类别:本地,适用终端/表类型:2级单相表,通信方式:窄带载波,频率范围/中心频率:421kHz,调制方式:BFSK","只","5000","2017-08-22","买方指定仓库地面交货"]
[null,"辽宁省电力有限公司","","2级单相表本地通信单元（窄带）","通信单元-通信单元类别:本地,适用终端/表类型:2级单相表,通信方式:窄带载波,频率范围/中心频率:421kHz,调制方式:BFSK","只","20500","2017-07-25","买方指定仓库地面交货"]
[null,"辽宁省电力有限公司","","2级单相表本地通信单元（窄带）","通信单元-通信单元类别:本地,适用终端/表类型:2级单相表,通信方式:窄带载波,频率范围/中心频率:270kHz,调制方式:BFSK","只","50000","2017-07-25","买方指定仓库地面交货"]
[null,"辽宁省电力有限公司","","2级单相表本地通信单元（窄带）","通信单元-通信单元类别:本地,适用终端/表类型:2级单相表,通信方式:窄带载波,频率范围/中心频率:270kHz,调制方式:BFSK","只","10000","2017-07-20","买方指定仓库地面交货"]
[null,"辽宁省电力有限公司","","计量现场作业终端","现场作业终端-屏幕尺寸范围:≥7.0英寸,购电卡接口:有","台","28","2017-07-25","买方指定仓库地面交货"]
[null,"辽宁省电力有限公司","","采集故障识别模块","现场作业终端外设-采集故障识别模块:有,计量故障识别模块:无,超高频RFID模块:无,蓝牙打印模块:无","个","28","2017-07-25","买方指定仓库地面交货"]
[null,"辽宁省电力有限公司","","单相计量故障识别模块","现场作业终端外设-采集故障识别模块:无,计量故障识别模块:单相,超高频RFID模块:无,蓝牙打印模块:无","个","28","2017-07-25","买方指定仓库地面交货"]
[null,"辽宁省电力有限公司","","现场打印模块","现场作业终端外设-采集故障识别模块:无,计量故障识别模块:无,超高频RFID模块:无,蓝牙打印模块:有","个","28","2017-07-25","买方指定仓库地面交货"]
[null,"辽宁省电力有限公司","","计量现场作业终端与外设收纳箱","现场作业终端与外设收纳箱-存放外设个数:4","个","28","2017-07-25","买方指定仓库地面交货"]
[null,"辽宁省电力有限公司","","采集故障识别模块","现场作业终端外设-采集故障识别模块:有,计量故障识别模块:无,超高频RFID模块:无,蓝牙打印模块:无","个","15","2017-09-21","买方指定仓库地面交货"]
[null,"辽宁省电力有限公司","","单相计量故障识别模块","现场作业终端外设-采集故障识别模块:无,计量故障识别模块:单相,超高频RFID模块:无,蓝牙打印模块:无","个","15","2017-09-21","买方指定仓库地面交货"]
[null,"辽宁省电力有限公司","","计量现场作业终端","现场作业终端-屏幕尺寸范围:(4.0～7.0)英寸,购电卡接口:有","台","15","2017-09-21","买方指定仓库地面交货"]
[null,"辽宁省电力有限公司","","单相计量故障识别模块","现场作业终端外设-采集故障识别模块:无,计量故障识别模块:单相,超高频RFID模块:无,蓝牙打印模块:无","个","12","2017-07-20","买方指定仓库地面交货"]
[null,"辽宁省电力有限公司","","计量现场作业终端","现场作业终端-屏幕尺寸范围:(4.0～7.0)英寸,购电卡接口:有","台","12","2017-07-20","买方指定仓库地面交货"]
[null,"辽宁省电力有限公司","","三相计量故障识别模块","现场作业终端外设-采集故障识别模块:无,计量故障识别模块:三相,超高频RFID模块:无,蓝牙打印模块:无","个","12","2017-07-20","买方指定仓库地面交货"]
[null,"辽宁省电力有限公司","","计量现场作业终端与外设收纳箱","现场作业终端与外设收纳箱-存放外设个数:1","个","12","2017-07-20","买方指定仓库地面交货"]
[null,"辽宁省电力有限公司","","超高频RFID模块","现场作业终端外设-采集故障识别模块:无,计量故障识别模块:无,超高频RFID模块:有,蓝牙打印模块:无","个","12","2017-07-20","买方指定仓库地面交货"]
[null,"辽宁省电力有限公司","","采集故障识别模块","现场作业终端外设-采集故障识别模块:有,计量故障识别模块:无,超高频RFID模块:无,蓝牙打印模块:无","个","15","2017-09-15","买方指定仓库地面交货"]
[null,"辽宁省电力有限公司","","三相计量故障识别模块","现场作业终端外设-采集故障识别模块:无,计量故障识别模块:三相,超高频RFID模块:无,蓝牙打印模块:无","个","12","2017-08-20","买方指定仓库地面交货"]
[null,"辽宁省电力有限公司","","计量现场作业终端","现场作业终端-屏幕尺寸范围:≥7.0英寸,购电卡接口:有","台","12","2017-08-20","买方指定仓库地面交货"]
[null,"辽宁省电力有限公司","","超高频RFID模块","现场作业终端外设-采集故障识别模块:无,计量故障识别模块:无,超高频RFID模块:有,蓝牙打印模块:无","个","12","2017-08-20","买方指定仓库地面交货"]
[null,"辽宁省电力有限公司","","计量现场作业终端与外设收纳箱","现场作业终端与外设收纳箱-存放外设个数:4","个","12","2017-08-20","买方指定仓库地面交货"]
[null,"辽宁省电力有限公司","","现场打印模块","现场作业终端外设-采集故障识别模块:无,计量故障识别模块:无,超高频RFID模块:无,蓝牙打印模块:有","个","12","2017-08-20","买方指定仓库地面交货"]
[null,"辽宁省电力有限公司","","计量现场作业终端与外设收纳箱","现场作业终端与外设收纳箱-存放外设个数:4","个","15","2017-09-18","买方指定仓库地面交货"]
[null,"辽宁省电力有限公司","","现场打印模块","现场作业终端外设-采集故障识别模块:无,计量故障识别模块:无,超高频RFID模块:无,蓝牙打印模块:有","个","15","2017-09-18","买方指定仓库地面交货"]
[null,"辽宁省电力有限公司","","三相计量故障识别模块","现场作业终端外设-采集故障识别模块:无,计量故障识别模块:三相,超高频RFID模块:无,蓝牙打印模块:无","个","15","2017-09-23","买方指定仓库地面交货"]
[null,"辽宁省电力有限公司","","超高频RFID模块","现场作业终端外设-采集故障识别模块:无,计量故障识别模块:无,超高频RFID模块:有,蓝牙打印模块:无","个","15","2017-09-23","买方指定仓库地面交货"]
[null,"辽宁省电力有限公司","","现场打印模块","现场作业终端外设-采集故障识别模块:无,计量故障识别模块:无,超高频RFID模块:无,蓝牙打印模块:有","个","15","2017-09-23","买方指定仓库地面交货"]
[null,"辽宁省电力有限公司","","计量现场作业终端与外设收纳箱","现场作业终端与外设收纳箱-存放外设个数:4","个","15","2017-09-23","买方指定仓库地面交货"]
[null,"辽宁省电力有限公司","","计量现场作业终端","现场作业终端-屏幕尺寸范围:≤4.0英寸,购电卡接口:有","台","15","2017-08-20","买方指定仓库地面交货"]
[null,"辽宁省电力有限公司","","三相计量故障识别模块","现场作业终端外设-采集故障识别模块:无,计量故障识别模块:三相,超高频RFID模块:无,蓝牙打印模块:无","个","15","2017-08-20","买方指定仓库地面交货"]
[null,"辽宁省电力有限公司","","超高频RFID模块","现场作业终端外设-采集故障识别模块:无,计量故障识别模块:无,超高频RFID模块:有,蓝牙打印模块:无","个","15","2017-08-20","买方指定仓库地面交货"]
[null,"辽宁省电力有限公司","","计量现场作业终端与外设收纳箱","现场作业终端与外设收纳箱-存放外设个数:1","个","15","2017-08-20","买方指定仓库地面交货"]
[null,"辽宁省电力有限公司","","采集故障识别模块","现场作业终端外设-采集故障识别模块:有,计量故障识别模块:无,超高频RFID模块:无,蓝牙打印模块:无","个","15","2017-07-20","买方指定仓库地面交货"]
[null,"辽宁省电力有限公司","","单相计量故障识别模块","现场作业终端外设-采集故障识别模块:无,计量故障识别模块:单相,超高频RFID模块:无,蓝牙打印模块:无","个","15","2017-07-20","买方指定仓库地面交货"]
[null,"辽宁省电力有限公司","","计量现场作业终端","现场作业终端-屏幕尺寸范围:≥7.0英寸,购电卡接口:有","台","15","2017-07-20","买方指定仓库地面交货"]
[null,"辽宁省电力有限公司","","三相计量故障识别模块","现场作业终端外设-采集故障识别模块:无,计量故障识别模块:三相,超高频RFID模块:无,蓝牙打印模块:无","个","15","2017-07-20","买方指定仓库地面交货"]
[null,"辽宁省电力有限公司","","2级单相费控智能电能表（模块-远程-开关内置-电池可换）","单相智能电能表-准确度等级:2级,费控方式:远程/电池可换,负荷开关:内置,通信模块接口:有,电压规格:220V,电流规格:5A","只","73450","2017-08-31","买方指定仓库地面交货"]
[null,"辽宁省电力有限公司","","2级单相费控智能电能表（模块-远程-开关内置-电池可换）","单相智能电能表-准确度等级:2级,费控方式:远程/电池可换,负荷开关:内置,通信模块接口:有,电压规格:220V,电流规格:5A","只","12000","2017-08-20","买方指定仓库地面交货"]
[null,"辽宁省电力有限公司","","2级单相费控智能电能表（模块-远程-开关内置-电池可换）","单相智能电能表-准确度等级:2级,费控方式:远程/电池可换,负荷开关:内置,通信模块接口:有,电压规格:220V,电流规格:5A","只","38622","2017-07-24","买方指定仓库地面交货"]
[null,"辽宁省电力有限公司","","2级单相费控智能电能表（模块-远程-开关内置-电池可换）","单相智能电能表-准确度等级:2级,费控方式:远程/电池可换,负荷开关:内置,通信模块接口:有,电压规格:220V,电流规格:5A","只","40075","2017-09-18","买方指定仓库地面交货"]
[null,"辽宁省电力有限公司","","2级单相表本地通信单元（窄带）","通信单元-通信单元类别:本地,适用终端/表类型:2级单相表,通信方式:窄带载波,频率范围/中心频率:421kHz,调制方式:BFSK","只","10000","2017-07-20","买方指定仓库地面交货"]
[null,"辽宁省电力有限公司","","2级单相表本地通信单元（宽带）","通信单元-通信单元类别:本地,适用终端/表类型:2级单相表,通信方式:宽带载波,频率范围/中心频率:2～12MHz,调制方式:OFDM","只","31000","2017-09-21","买方指定仓库地面交货"]
[null,"辽宁省电力有限公司","","计量现场作业终端","现场作业终端-屏幕尺寸范围:(4.0～7.0)英寸,购电卡接口:有","台","32","2017-08-25","买方指定仓库地面交货"]
[null,"辽宁省电力有限公司","","采集故障识别模块","现场作业终端外设-采集故障识别模块:有,计量故障识别模块:无,超高频RFID模块:无,蓝牙打印模块:无","个","32","2017-08-25","买方指定仓库地面交货"]
[null,"辽宁省电力有限公司","","单相计量故障识别模块","现场作业终端外设-采集故障识别模块:无,计量故障识别模块:单相,超高频RFID模块:无,蓝牙打印模块:无","个","32","2017-08-25","买方指定仓库地面交货"]
[null,"辽宁省电力有限公司","","三相计量故障识别模块","现场作业终端外设-采集故障识别模块:无,计量故障识别模块:三相,超高频RFID模块:无,蓝牙打印模块:无","个","32","2017-08-25","买方指定仓库地面交货"]
[null,"辽宁省电力有限公司","","超高频RFID模块","现场作业终端外设-采集故障识别模块:无,计量故障识别模块:无,超高频RFID模块:有,蓝牙打印模块:无","个","32","2017-08-25","买方指定仓库地面交货"]
[null,"辽宁省电力有限公司","","三相计量故障识别模块","现场作业终端外设-采集故障识别模块:无,计量故障识别模块:三相,超高频RFID模块:无,蓝牙打印模块:无","个","15","2017-08-22","买方指定仓库地面交货"]
[null,"辽宁省电力有限公司","","超高频RFID模块","现场作业终端外设-采集故障识别模块:无,计量故障识别模块:无,超高频RFID模块:有,蓝牙打印模块:无","个","15","2017-08-22","买方指定仓库地面交货"]
[null,"辽宁省电力有限公司","","现场打印模块","现场作业终端外设-采集故障识别模块:无,计量故障识别模块:无,超高频RFID模块:无,蓝牙打印模块:有","个","15","2017-08-22","买方指定仓库地面交货"]
[null,"辽宁省电力有限公司","","计量现场作业终端","现场作业终端-屏幕尺寸范围:≥7.0英寸,购电卡接口:有","台","15","2017-08-22","买方指定仓库地面交货"]
[null,"辽宁省电力有限公司","","计量现场作业终端与外设收纳箱","现场作业终端与外设收纳箱-存放外设个数:4","个","15","2017-08-22","买方指定仓库地面交货"]
[null,"辽宁省电力有限公司","","三相计量故障识别模块","现场作业终端外设-采集故障识别模块:无,计量故障识别模块:三相,超高频RFID模块:无,蓝牙打印模块:无","个","15","2017-09-21","买方指定仓库地面交货"]
[null,"辽宁省电力有限公司","","计量现场作业终端与外设收纳箱","现场作业终端与外设收纳箱-存放外设个数:4","个","15","2017-09-21","买方指定仓库地面交货"]
[null,"辽宁省电力有限公司","","超高频RFID模块","现场作业终端外设-采集故障识别模块:无,计量故障识别模块:无,超高频RFID模块:有,蓝牙打印模块:无","个","15","2017-09-21","买方指定仓库地面交货"]
[null,"辽宁省电力有限公司","","现场打印模块","现场作业终端外设-采集故障识别模块:无,计量故障识别模块:无,超高频RFID模块:无,蓝牙打印模块:有","个","15","2017-09-21","买方指定仓库地面交货"]
[null,"辽宁省电力有限公司","","采集故障识别模块","现场作业终端外设-采集故障识别模块:有,计量故障识别模块:无,超高频RFID模块:无,蓝牙打印模块:无","个","12","2017-07-20","买方指定仓库地面交货"]
[null,"辽宁省电力有限公司","","计量现场作业终端","现场作业终端-屏幕尺寸范围:(4.0～7.0)英寸,购电卡接口:有","台","15","2017-09-18","买方指定仓库地面交货"]
[null,"辽宁省电力有限公司","","采集故障识别模块","现场作业终端外设-采集故障识别模块:有,计量故障识别模块:无,超高频RFID模块:无,蓝牙打印模块:无","个","15","2017-09-18","买方指定仓库地面交货"]
[null,"辽宁省电力有限公司","","单相计量故障识别模块","现场作业终端外设-采集故障识别模块:无,计量故障识别模块:单相,超高频RFID模块:无,蓝牙打印模块:无","个","15","2017-09-18","买方指定仓库地面交货"]
[null,"辽宁省电力有限公司","","三相计量故障识别模块","现场作业终端外设-采集故障识别模块:无,计量故障识别模块:三相,超高频RFID模块:无,蓝牙打印模块:无","个","15","2017-09-18","买方指定仓库地面交货"]
[null,"辽宁省电力有限公司","","超高频RFID模块","现场作业终端外设-采集故障识别模块:无,计量故障识别模块:无,超高频RFID模块:有,蓝牙打印模块:无","个","15","2017-09-18","买方指定仓库地面交货"]
[null,"辽宁省电力有限公司","","单相计量故障识别模块","现场作业终端外设-采集故障识别模块:无,计量故障识别模块:单相,超高频RFID模块:无,蓝牙打印模块:无","个","15","2017-08-20","买方指定仓库地面交货"]
[null,"辽宁省电力有限公司","","三相计量故障识别模块","现场作业终端外设-采集故障识别模块:无,计量故障识别模块:三相,超高频RFID模块:无,蓝牙打印模块:无","个","15","2017-08-20","买方指定仓库地面交货"]
[null,"辽宁省电力有限公司","","采集故障识别模块","现场作业终端外设-采集故障识别模块:有,计量故障识别模块:无,超高频RFID模块:无,蓝牙打印模块:无","个","15","2017-08-20","买方指定仓库地面交货"]
[null,"辽宁省电力有限公司","","现场打印模块","现场作业终端外设-采集故障识别模块:无,计量故障识别模块:无,超高频RFID模块:无,蓝牙打印模块:有","个","15","2017-08-20","买方指定仓库地面交货"]
[null,"辽宁省电力有限公司","","超高频RFID模块","现场作业终端外设-采集故障识别模块:无,计量故障识别模块:无,超高频RFID模块:有,蓝牙打印模块:无","个","15","2017-08-20","买方指定仓库地面交货"]
[null,"辽宁省电力有限公司","","2级单相表本地通信单元（窄带）","通信单元-通信单元类别:本地,适用终端/表类型:2级单相表,通信方式:窄带载波,频率范围/中心频率:270kHz,调制方式:BFSK","只","38622","2017-07-24","买方指定仓库地面交货"]
[null,"辽宁省电力有限公司","","计量现场作业终端与外设收纳箱","现场作业终端与外设收纳箱-存放外设个数:4","个","32","2017-08-25","买方指定仓库地面交货"]
[null,"辽宁省电力有限公司","","计量现场作业终端","现场作业终端-屏幕尺寸范围:≥7.0英寸,购电卡接口:有","台","36","2017-08-31","买方指定仓库地面交货"]
[null,"辽宁省电力有限公司","","采集故障识别模块","现场作业终端外设-采集故障识别模块:有,计量故障识别模块:无,超高频RFID模块:无,蓝牙打印模块:无","个","36","2017-08-31","买方指定仓库地面交货"]
[null,"辽宁省电力有限公司","","单相计量故障识别模块","现场作业终端外设-采集故障识别模块:无,计量故障识别模块:单相,超高频RFID模块:无,蓝牙打印模块:无","个","36","2017-08-31","买方指定仓库地面交货"]
[null,"辽宁省电力有限公司","","超高频RFID模块","现场作业终端外设-采集故障识别模块:无,计量故障识别模块:无,超高频RFID模块:有,蓝牙打印模块:无","个","36","2017-08-31","买方指定仓库地面交货"]
[null,"辽宁省电力有限公司","","现场打印模块","现场作业终端外设-采集故障识别模块:无,计量故障识别模块:无,超高频RFID模块:无,蓝牙打印模块:有","个","36","2017-08-31","买方指定仓库地面交货"]
[null,"辽宁省电力有限公司","","采集故障识别模块","现场作业终端外设-采集故障识别模块:有,计量故障识别模块:无,超高频RFID模块:无,蓝牙打印模块:无","个","15","2017-07-24","买方指定仓库地面交货"]
[null,"辽宁省电力有限公司","","单相计量故障识别模块","现场作业终端外设-采集故障识别模块:无,计量故障识别模块:单相,超高频RFID模块:无,蓝牙打印模块:无","个","15","2017-07-24","买方指定仓库地面交货"]
[null,"辽宁省电力有限公司","","三相计量故障识别模块","现场作业终端外设-采集故障识别模块:无,计量故障识别模块:三相,超高频RFID模块:无,蓝牙打印模块:无","个","15","2017-07-24","买方指定仓库地面交货"]
[null,"辽宁省电力有限公司","","超高频RFID模块","现场作业终端外设-采集故障识别模块:无,计量故障识别模块:无,超高频RFID模块:有,蓝牙打印模块:无","个","15","2017-07-24","买方指定仓库地面交货"]
[null,"辽宁省电力有限公司","","计量现场作业终端与外设收纳箱","现场作业终端与外设收纳箱-存放外设个数:4","个","15","2017-07-24","买方指定仓库地面交货"]
[null,"辽宁省电力有限公司","","计量现场作业终端","现场作业终端-屏幕尺寸范围:(4.0～7.0)英寸,购电卡接口:有","台","15","2017-08-20","买方指定仓库地面交货"]
[null,"辽宁省电力有限公司","","计量现场作业终端与外设收纳箱","现场作业终端与外设收纳箱-存放外设个数:2","个","15","2017-08-20","买方指定仓库地面交货"]
[null,"辽宁省电力有限公司","","采集故障识别模块","现场作业终端外设-采集故障识别模块:有,计量故障识别模块:无,超高频RFID模块:无,蓝牙打印模块:无","个","15","2017-08-20","买方指定仓库地面交货"]
[null,"辽宁省电力有限公司","","单相计量故障识别模块","现场作业终端外设-采集故障识别模块:无,计量故障识别模块:单相,超高频RFID模块:无,蓝牙打印模块:无","个","15","2017-08-20","买方指定仓库地面交货"]
[null,"辽宁省电力有限公司","","三相计量故障识别模块","现场作业终端外设-采集故障识别模块:无,计量故障识别模块:三相,超高频RFID模块:无,蓝牙打印模块:无","个","28","2017-07-25","买方指定仓库地面交货"]
["包37SD1","山东电力集团公司","","2级单相费控智能电能表（模块-远程-开关内置-电池可换）","单相智能电能表-准确度等级:2级,费控方式:远程/电池可换,负荷开关:内置,通信模块接口:有,电压规格:220V,电流规格:5A","只","450000","2018-06-30","买方指定仓库地面交货"]
["包37SD2","山东电力集团公司","","2级单相费控智能电能表（模块-远程-开关内置-电池可换）","单相智能电能表-准确度等级:2级,费控方式:远程/电池可换,负荷开关:内置,通信模块接口:有,电压规格:220V,电流规格:5A","只","450000","2018-06-30","买方指定仓库地面交货"]
["包37SD3","山东电力集团公司","","2级单相费控智能电能表（模块-远程-开关内置-电池可换）","单相智能电能表-准确度等级:2级,费控方式:远程/电池可换,负荷开关:内置,通信模块接口:有,电压规格:220V,电流规格:5A","只","360000","2018-06-30","买方指定仓库地面交货"]
[null,"山东电力集团公司","","2级单相表本地通信单元（窄带）","通信单元-通信单元类别:本地,适用终端/表类型:2级单相表,通信方式:窄带载波,频率范围/中心频率:421kHz,调制方式:BFSK","只","183436","2018-06-30","买方指定仓库地面交货"]
[null,"山东电力集团公司","","2级单相表本地通信单元（窄带）","通信单元-通信单元类别:本地,适用终端/表类型:2级单相表,通信方式:窄带载波,频率范围/中心频率:其他,调制方式:其他","只","154341","2018-06-30","买方指定仓库地面交货"]
["包38GW1","重庆市电力公司","国网重庆公司2017年营销类物资协议库存招标采购","2级单相表本地通信单元（窄带）","通信单元-通信单元类别:本地,适用终端/表类型:2级单相表,通信方式:窄带载波,频率范围/中心频率:270kHz,调制方式:BFSK","只","52000","2018-06-16","买方指定仓库地面交货"]
[null,"重庆市电力公司","国网重庆公司2017年营销类物资协议库存招标采购","2级单相表本地通信单元（窄带）","通信单元-通信单元类别:本地,适用终端/表类型:2级单相表,通信方式:窄带载波,频率范围/中心频率:421kHz,调制方式:BFSK","只","300000","2018-06-16","买方指定仓库地面交货"]
[null,"重庆市电力公司","国网重庆公司2017年营销类物资协议库存招标采购","计量现场作业终端","现场作业终端-屏幕尺寸范围:(4.0～7.0)英寸,购电卡接口:无","台","400","2018-06-16","买方指定仓库地面交货"]
[null,"重庆市电力公司","国网重庆公司2017年营销类物资协议库存招标采购","2级单相费控智能电能表（模块-远程-开关外置-电池可换）","单相智能电能表-准确度等级:2级,费控方式:远程/电池可换,负荷开关:外置,通信模块接口:有,电压规格:220V,电流规格:10A","只","20000","2018-06-16","买方指定仓库地面交货"]
[null,"重庆市电力公司","国网重庆公司2017年营销类物资协议库存招标采购","2级单相费控智能电能表（模块-远程-开关外置-电池可换）","单相智能电能表-准确度等级:2级,费控方式:远程/电池可换,负荷开关:外置,通信模块接口:有,电压规格:220V,电流规格:10A","只","15000","2018-06-16","买方指定仓库地面交货"]
[null,"重庆市电力公司","国网重庆公司2017年营销类物资协议库存招标采购","2级单相表本地通信单元（窄带）","通信单元-通信单元类别:本地,适用终端/表类型:2级单相表,通信方式:窄带载波,频率范围/中心频率:其他,调制方式:其他","只","70000","2018-06-16","买方指定仓库地面交货"]
[null,"重庆市电力公司","国网重庆公司2017年营销类物资协议库存招标采购","2级单相表本地通信单元（宽带）","通信单元-通信单元类别:本地,适用终端/表类型:2级单相表,通信方式:宽带载波,频率范围/中心频率:2～12MHz,调制方式:OFDM","只","13000","2018-06-16","买方指定仓库地面交货"]
[null,"辽宁省电力有限公司","","2级单相表本地通信单元（窄带）","通信单元-通信单元类别:本地,适用终端/表类型:2级单相表,通信方式:窄带载波,频率范围/中心频率:270kHz,调制方式:BFSK","只","500","2017-07-24","买方指定仓库地面交货"]
[null,"重庆市电力公司","国网重庆公司2017年营销类物资协议库存招标采购","2级单相费控智能电能表（模块-远程-开关外置-电池可换）","单相智能电能表-准确度等级:2级,费控方式:远程/电池可换,负荷开关:外置,通信模块接口:有,电压规格:220V,电流规格:5A","只","120000","2018-06-16","买方指定仓库地面交货"]
[null,"重庆市电力公司","国网重庆公司2017年营销类物资协议库存招标采购","2级单相费控智能电能表（模块-远程-开关外置-电池可换）","单相智能电能表-准确度等级:2级,费控方式:远程/电池可换,负荷开关:外置,通信模块接口:有,电压规格:220V,电流规格:5A","只","280000","2018-06-16","买方指定仓库地面交货"]
[null,"辽宁省电力有限公司","","2级单相费控智能电能表（模块-远程-开关外置-电池可换）","单相智能电能表-准确度等级:2级,费控方式:远程/电池可换,负荷开关:外置,通信模块接口:有,电压规格:220V,电流规格:10A","只","500","2017-07-24","买方指定仓库地面交货"]
["包39GW1","安徽省电力公司","","2级单相费控智能电能表（远程-开关内置-电池可换）","单相智能电能表-准确度等级:2级,费控方式:远程/电池可换,负荷开关:内置,通信模块接口:无,电压规格:220V,电流规格:5A","只","159000","2017-07-10","买方指定仓库地面交货"]
[null,"江苏省电力公司","","2级单相费控智能电能表（远程-开关内置-电池可换）","单相智能电能表-准确度等级:2级,费控方式:远程/电池可换,负荷开关:内置,通信模块接口:无,电压规格:220V,电流规格:5A","只","30000","2018-04-15","买方指定仓库地面交货"]
["包41GW1","新疆电力公司","国家电网公司2017年第一次电能表（含用电信息采集）","2级单相表本地通信单元（窄带）","通信单元-通信单元类别:本地,适用终端/表类型:2级单相表,通信方式:窄带载波,频率范围/中心频率:270kHz,调制方式:BFSK","只","119588","2017-10-30","买方指定仓库车板交货"]
[null,"新疆电力公司","国家电网公司2017年第一次电能表（含用电信息采集）","2级单相表本地通信单元（窄带）","通信单元-通信单元类别:本地,适用终端/表类型:2级单相表,通信方式:窄带载波,频率范围/中心频率:421kHz,调制方式:BFSK","只","313150","2017-10-30","买方指定仓库车板交货"]
[null,"新疆电力公司","国家电网公司2017年第一次电能表（含用电信息采集）","2级单相本地费控智能电能表（模块-CPU卡-开关内置-电池可换）","单相智能电能表-准确度等级:2级,费控方式:本地/电池可换,负荷开关:内置,通信模块接口:有,电压规格:220V,电流规格:5A","只","445398","2017-10-30","买方指定仓库车板交货"]
[null,"安徽省电力公司","","2级单相本地费控智能电能表（模块-CPU卡-开关内置-电池可换）","单相智能电能表-准确度等级:2级,费控方式:本地/电池可换,负荷开关:内置,通信模块接口:有,电压规格:220V,电流规格:5A","只","10000","2017-07-10","买方指定仓库地面交货"]
[null,"辽宁省电力有限公司","","2级单相表本地通信单元（窄带）","通信单元-通信单元类别:本地,适用终端/表类型:2级单相表,通信方式:窄带载波,频率范围/中心频率:421kHz,调制方式:BFSK","只","100","2017-07-20","买方指定仓库地面交货"]
[null,"辽宁省电力有限公司","","2级单相本地费控智能电能表（模块-CPU卡-开关内置-电池可换）","单相智能电能表-准确度等级:2级,费控方式:本地/电池可换,负荷开关:内置,通信模块接口:有,电压规格:220V,电流规格:5A","只","100","2017-07-20","买方指定仓库地面交货"]
[null,"安徽省电力公司","","2级单相表本地通信单元（窄带）","通信单元-通信单元类别:本地,适用终端/表类型:2级单相表,通信方式:窄带载波,频率范围/中心频率:421kHz,调制方式:BFSK","只","10000","2017-07-10","买方指定仓库地面交货"]
[null,"新疆电力公司","国家电网公司2017年第一次电能表（含用电信息采集）","2级单相表本地通信单元（窄带）","通信单元-通信单元类别:本地,适用终端/表类型:2级单相表,通信方式:窄带载波,频率范围/中心频率:132kHz,调制方式:BPSK","只","57200","2017-10-30","买方指定仓库车板交货"]

{"sheet":"1级三相智能电能表","index":1,"n_rows":244,"n_cols":9,"rows_kept":244,"merged":[[0,0,0,8],[1,0,1,8],[3,0,7,0],[8,0,16,0],[17,0,19,0],[20,0,25,0],[27,0,42,0],[43,0,54,0],[55,0,64,0],[65,0,128,0],[129,0,135,0],[136,0,140,0],[141,0,146,0],[147,0,149,0],[150,0,155,0],[156,0,158,0],[159,0,162,0],[163,0,203,0],[204,0,208,0],[209,0,211,0],[216,0,237,0],[238,0,239,0],[240,0,241,0]],"flags":["formulas_cached_only"]}
["国家电网公司2017年第一次电能表及用电信息采集设备招标活动\n货物需求一览表\n(1级三相智能电能表)"]
["分标编号:0711-17OTL03922000-2"]
["包号","项目单位","项目名称","招标货物","物资描述","单位","行数量","交货日期","交货地点"]
["包13GW1","安徽省电力公司","","1级三相费控智能电能表（模块-远程-开关内置）","三相智能电能表-准确度等级:1级,费控方式:远程,负荷开关:内置,通信模块接口:有,电压规格:3×220/380V,电流规格:5A","只","63300","2017-07-10","买方指定仓库地面交货"]
[null,"安徽省电力公司","","1级三相表本地通信单元（窄带）","通信单元-通信单元类别:本地,适用终端/表类型:1级三相表,通信方式:窄带载波,频率范围/中心频率:其他,调制方式:其他","只","940","2017-07-10","买方指定仓库地面交货"]
[null,"上海市电力公司","国网上海公司2017年第一次电能表（含用电信息采集）项目","1级三相费控智能电能表（模块-远程-开关内置）","三相智能电能表-准确度等级:1级,费控方式:远程,负荷开关:内置,通信模块接口:有,电压规格:3×220/380V,电流规格:5A","只","40000","2018-04-30","买方指定仓库车板交货"]
[null,"安徽省电力公司","","1级三相表本地通信单元（窄带）","通信单元-通信单元类别:本地,适用终端/表类型:1级三相表,通信方式:窄带载波,频率范围/中心频率:132kHz,调制方式:BPSK","只","23920","2017-07-10","买方指定仓库地面交货"]
[null,"安徽省电力公司","","1级三相表本地通信单元（窄带）","通信单元-通信单元类别:本地,适用终端/表类型:1级三相表,通信方式:窄带载波,频率范围/中心频率:421kHz,调制方式:BFSK","只","38440","2017-07-10","买方指定仓库地面交货"]
["包13GW2","福建省电力有限公司","国网福建省电力有限公司采购","1级三相表本地通信单元（窄带）","通信单元-通信单元类别:本地,适用终端/表类型:1级三相表,通信方式:窄带载波,频率范围/中心频率:421kHz,调制方式:BFSK","只","16000","2018-06-30","买方指定仓库地面交货"]
[null,"福建省电力有限公司","国网福建省电力有限公司采购","1级三相表本地通信单元（窄带）","通信单元-通信单元类别:本地,适用终端/表类型:1级三相表,通信方式:窄带载波,频率范围/中心频率:其他,调制方式:其他","只","15000","2018-06-30","买方指定仓库地面交货"]
[null,"福建省电力有限公司","国网福建省电力有限公司采购","1级三相费控智能电能表（模块-远程-开关内置）","三相智能电能表-准确度等级:1级,费控方式:远程,负荷开关:内置,通信模块接口:有,电压规格:3×220/380V,电流规格:5A","只","88000","2018-06-30","买方指定仓库地面交货"]
[null,"新疆电力公司","国家电网公司2017年第一次电能表（含用电信息采集）","1级三相费控智能电能表（模块-远程-开关内置）","三相智能电能表-准确度等级:1级,费控方式:远程,负荷开关:内置,通信模块接口:有,电压规格:3×220/380V,电流规格:5A","只","2200","2017-10-30","买方指定仓库车板交货"]
[null,"新疆电力公司","国家电网公司2017年第一次电能表（含用电信息采集）","1级三相表本地通信单元（窄带）","通信单元-通信单元类别:本地,适用终端/表类型:1级三相表,通信方式:窄带载波,频率范围/中心频率:421kHz,调制方式:BFSK","只","1210","2017-10-30","买方指定仓库车板交货"]
[null,"新疆电力公司","国家电网公司2017年第一次电能表（含用电信息采集）","1级三相表本地通信单元（窄带）","通信单元-通信单元类别:本地,适用终端/表类型:1级三相表,通信方式:窄带载波,频率范围/中心频率:270kHz,调制方式:BFSK","只","1210","2017-10-30","买方指定仓库车板交货"]
[null,"福建省电力有限公司","国网福建省电力有限公司采购","1级三相表本地通信单元（窄带）","通信单元-通信单元类别:本地,适用终端/表类型:1级三相表,通信方式:窄带载波,频率范围/中心频率:270kHz,调制方式:BFSK","只","7602","2018-06-30","买方指定仓库地面交货"]
[null,"福建省电力有限公司","国网福建省电力有限公司采购","1级三相表本地通信单元（宽带）","通信单元-通信单元类别:本地,适用终端/表类型:1级三相表,通信方式:宽带载波,频率范围/中心频率:2～12MHz,调制方式:OFDM","只","50000","2018-06-30","买方指定仓库地面交货"]
[null,"福建省电力有限公司","国网福建省电力有限公司采购","1级三相表本地通信单元（窄带）","通信单元-通信单元类别:本地,适用终端/表类型:1级三相表,通信方式:窄带载波,频率范围/中心频率:132kHz,调制方式:BPSK","只","7780","2018-06-30","买方指定仓库地面交货"]
["包13GW3","西藏电力有限公司","国网西藏电力有限公司各供电公司营销专项、电网基建/户表","1级三相费控智能电能表（模块-远程-开关内置）","三相智能电能表-准确度等级:1级,费控方式:远程,负荷开关:内置,通信模块接口:有,电压规格:3×220/380V,电流规格:5A","只","5491","2017-06-30","买方指定仓库地面交货"]
[null,"西藏电力有限公司","国网西藏电力有限公司各供电公司营销专项、电网基建/户表","1级三相表本地通信单元（窄带）","通信单元-通信单元类别:本地,适用终端/表类型:1级三相表,通信方式:窄带载波,频率范围/中心频率:421kHz,调制方式:BFSK","只","5491","2017-06-30","买方指定仓库地面交货"]
[null,"湖北省电力公司","","1级三相费控智能电能表（模块-远程-开关内置）","三相智能电能表-准确度等级:1级,费控方式:远程,负荷开关:内置,通信模块接口:有,电压规格:3×220/380V,电流规格:5A","只","150000","2017-07-31","买方指定仓库地面交货"]
["包13GW4","江西省电力公司","","1级三相表本地通信单元（窄带）","通信单元-通信单元类别:本地,适用终端/表类型:1级三相表,通信方式:窄带载波,频率范围/中心频率:421kHz,调制方式:BFSK","只","2000","2017-09-15","买方指定仓库地面交货"]
[null,"江西省电力公司","","1级三相费控智能电能表（模块-远程-开关内置）","三相智能电能表-准确度等级:1级,费控方式:远程,负荷开关:内置,通信模块接口:有,电压规格:3×220/380V,电流规格:5A","只","77200","2017-09-15","买方指定仓库地面交货"]
[null,"山西省电力公司","","1级三相费控智能电能表（模块-远程-开关内置）","三相智能电能表-准确度等级:1级,费控方式:远程,负荷开关:内置,通信模块接口:有,电压规格:3×220/380V,电流规格:5A","只","31989","2018-04-30","买方指定仓库地面交货"]
[null,"江西省电力公司","","1级三相表本地通信单元（宽带）","通信单元-通信单元类别:本地,适用终端/表类型:1级三相表,通信方式:宽带载波,频率范围/中心频率:2～12MHz,调制方式:OFDM","只","7200","2017-09-15","买方指定仓库地面交货"]
[null,"江西省电力公司","","1级三相表本地通信单元（窄带）","通信单元-通信单元类别:本地,适用终端/表类型:1级三相表,通信方式:窄带载波,频率范围/中心频率:270kHz,调制方式:BFSK","只","38000","2017-09-15","买方指定仓库地面交货"]
[null,"江西省电力公司","","1级三相表本地通信单元（窄带）","通信单元-通信单元类别:本地,适用终端/表类型:1级三相表,通信方式:窄带载波,频率范围/中心频率:其他,调制方式:其他","只","30000","2017-09-15","买方指定仓库地面交货"]
["包13HB1","湖北省电力公司","","1级三相费控智能电能表（模块-远程-开关内置）","三相智能电能表-准确度等级:1级,费控方式:远程,负荷开关:内置,通信模块接口:有,电压规格:3×220/380V,电流规格:5A","只","50000","2017-07-31","买方指定仓库地面交货"]
["包13MD1","内蒙古东部电力有限公司","","1级三相费控智能电能表（模块-远程-开关内置）","三相智能电能表-准确度等级:1级,费控方式:远程,负荷开关:内置,通信模块接口:有,电压规格:3×220/380V,电流规格:5A","只","1205","2017-12-31","买方指定仓库地面交货"]
[null,"内蒙古东部电力有限公司","","1级三相表本地通信单元（宽带）","通信单元-通信单元类别:本地,适用终端/表类型:1级三相表,通信方式:宽带载波,频率范围/中心频率:2～12MHz,调制方式:OFDM","只","29200","2017-12-31","买方指定仓库地面交货"]
[null,"内蒙古东部电力有限公司","","1级三相表本地通信单元（宽带）","通信单元-通信单元类别:本地,适用终端/表类型:1级三相表,通信方式:宽带载波,频率范围/中心频率:2～12MHz,调制方式:OFDM","只","10558","2017-12-31","买方指定仓库地面交货"]
[null,"内蒙古东部电力有限公司","","1级三相表本地通信单元（宽带）","通信单元-通信单元类别:本地,适用终端/表类型:1级三相表,通信方式:宽带载波,频率范围/中心频率:2～12MHz,调制方式:OFDM","只","24056","2017-12-31","买方指定仓库地面交货"]
[null,"内蒙古东部电力有限公司","","1级三相费控智能电能表（模块-远程-开关内置）","三相智能电能表-准确度等级:1级,费控方式:远程,负荷开关:内置,通信模块接口:有,电压规格:3×220/380V,电流规格:5A","只","1","2017-12-31","买方指定仓库地面交货"]
[null,"内蒙古东部电力有限公司","","1级三相费控智能电能表（模块-远程-开关内置）","三相智能电能表-准确度等级:1级,费控方式:远程,负荷开关:内置,通信模块接口:有,电压规格:3×220/380V,电流规格:5A","只","330","2017-12-31","买方指定仓库地面交货"]
[null,"内蒙古东部电力有限公司","","1级三相费控智能电能表（模块-远程-开关内置）","三相智能电能表-准确度等级:1级,费控方式:远程,负荷开关:内置,通信模块接口:有,电压规格:3×220/380V,电流规格:5A","只","917","2017-12-31","买方指定仓库地面交货"]
[null,"内蒙古东部电力有限公司","","1级三相费控智能电能表（模块-远程-开关内置）","三相智能电能表-准确度等级:1级,费控方式:远程,负荷开关:内置,通信模块接口:有,电压规格:3×220/380V,电流规格:5A","只","18570","2017-12-31","买方指定仓库地面交货"]
[null,"内蒙古东部电力有限公司","","1级三相费控智能电能表（模块-远程-开关内置）","三相智能电能表-准确度等级:1级,费控方式:远程,负荷开关:内置,通信模块接口:有,电压规格:3×220/380V,电流规格:5A","只","4604","2017-12-31","买方指定仓库地面交货"]
[null,"内蒙古东部电力有限公司","","1级三相费控智能电能表（模块-远程-开关内置）","三相智能电能表-准确度等级:1级,费控方式:远程,负荷开关:内置,通信模块接口:有,电压规格:3×220/380V,电流规格:5A","只","500","2017-12-31","买方指定仓库地面交货"]
[null,"内蒙古东部电力有限公司","","1级三相表本地通信单元（窄带）","通信单元-通信单元类别:本地,适用终端/表类型:1级三相表,通信方式:窄带载波,频率范围/中心频率:421kHz,调制方式:BFSK","只","30192","2017-12-31","买方指定仓库地面交货"]
[null,"内蒙古东部电力有限公司","","1级三相费控智能电能表（模块-远程-开关内置）","三相智能电能表-准确度等级:1级,费控方式:远程,负荷开关:内置,通信模块接口:有,电压规格:3×220/380V,电流规格:5A","只","25","2017-12-31","买方指定仓库地面交货"]
[null,"内蒙古东部电力有限公司","","1级三相费控智能电能表（模块-远程-开关内置）","三相智能电能表-准确度等级:1级,费控方式:远程,负荷开关:内置,通信模块接口:有,电压规格:3×220/380V,电流规格:5A","只","3692","2017-12-31","买方指定仓库地面交货"]
[null,"内蒙古东部电力有限公司","","1级三相费控智能电能表（模块-远程-开关内置）","三相智能电能表-准确度等级:1级,费控方式:远程,负荷开关:内置,通信模块接口:有,电压规格:3×220/380V,电流规格:5A","只","136","2017-12-31","买方指定仓库地面交货"]
[null,"内蒙古东部电力有限公司","","1级三相费控智能电能表（模块-远程-开关内置）","三相智能电能表-准确度等级:1级,费控方式:远程,负荷开关:内置,通信模块接口:有,电压规格:3×220/380V,电流规格:5A","只","8240","2017-12-31","买方指定仓库地面交货"]
[null,"内蒙古东部电力有限公司","","1级三相费控智能电能表（模块-远程-开关内置）","三相智能电能表-准确度等级:1级,费控方式:远程,负荷开关:内置,通信模块接口:有,电压规格:3×220/380V,电流规格:5A","只","48459","2017-12-31","买方指定仓库地面交货"]
["包14GW1","安徽省电力公司","","1级三相表本地通信单元（窄带）","通信单元-通信单元类别:本地,适用终端/表类型:1级三相表,通信方式:窄带载波,频率范围/中心频率:421kHz,调制方式:BFSK","只","11200","2017-07-10","买方指定仓库地面交货"]
[null,"天津市电力公司","","1级三相表本地通信单元（窄带）","通信单元-通信单元类别:本地,适用终端/表类型:1级三相表,通信方式:窄带载波,频率范围/中心频率:132kHz,调制方式:BPSK","只","200","2017-12-31","买方指定仓库地面交货"]
[null,"天津市电力公司","","1级三相表本地通信单元（窄带）","通信单元-通信单元类别:本地,适用终端/表类型:1级三相表,通信方式:窄带载波,频率范围/中心频率:270kHz,调制方式:BFSK","只","6000","2017-12-31","买方指定仓库地面交货"]
[null,"天津市电力公司","","1级三相表本地通信单元（窄带）","通信单元-通信单元类别:本地,适用终端/表类型:1级三相表,通信方式:窄带载波,频率范围/中心频率:421kHz,调制方式:BFSK","只","4000","2017-12-31","买方指定仓库地面交货"]
[null,"天津市电力公司","","1级三相表本地通信单元（窄带）","通信单元-通信单元类别:本地,适用终端/表类型:1级三相表,通信方式:窄带载波,频率范围/中心频率:其他,调制方式:其他","只","7400","2017-12-31","买方指定仓库地面交货"]
[null,"天津市电力公司","","1级三相表本地通信单元（宽带）","通信单元-通信单元类别:本地,适用终端/表类型:1级三相表,通信方式:宽带载波,频率范围/中心频率:2～12MHz,调制方式:OFDM","只","2400","2017-12-31","买方指定仓库地面交货"]
[null,"新疆电力公司","国家电网公司2017年第一次电能表（含用电信息采集）","1级三相表本地通信单元（窄带）","通信单元-通信单元类别:本地,适用终端/表类型:1级三相表,通信方式:窄带载波,频率范围/中心频率:132kHz,调制方式:BPSK","只","7700","2017-10-30","买方指定仓库车板交货"]
[null,"新疆电力公司","国家电网公司2017年第一次电能表（含用电信息采集）","1级三相表本地通信单元（窄带）","通信单元-通信单元类别:本地,适用终端/表类型:1级三相表,通信方式:窄带载波,频率范围/中心频率:270kHz,调制方式:BFSK","只","6714","2017-10-30","买方指定仓库车板交货"]
[null,"新疆电力公司","国家电网公司2017年第一次电能表（含用电信息采集）","1级三相表本地通信单元（窄带）","通信单元-通信单元类别:本地,适用终端/表类型:1级三相表,通信方式:窄带载波,频率范围/中心频率:421kHz,调制方式:BFSK","只","10387","2017-10-30","买方指定仓库车板交货"]
[null,"新疆电力公司","国家电网公司2017年第一次电能表（含用电信息采集）","1级三相费控智能电能表（模块-CPU卡-开关内置）","三相智能电能表-准确度等级:1级,费控方式:本地,负荷开关:内置,通信模块接口:有,电压规格:3×220/380V,电流规格:5A","只","22547","2017-10-30","买方指定仓库车板交货"]
[null,"天津市电力公司","","1级三相费控智能电能表（模块-CPU卡-开关内置）","三相智能电能表-准确度等级:1级,费控方式:本地,负荷开关:内置,通信模块接口:有,电压规格:3×220/380V,电流规格:5A","只","20000","2017-12-31","买方指定仓库地面交货"]
[null,"安徽省电力公司","","1级三相费控智能电能表（模块-CPU卡-开关内置）","三相智能电能表-准确度等级:1级,费控方式:本地,负荷开关:内置,通信模块接口:有,电压规格:3×220/380V,电流规格:5A","只","11200","2017-07-10","买方指定仓库地面交货"]
["包16GW1","福建省电力有限公司","国网福建省电力有限公司采购","1级三相表本地通信单元（窄带）","通信单元-通信单元类别:本地,适用终端/表类型:1级三相表,通信方式:窄带载波,频率范围/中心频率:421kHz,调制方式:BFSK","只","1000","2018-06-30","买方指定仓库地面交货"]
[null,"福建省电力有限公司","国网福建省电力有限公司采购","1级三相表本地通信单元（窄带）","通信单元-通信单元类别:本地,适用终端/表类型:1级三相表,通信方式:窄带载波,频率范围/中心频率:132kHz,调制方式:BPSK","只","3000","2018-06-30","买方指定仓库地面交货"]
[null,"福建省电力有限公司","国网福建省电力有限公司采购","1级三相表本地通信单元（窄带）","通信单元-通信单元类别:本地,适用终端/表类型:1级三相表,通信方式:窄带载波,频率范围/中心频率:270kHz,调制方式:BFSK","只","10000","2018-06-30","买方指定仓库地面交货"]
[null,"福建省电力有限公司","国网福建省电力有限公司采购","1级三相费控智能电能表（模块-远程-开关外置）","三相智能电能表-准确度等级:1级,费控方式:远程,负荷开关:外置,通信模块接口:有,电压规格:3×220/380V,电流规格:1.5A","只","14000","2018-06-30","买方指定仓库地面交货"]
[null,"上海市电力公司","国网上海公司2017年第一次电能表（含用电信息采集）项目","1级三相费控智能电能表（模块-远程-开关外置）","三相智能电能表-准确度等级:1级,费控方式:远程,负荷开关:外置,通信模块接口:有,电压规格:3×220/380V,电流规格:10A","只","10000","2018-04-30","买方指定仓库车板交货"]
[null,"重庆市电力公司","国网重庆公司2017年营销类物资协议库存招标采购","1级三相表本地通信单元（窄带）","通信单元-通信单元类别:本地,适用终端/表类型:1级三相表,通信方式:窄带载波,频率范围/中心频率:270kHz,调制方式:BFSK","只","5000","2018-06-16","买方指定仓库地面交货"]
[null,"重庆市电力公司","国网重庆公司2017年营销类物资协议库存招标采购","1级三相表本地通信单元（窄带）","通信单元-通信单元类别:本地,适用终端/表类型:1级三相表,通信方式:窄带载波,频率范围/中心频率:其他,调制方式:其他","只","10000","2018-06-16","买方指定仓库地面交货"]
[null,"重庆市电力公司","国网重庆公司2017年营销类物资协议库存招标采购","1级三相费控智能电能表（模块-远程-开关外置）","三相智能电能表-准确度等级:1级,费控方式:远程,负荷开关:外置,通信模块接口:有,电压规格:3×220/380V,电流规格:10A","只","7000","2018-06-16","买方指定仓库地面交货"]
[null,"重庆市电力公司","国网重庆公司2017年营销类物资协议库存招标采购","1级三相费控智能电能表（模块-远程-开关外置）","三相智能电能表-准确度等级:1级,费控方式:远程,负荷开关:外置,通信模块接口:有,电压规格:3×220/380V,电流规格:5A","只","23000","2018-06-16","买方指定仓库地面交货"]
[null,"重庆市电力公司","国网重庆公司2017年营销类物资协议库存招标采购","1级三相表本地通信单元（窄带）","通信单元-通信单元类别:本地,适用终端/表类型:1级三相表,通信方式:窄带载波,频率范围/中心频率:421kHz,调制方式:BFSK","只","15000","2018-06-16","买方指定仓库地面交货"]
["包16GW2","辽宁省电力有限公司","","1级三相费控智能电能表（模块-远程-开关外置）","三相智能电能表-准确度等级:1级,费控方式:远程,负荷开关:外置,通信模块接口:有,电压规格:3×220/380V,电流规格:5A","只","4300","2017-08-31","买方指定仓库地面交货"]
[null,"辽宁省电力有限公司","","1级三相费控智能电能表（模块-远程-开关外置）","三相智能电能表-准确度等级:1级,费控方式:远程,负荷开关:外置,通信模块接口:有,电压规格:3×220/380V,电流规格:5A","只","3000","2017-08-25","买方指定仓库地面交货"]
[null,"辽宁省电力有限公司","","1级三相费控智能电能表（模块-远程-开关外置）","三相智能电能表-准确度等级:1级,费控方式:远程,负荷开关:外置,通信模块接口:有,电压规格:3×220/380V,电流规格:5A","只","600","2017-07-20","买方指定仓库地面交货"]
[null,"辽宁省电力有限公司","","1级三相费控智能电能表（模块-远程-开关外置）","三相智能电能表-准确度等级:1级,费控方式:远程,负荷开关:外置,通信模块接口:有,电压规格:3×220/380V,电流规格:10A","只","1800","2017-09-21","买方指定仓库地面交货"]
[null,"辽宁省电力有限公司","","1级三相费控智能电能表（模块-远程-开关外置）","三相智能电能表-准确度等级:1级,费控方式:远程,负荷开关:外置,通信模块接口:有,电压规格:3×220/380V,电流规格:1.5A","只","600","2017-09-21","买方指定仓库地面交货"]
[null,"辽宁省电力有限公司","","1级三相费控智能电能表（模块-远程-开关外置）","三相智能电能表-准确度等级:1级,费控方式:远程,负荷开关:外置,通信模块接口:有,电压规格:3×220/380V,电流规格:1.5A","只","400","2017-07-20","买方指定仓库地面交货"]
[null,"辽宁省电力有限公司","","1级三相费控智能电能表（模块-远程-开关外置）","三相智能电能表-准确度等级:1级,费控方式:远程,负荷开关:外置,通信模块接口:有,电压规格:3×220/380V,电流规格:1.5A","只","700","2017-09-18","买方指定仓库地面交货"]
[null,"辽宁省电力有限公司","","1级三相表本地通信单元（窄带）","通信单元-通信单元类别:本地,适用终端/表类型:1级三相表,通信方式:窄带载波,频率范围/中心频率:421kHz,调制方式:BFSK","只","4300","2017-08-31","买方指定仓库地面交货"]
[null,"辽宁省电力有限公司","","1级三相表本地通信单元（窄带）","通信单元-通信单元类别:本地,适用终端/表类型:1级三相表,通信方式:窄带载波,频率范围/中心频率:270kHz,调制方式:BFSK","只","200","2017-07-25","买方指定仓库地面交货"]
[null,"山西省电力公司","","1级三相费控智能电能表（模块-远程-开关外置）","三相智能电能表-准确度等级:1级,费控方式:远程,负荷开关:外置,通信模块接口:有,电压规格:3×220/380V,电流规格:1.5A","只","7559","2018-04-30","买方指定仓库地面交货"]
[null,"山西省电力公司","","1级三相费控智能电能表（模块-远程-开关外置）","三相智能电能表-准确度等级:1级,费控方式:远程,负荷开关:外置,通信模块接口:有,电压规格:3×220/380V,电流规格:10A","只","12579","2018-04-30","买方指定仓库地面交货"]
[null,"内蒙古东部电力有限公司","","1级三相表本地通信单元（窄带）","通信单元-通信单元类别:本地,适用终端/表类型:1级三相表,通信方式:窄带载波,频率范围/中心频率:421kHz,调制方式:BFSK","只","347","2017-12-31","买方指定仓库地面交货"]
[null,"内蒙古东部电力有限公司","","1级三相表本地通信单元（宽带）","通信单元-通信单元类别:本地,适用终端/表类型:1级三相表,通信方式:宽带载波,频率范围/中心频率:2～12MHz,调制方式:OFDM","只","600","2017-12-31","买方指定仓库地面交货"]
[null,"内蒙古东部电力有限公司","","1级三相表本地通信单元（窄带）","通信单元-通信单元类别:本地,适用终端/表类型:1级三相表,通信方式:窄带载波,频率范围/中心频率:其他,调制方式:其他","只","1213","2017-12-31","买方指定仓库地面交货"]
[null,"内蒙古东部电力有限公司","","1级三相表本地通信单元（窄带）","通信单元-通信单元类别:本地,适用终端/表类型:1级三相表,通信方式:窄带载波,频率范围/中心频率:270kHz,调制方式:BFSK","只","100","2017-12-31","买方指定仓库地面交货"]
[null,"内蒙古东部电力有限公司","","1级三相表本地通信单元（窄带）","通信单元-通信单元类别:本地,适用终端/表类型:1级三相表,通信方式:窄带载波,频率范围/中心频率:421kHz,调制方式:BFSK","只","200","2017-12-31","买方指定仓库地面交货"]
[null,"内蒙古东部电力有限公司","","1级三相表本地通信单元（窄带）","通信单元-通信单元类别:本地,适用终端/表类型:1级三相表,通信方式:窄带载波,频率范围/中心频率:其他,调制方式:其他","只","972","2017-12-31","买方指定仓库地面交货"]
[null,"内蒙古东部电力有限公司","","1级三相表本地通信单元（窄带）","通信单元-通信单元类别:本地,适用终端/表类型:1级三相表,通信方式:窄带载波,频率范围/中心频率:其他,调制方式:其他","只","153","2017-12-31","买方指定仓库地面交货"]
[null,"内蒙古东部电力有限公司","","1级三相表本地通信单元（宽带）","通信单元-通信单元类别:本地,适用终端/表类型:1级三相表,通信方式:宽带载波,频率范围/中心频率:2～12MHz,调制方式:OFDM","只","3900","2017-12-31","买方指定仓库地面交货"]
[null,"内蒙古东部电力有限公司","","1级三相表本地通信单元（窄带）","通信单元-通信单元类别:本地,适用终端/表类型:1级三相表,通信方式:窄带载波,频率范围/中心频率:132kHz,调制方式:BPSK","只","63","2017-12-31","买方指定仓库地面交货"]
[null,"辽宁省电力有限公司","","1级三相表本地通信单元（窄带）","通信单元-通信单元类别:本地,适用终端/表类型:1级三相表,通信方式:窄带载波,频率范围/中心频率:270kHz,调制方式:BFSK","只","2000","2017-09-15","买方指定仓库地面交货"]
[null,"辽宁省电力有限公司","","1级三相表本地通信单元（窄带）","通信单元-通信单元类别:本地,适用终端/表类型:1级三相表,通信方式:窄带载波,频率范围/中心频率:270kHz,调制方式:BFSK","只","700","2017-09-18","买方指定仓库地面交货"]
[null,"内蒙古东部电力有限公司","","1级三相费控智能电能表（模块-远程-开关外置）","三相智能电能表-准确度等级:1级,费控方式:远程,负荷开关:外置,通信模块接口:有,电压规格:3×220/380V,电流规格:1.5A","只","337","2017-12-31","买方指定仓库地面交货"]
[null,"内蒙古东部电力有限公司","","1级三相费控智能电能表（模块-远程-开关外置）","三相智能电能表-准确度等级:1级,费控方式:远程,负荷开关:外置,通信模块接口:有,电压规格:3×220/380V,电流规格:1.5A","只","112","2017-12-31","买方指定仓库地面交货"]
[null,"内蒙古东部电力有限公司","","1级三相费控智能电能表（模块-远程-开关外置）","三相智能电能表-准确度等级:1级,费控方式:远程,负荷开关:外置,通信模块接口:有,电压规格:3×220/380V,电流规格:1.5A","只","531","2017-12-31","买方指定仓库地面交货"]
[null,"内蒙古东部电力有限公司","","1级三相表本地通信单元（窄带）","通信单元-通信单元类别:本地,适用终端/表类型:1级三相表,通信方式:窄带载波,频率范围/中心频率:421kHz,调制方式:BFSK","只","200","2017-12-31","买方指定仓库地面交货"]
[null,"内蒙古东部电力有限公司","","1级三相表本地通信单元（宽带）","通信单元-通信单元类别:本地,适用终端/表类型:1级三相表,通信方式:宽带载波,频率范围/中心频率:2～12MHz,调制方式:OFDM","只","354","2017-12-31","买方指定仓库地面交货"]
[null,"内蒙古东部电力有限公司","","1级三相表本地通信单元（窄带）","通信单元-通信单元类别:本地,适用终端/表类型:1级三相表,通信方式:窄带载波,频率范围/中心频率:421kHz,调制方式:BFSK","只","300","2017-12-31","买方指定仓库地面交货"]
[null,"内蒙古东部电力有限公司","","1级三相表本地通信单元（宽带）","通信单元-通信单元类别:本地,适用终端/表类型:1级三相表,通信方式:宽带载波,频率范围/中心频率:2～12MHz,调制方式:OFDM","只","500","2017-12-31","买方指定仓库地面交货"]
[null,"内蒙古东部电力有限公司","","1级三相表本地通信单元（窄带）","通信单元-通信单元类别:本地,适用终端/表类型:1级三相表,通信方式:窄带载波,频率范围/中心频率:421kHz,调制方式:BFSK","只","300","2017-12-31","买方指定仓库地面交货"]
[null,"辽宁省电力有限公司","","1级三相费控智能电能表（模块-远程-开关外置）","三相智能电能表-准确度等级:1级,费控方式:远程,负荷开关:外置,通信模块接口:有,电压规格:3×220/380V,电流规格:5A","只","3000","2017-08-25","买方指定仓库地面交货"]
[null,"辽宁省电力有限公司","","1级三相费控智能电能表（模块-远程-开关外置）","三相智能电能表-准确度等级:1级,费控方式:远程,负荷开关:外置,通信模块接口:有,电压规格:3×220/380V,电流规格:5A","只","2000","2017-09-15","买方指定仓库地面交货"]
[null,"辽宁省电力有限公司","","1级三相费控智能电能表（模块-远程-开关外置）","三相智能电能表-准确度等级:1级,费控方式:远程,负荷开关:外置,通信模块接口:有,电压规格:3×220/380V,电流规格:5A","只","200","2017-07-25","买方指定仓库地面交货"]
[null,"辽宁省电力有限公司","","1级三相费控智能电能表（模块-远程-开关外置）","三相智能电能表-准确度等级:1级,费控方式:远程,负荷开关:外置,通信模块接口:有,电压规格:3×220/380V,电流规格:1.5A","只","2200","2017-07-20","买方指定仓库地面交货"]
[null,"辽宁省电力有限公司","","1级三相费控智能电能表（模块-远程-开关外置）","三相智能电能表-准确度等级:1级,费控方式:远程,负荷开关:外置,通信模块接口:有,电压规格:3×220/380V,电流规格:10A","只","6500","2017-07-20","买方指定仓库地面交货"]
[null,"辽宁省电力有限公司","","1级三相表本地通信单元（窄带）","通信单元-通信单元类别:本地,适用终端/表类型:1级三相表,通信方式:窄带载波,频率范围/中心频率:270kHz,调制方式:BFSK","只","3000","2017-08-25","买方指定仓库地面交货"]
[null,"辽宁省电力有限公司","","1级三相表本地通信单元（窄带）","通信单元-通信单元类别:本地,适用终端/表类型:1级三相表,通信方式:窄带载波,频率范围/中心频率:421kHz,调制方式:BFSK","只","3000","2017-08-25","买方指定仓库地面交货"]
[null,"辽宁省电力有限公司","","1级三相表本地通信单元（宽带）","通信单元-通信单元类别:本地,适用终端/表类型:1级三相表,通信方式:宽带载波,频率范围/中心频率:2～12MHz,调制方式:OFDM","只","1800","2017-09-21","买方指定仓库地面交货"]
[null,"辽宁省电力有限公司","","1级三相表本地通信单元（宽带）","通信单元-通信单元类别:本地,适用终端/表类型:1级三相表,通信方式:宽带载波,频率范围/中心频率:2～12MHz,调制方式:OFDM","只","600","2017-09-21","买方指定仓库地面交货"]
[null,"辽宁省电力有限公司","","1级三相表本地通信单元（窄带）","通信单元-通信单元类别:本地,适用终端/表类型:1级三相表,通信方式:窄带载波,频率范围/中心频率:270kHz,调制方式:BFSK","只","600","2017-07-20","买方指定仓库地面交货"]
[null,"辽宁省电力有限公司","","1级三相表本地通信单元（窄带）","通信单元-通信单元类别:本地,适用终端/表类型:1级三相表,通信方式:窄带载波,频率范围/中心频率:421kHz,调制方式:BFSK","只","400","2017-07-20","买方指定仓库地面交货"]
[null,"辽宁省电力有限公司","","1级三相表本地通信单元（窄带）","通信单元-通信单元类别:本地,适用终端/表类型:1级三相表,通信方式:窄带载波,频率范围/中心频率:其他,调制方式:其他","只","2200","2017-07-20","买方指定仓库地面交货"]
[null,"辽宁省电力有限公司","","1级三相表本地通信单元（窄带）","通信单元-通信单元类别:本地,适用终端/表类型:1级三相表,通信方式:窄带载波,频率范围/中心频率:其他,调制方式:其他","只","6500","2017-07-20","买方指定仓库地面交货"]
[null,"内蒙古东部电力有限公司","","1级三相表本地通信单元（窄带）","通信单元-通信单元类别:本地,适用终端/表类型:1级三相表,通信方式:窄带载波,频率范围/中心频率:421kHz,调制方式:BFSK","只","100","2017-12-31","买方指定仓库地面交货"]
[null,"黑龙江省电力有限公司","","1级三相费控智能电能表（模块-远程-开关外置）","三相智能电能表-准确度等级:1级,费控方式:远程,负荷开关:外置,通信模块接口:有,电压规格:3×220/380V,电流规格:5A","只","2968","2018-04-20","买方指定仓库地面交货"]
[null,"黑龙江省电力有限公司","","1级三相费控智能电能表（模块-远程-开关外置）","三相智能电能表-准确度等级:1级,费控方式:远程,负荷开关:外置,通信模块接口:有,电压规格:3×220/380V,电流规格:1.5A","只","7661","2018-04-20","买方指定仓库地面交货"]
[null,"黑龙江省电力有限公司","","1级三相表本地通信单元（宽带）","通信单元-通信单元类别:本地,适用终端/表类型:1级三相表,通信方式:宽带载波,频率范围/中心频率:2～12MHz,调制方式:OFDM","只","380","2018-04-20","买方指定仓库地面交货"]
[null,"黑龙江省电力有限公司","","1级三相费控智能电能表（模块-远程-开关外置）","三相智能电能表-准确度等级:1级,费控方式:远程,负荷开关:外置,通信模块接口:有,电压规格:3×220/380V,电流规格:10A","只","4676","2018-04-20","买方指定仓库地面交货"]
[null,"黑龙江省电力有限公司","","1级三相表本地通信单元（窄带）","通信单元-通信单元类别:本地,适用终端/表类型:1级三相表,通信方式:窄带载波,频率范围/中心频率:421kHz,调制方式:BFSK","只","9123","2018-04-20","买方指定仓库地面交货"]
[null,"黑龙江省电力有限公司","","1级三相表本地通信单元（窄带）","通信单元-通信单元类别:本地,适用终端/表类型:1级三相表,通信方式:窄带载波,频率范围/中心频率:270kHz,调制方式:BFSK","只","5922","2018-04-20","买方指定仓库地面交货"]
[null,"内蒙古东部电力有限公司","","1级三相费控智能电能表（模块-远程-开关外置）","三相智能电能表-准确度等级:1级,费控方式:远程,负荷开关:外置,通信模块接口:有,电压规格:3×220/380V,电流规格:1.5A","只","4735","2017-12-31","买方指定仓库地面交货"]
[null,"内蒙古东部电力有限公司","","1级三相费控智能电能表（模块-远程-开关外置）","三相智能电能表-准确度等级:1级,费控方式:远程,负荷开关:外置,通信模块接口:有,电压规格:3×220/380V,电流规格:1.5A","只","44","2017-12-31","买方指定仓库地面交货"]
[null,"内蒙古东部电力有限公司","","1级三相费控智能电能表（模块-远程-开关外置）","三相智能电能表-准确度等级:1级,费控方式:远程,负荷开关:外置,通信模块接口:有,电压规格:3×220/380V,电流规格:1.5A","只","570","2017-12-31","买方指定仓库地面交货"]
[null,"内蒙古东部电力有限公司","","1级三相费控智能电能表（模块-远程-开关外置）","三相智能电能表-准确度等级:1级,费控方式:远程,负荷开关:外置,通信模块接口:有,电压规格:3×220/380V,电流规格:10A","只","7075","2017-12-31","买方指定仓库地面交货"]
[null,"内蒙古东部电力有限公司","","1级三相费控智能电能表（模块-远程-开关外置）","三相智能电能表-准确度等级:1级,费控方式:远程,负荷开关:外置,通信模块接口:有,电压规格:3×220/380V,电流规格:1.5A","只","10352","2017-12-31","买方指定仓库地面交货"]
[null,"内蒙古东部电力有限公司","","1级三相表本地通信单元（窄带）","通信单元-通信单元类别:本地,适用终端/表类型:1级三相表,通信方式:窄带载波,频率范围/中心频率:421kHz,调制方式:BFSK","只","800","2017-12-31","买方指定仓库地面交货"]
[null,"内蒙古东部电力有限公司","","1级三相表本地通信单元（宽带）","通信单元-通信单元类别:本地,适用终端/表类型:1级三相表,通信方式:宽带载波,频率范围/中心频率:2～12MHz,调制方式:OFDM","只","136","2017-12-31","买方指定仓库地面交货"]
[null,"内蒙古东部电力有限公司","","1级三相表本地通信单元（宽带）","通信单元-通信单元类别:本地,适用终端/表类型:1级三相表,通信方式:宽带载波,频率范围/中心频率:2～12MHz,调制方式:OFDM","只","22","2017-12-31","买方指定仓库地面交货"]
[null,"内蒙古东部电力有限公司","","1级三相表本地通信单元（窄带）","通信单元-通信单元类别:本地,适用终端/表类型:1级三相表,通信方式:窄带载波,频率范围/中心频率:421kHz,调制方式:BFSK","只","20","2017-12-31","买方指定仓库地面交货"]
[null,"内蒙古东部电力有限公司","","1级三相表本地通信单元（宽带）","通信单元-通信单元类别:本地,适用终端/表类型:1级三相表,通信方式:宽带载波,频率范围/中心频率:2～12MHz,调制方式:OFDM","只","92","2017-12-31","买方指定仓库地面交货"]
[null,"内蒙古东部电力有限公司","","1级三相表本地通信单元（窄带）","通信单元-通信单元类别:本地,适用终端/表类型:1级三相表,通信方式:窄带载波,频率范围/中心频率:其他,调制方式:其他","只","593","2017-12-31","买方指定仓库地面交货"]
[null,"内蒙古东部电力有限公司","","1级三相表本地通信单元（宽带）","通信单元-通信单元类别:本地,适用终端/表类型:1级三相表,通信方式:宽带载波,频率范围/中心频率:2～12MHz,调制方式:OFDM","只","69","2017-12-31","买方指定仓库地面交货"]
[null,"内蒙古东部电力有限公司","","1级三相表本地通信单元（宽带）","通信单元-通信单元类别:本地,适用终端/表类型:1级三相表,通信方式:宽带载波,频率范围/中心频率:2～12MHz,调制方式:OFDM","只","200","2017-12-31","买方指定仓库地面交货"]
[null,"内蒙古东部电力有限公司","","1级三相表本地通信单元（窄带）","通信单元-通信单元类别:本地,适用终端/表类型:1级三相表,通信方式:窄带载波,频率范围/中心频率:300kHz,调制方式:BPSK","只","12770","2017-12-31","买方指定仓库地面交货"]
["包16GW3","西藏电力有限公司","国网西藏电力有限公司各供电公司营销专项、电网基建/户表","1级三相费控智能电能表（模块-远程-开关外置）","三相智能电能表-准确度等级:1级,费控方式:远程,负荷开关:外置,通信模块接口:有,电压规格:3×220/380V,电流规格:1.5A","只","2800","2017-06-30","买方指定仓库地面交货"]
[null,"西藏电力有限公司","国网西藏电力有限公司各供电公司营销专项、电网基建/户表","1级三相表本地通信单元（窄带）","通信单元-通信单元类别:本地,适用终端/表类型:1级三相表,通信方式:窄带载波,频率范围/中心频率:421kHz,调制方式:BFSK","只","5408","2017-06-30","买方指定仓库地面交货"]
[null,"西藏电力有限公司","国网西藏电力有限公司各供电公司营销专项、电网基建/户表","1级三相表远程通信单元（CDMA）","通信单元-通信单元类别:远程,适用终端/表类型:1级三相表,通信方式:无线公网CDMA,频率范围/中心频率:无,调制方式:无","只","600","2017-06-30","买方指定仓库地面交货"]
[null,"西藏电力有限公司","国网西藏电力有限公司各供电公司营销专项、电网基建/户表","1级三相费控智能电能表（模块-远程-开关外置）","三相智能电能表-准确度等级:1级,费控方式:远程,负荷开关:外置,通信模块接口:有,电压规格:3×220/380V,电流规格:10A","只","206","2017-06-30","买方指定仓库地面交货"]
[null,"山东电力集团公司","","1级三相费控智能电能表（模块-远程-开关外置）","三相智能电能表-准确度等级:1级,费控方式:远程,负荷开关:外置,通信模块接口:有,电压规格:3×220/380V,电流规格:10A","只","150000","2018-06-30","买方指定仓库地面交货"]
[null,"山东电力集团公司","","1级三相表远程通信单元（4G）","通信单元-通信单元类别:远程,适用终端/表类型:1级三相表,通信方式:无线公网4G,频率范围/中心频率:无,调制方式:无","只","150000","2018-06-30","买方指定仓库地面交货"]
[null,"西藏电力有限公司","国网西藏电力有限公司各供电公司营销专项、电网基建/户表","1级三相费控智能电能表（模块-远程-开关外置）","三相智能电能表-准确度等级:1级,费控方式:远程,负荷开关:外置,通信模块接口:有,电压规格:3×100V,电流规格:1.5A","只","1450","2017-06-30","买方指定仓库地面交货"]
["包16GW4","山东电力集团公司","","1级三相表远程通信单元（4G）","通信单元-通信单元类别:远程,适用终端/表类型:1级三相表,通信方式:无线公网4G,频率范围/中心频率:无,调制方式:无","只","150000","2018-06-30","买方指定仓库地面交货"]
[null,"新疆电力公司","国家电网公司2017年第一次电能表（含用电信息采集）","1级三相表本地通信单元（窄带）","通信单元-通信单元类别:本地,适用终端/表类型:1级三相表,通信方式:窄带载波,频率范围/中心频率:270kHz,调制方式:BFSK","只","2095","2017-10-30","买方指定仓库车板交货"]
[null,"新疆电力公司","国家电网公司2017年第一次电能表（含用电信息采集）","1级三相表本地通信单元（窄带）","通信单元-通信单元类别:本地,适用终端/表类型:1级三相表,通信方式:窄带载波,频率范围/中心频率:421kHz,调制方式:BFSK","只","2645","2017-10-30","买方指定仓库车板交货"]
[null,"山东电力集团公司","","1级三相费控智能电能表（模块-远程-开关外置）","三相智能电能表-准确度等级:1级,费控方式:远程,负荷开关:外置,通信模块接口:有,电压规格:3×220/380V,电流规格:10A","只","150000","2018-06-30","买方指定仓库地面交货"]
[null,"新疆电力公司","国家电网公司2017年第一次电能表（含用电信息采集）","1级三相费控智能电能表（模块-远程-开关外置）","三相智能电能表-准确度等级:1级,费控方式:远程,负荷开关:外置,通信模块接口:有,电压规格:3×220/380V,电流规格:1.5A","只","4308","2017-10-30","买方指定仓库车板交货"]
["包16HA1","河南省电力公司","","1级三相表本地通信单元（窄带）","通信单元-通信单元类别:本地,适用终端/表类型:1级三相表,通信方式:窄带载波,频率范围/中心频率:421kHz,调制方式:BFSK","只","14652","2018-04-10","买方指定仓库地面交货"]
[null,"河南省电力公司","","1级三相费控智能电能表（模块-远程-开关外置）","三相智能电能表-准确度等级:1级,费控方式:远程,负荷开关:外置,通信模块接口:有,电压规格:3×220/380V,电流规格:5A","只","100000","2018-04-10","买方指定仓库地面交货"]
[null,"河南省电力公司","","1级三相表本地通信单元（窄带）","通信单元-通信单元类别:本地,适用终端/表类型:1级三相表,通信方式:窄带载波,频率范围/中心频率:其他,调制方式:其他","只","13464","2018-04-10","买方指定仓库地面交货"]
[null,"河南省电力公司","","1级三相表本地通信单元（窄带）","通信单元-通信单元类别:本地,适用终端/表类型:1级三相表,通信方式:窄带载波,频率范围/中心频率:270kHz,调制方式:BFSK","只","1980","2018-04-10","买方指定仓库地面交货"]
[null,"河南省电力公司","","1级三相表本地通信单元（宽带）","通信单元-通信单元类别:本地,适用终端/表类型:1级三相表,通信方式:宽带载波,频率范围/中心频率:2～12MHz,调制方式:OFDM","只","30800","2018-04-10","买方指定仓库地面交货"]
[null,"河南省电力公司","","1级三相表本地通信单元（窄带）","通信单元-通信单元类别:本地,适用终端/表类型:1级三相表,通信方式:窄带载波,频率范围/中心频率:132kHz,调制方式:BPSK","只","9504","2018-04-10","买方指定仓库地面交货"]
["包16HA2","河南省电力公司","","1级三相表本地通信单元（宽带）","通信单元-通信单元类别:本地,适用终端/表类型:1级三相表,通信方式:宽带载波,频率范围/中心频率:2～12MHz,调制方式:OFDM","只","22000","2018-04-10","买方指定仓库地面交货"]
[null,"河南省电力公司","","1级三相费控智能电能表（模块-远程-开关外置）","三相智能电能表-准确度等级:1级,费控方式:远程,负荷开关:外置,通信模块接口:有,电压规格:3×220/380V,电流规格:5A","只","100000","2018-04-10","买方指定仓库地面交货"]
[null,"河南省电力公司","","1级三相表本地通信单元（微功率）","通信单元-通信单元类别:本地,适用终端/表类型:1级三相表,通信方式:微功率,频率范围/中心频率:470～510MHz,调制方式:GFSK","只","39600","2018-04-10","买方指定仓库地面交货"]
["包16JX1","江西省电力公司","","1级三相表本地通信单元（微功率）","通信单元-通信单元类别:本地,适用终端/表类型:1级三相表,通信方式:微功率,频率范围/中心频率:470～510MHz,调制方式:GFSK","只","100","2017-09-15","买方指定仓库地面交货"]
[null,"江西省电力公司","","1级三相费控智能电能表（模块-远程-开关外置）","三相智能电能表-准确度等级:1级,费控方式:远程,负荷开关:外置,通信模块接口:有,电压规格:3×220/380V,电流规格:1.5A","只","44680","2017-09-15","买方指定仓库地面交货"]
[null,"江西省电力公司","","1级三相表本地通信单元（窄带）","通信单元-通信单元类别:本地,适用终端/表类型:1级三相表,通信方式:窄带载波,频率范围/中心频率:421kHz,调制方式:BFSK","只","1700","2017-09-15","买方指定仓库地面交货"]
[null,"江西省电力公司","","1级三相表本地通信单元（窄带）","通信单元-通信单元类别:本地,适用终端/表类型:1级三相表,通信方式:窄带载波,频率范围/中心频率:其他,调制方式:其他","只","9500","2017-09-15","买方指定仓库地面交货"]
[null,"江西省电力公司","","1级三相表本地通信单元（窄带）","通信单元-通信单元类别:本地,适用终端/表类型:1级三相表,通信方式:窄带载波,频率范围/中心频率:270kHz,调制方式:BFSK","只","28800","2017-09-15","买方指定仓库地面交货"]
[null,"江西省电力公司","","1级三相表本地通信单元（宽带）","通信单元-通信单元类别:本地,适用终端/表类型:1级三相表,通信方式:宽带载波,频率范围/中心频率:2～12MHz,调制方式:OFDM","只","4580","2017-09-15","买方指定仓库地面交货"]
["包16SD1","山东电力集团公司","","1级三相费控智能电能表（模块-远程-开关外置）","三相智能电能表-准确度等级:1级,费控方式:远程,负荷开关:外置,通信模块接口:有,电压规格:3×220/380V,电流规格:10A","只","57910","2018-06-30","买方指定仓库地面交货"]
[null,"山东电力集团公司","","1级三相表远程通信单元（4G）","通信单元-通信单元类别:远程,适用终端/表类型:1级三相表,通信方式:无线公网4G,频率范围/中心频率:无,调制方式:无","只","100000","2018-06-30","买方指定仓库地面交货"]
[null,"山东电力集团公司","","1级三相费控智能电能表（模块-远程-开关外置）","三相智能电能表-准确度等级:1级,费控方式:远程,负荷开关:外置,通信模块接口:有,电压规格:3×220/380V,电流规格:1.5A","只","42090","2018-06-30","买方指定仓库地面交货"]
["包16SD2","山东电力集团公司","","1级三相费控智能电能表（模块-远程-开关外置）","三相智能电能表-准确度等级:1级,费控方式:远程,负荷开关:外置,通信模块接口:有,电压规格:3×220/380V,电流规格:10A","只","42770","2018-06-30","买方指定仓库地面交货"]
[null,"山东电力集团公司","","1级三相表本地通信单元（窄带）","通信单元-通信单元类别:本地,适用终端/表类型:1级三相表,通信方式:窄带载波,频率范围/中心频率:421kHz,调制方式:BFSK","只","33693","2018-06-30","买方指定仓库地面交货"]
[null,"山东电力集团公司","","1级三相表本地通信单元（窄带）","通信单元-通信单元类别:本地,适用终端/表类型:1级三相表,通信方式:窄带载波,频率范围/中心频率:其他,调制方式:其他","只","7018","2018-06-30","买方指定仓库地面交货"]
[null,"山东电力集团公司","","1级三相表远程通信单元（4G）","通信单元-通信单元类别:远程,适用终端/表类型:1级三相表,通信方式:无线公网4G,频率范围/中心频率:无,调制方式:无","只","5760","2018-06-30","买方指定仓库地面交货"]
["包17GW1","辽宁省电力有限公司","","1级三相费控智能电能表（模块-CPU卡-开关外置）","三相智能电能表-准确度等级:1级,费控方式:本地,负荷开关:外置,通信模块接口:有,电压规格:3×220/380V,电流规格:5A","只","4000","2017-09-15","买方指定仓库地面交货"]
[null,"辽宁省电力有限公司","","1级三相费控智能电能表（模块-CPU卡-开关外置）","三相智能电能表-准确度等级:1级,费控方式:本地,负荷开关:外置,通信模块接口:有,电压规格:3×220/380V,电流规格:5A","只","100","2017-07-20","买方指定仓库地面交货"]
[null,"辽宁省电力有限公司","","1级三相费控智能电能表（模块-CPU卡-开关外置）","三相智能电能表-准确度等级:1级,费控方式:本地,负荷开关:外置,通信模块接口:有,电压规格:3×220/380V,电流规格:10A","只","500","2017-08-23","买方指定仓库地面交货"]
[null,"辽宁省电力有限公司","","1级三相表本地通信单元（窄带）","通信单元-通信单元类别:本地,适用终端/表类型:1级三相表,通信方式:窄带载波,频率范围/中心频率:270kHz,调制方式:BFSK","只","1000","2017-08-25","买方指定仓库地面交货"]
[null,"吉林省电力有限公司","","1级三相表本地通信单元（窄带）","通信单元-通信单元类别:本地,适用终端/表类型:1级三相表,通信方式:窄带载波,频率范围/中心频率:421kHz,调制方式:BFSK","只","30000","2017-12-30","买方指定仓库地面交货"]
[null,"吉林省电力有限公司","","1级三相费控智能电能表（模块-CPU卡-开关外置）","三相智能电能表-准确度等级:1级,费控方式:本地,负荷开关:外置,通信模块接口:有,电压规格:3×220/380V,电流规格:5A","只","30000","2017-12-30","买方指定仓库地面交货"]
[null,"辽宁省电力有限公司","","1级三相费控智能电能表（模块-CPU卡-开关外置）","三相智能电能表-准确度等级:1级,费控方式:本地,负荷开关:外置,通信模块接口:有,电压规格:3×220/380V,电流规格:10A","只","2000","2017-09-18","买方指定仓库地面交货"]
[null,"辽宁省电力有限公司","","1级三相费控智能电能表（模块-CPU卡-开关外置）","三相智能电能表-准确度等级:1级,费控方式:本地,负荷开关:外置,通信模块接口:有,电压规格:3×220/380V,电流规格:10A","只","2000","2017-08-22","买方指定仓库地面交货"]
[null,"辽宁省电力有限公司","","1级三相费控智能电能表（模块-CPU卡-开关外置）","三相智能电能表-准确度等级:1级,费控方式:本地,负荷开关:外置,通信模块接口:有,电压规格:3×220/380V,电流规格:5A","只","9300","2017-07-25","买方指定仓库地面交货"]
[null,"辽宁省电力有限公司","","1级三相费控智能电能表（模块-CPU卡-开关外置）","三相智能电能表-准确度等级:1级,费控方式:本地,负荷开关:外置,通信模块接口:有,电压规格:3×220/380V,电流规格:5A","只","500","2017-08-20","买方指定仓库地面交货"]
[null,"辽宁省电力有限公司","","1级三相费控智能电能表（模块-CPU卡-开关外置）","三相智能电能表-准确度等级:1级,费控方式:本地,负荷开关:外置,通信模块接口:有,电压规格:3×220/380V,电流规格:10A","只","4000","2017-09-18","买方指定仓库地面交货"]
[null,"辽宁省电力有限公司","","1级三相费控智能电能表（模块-CPU卡-开关外置）","三相智能电能表-准确度等级:1级,费控方式:本地,负荷开关:外置,通信模块接口:有,电压规格:3×220/380V,电流规格:10A","只","500","2017-08-23","买方指定仓库地面交货"]
[null,"辽宁省电力有限公司","","1级三相表本地通信单元（窄带）","通信单元-通信单元类别:本地,适用终端/表类型:1级三相表,通信方式:窄带载波,频率范围/中心频率:270kHz,调制方式:BFSK","只","2000","2017-08-25","买方指定仓库地面交货"]
[null,"辽宁省电力有限公司","","1级三相表本地通信单元（窄带）","通信单元-通信单元类别:本地,适用终端/表类型:1级三相表,通信方式:窄带载波,频率范围/中心频率:421kHz,调制方式:BFSK","只","2000","2017-08-25","买方指定仓库地面交货"]
[null,"吉林省电力有限公司","","计量现场作业终端与外设收纳箱","现场作业终端与外设收纳箱-存放外设个数:4","个","30","2017-12-30","买方指定仓库地面交货"]
[null,"吉林省电力有限公司","","超高频RFID模块","现场作业终端外设-采集故障识别模块:无,计量故障识别模块:无,超高频RFID模块:有,蓝牙打印模块:无","个","30","2017-12-30","买方指定仓库地面交货"]
[null,"吉林省电力有限公司","","三相计量故障识别模块","现场作业终端外设-采集故障识别模块:无,计量故障识别模块:三相,超高频RFID模块:无,蓝牙打印模块:无","个","30","2017-12-30","买方指定仓库地面交货"]
[null,"吉林省电力有限公司","","采集故障识别模块","现场作业终端外设-采集故障识别模块:有,计量故障识别模块:无,超高频RFID模块:无,蓝牙打印模块:无","个","30","2017-12-30","买方指定仓库地面交货"]
[null,"吉林省电力有限公司","","现场打印模块","现场作业终端外设-采集故障识别模块:无,计量故障识别模块:无,超高频RFID模块:无,蓝牙打印模块:有","个","30","2017-12-30","买方指定仓库地面交货"]
[null,"吉林省电力有限公司","","单相计量故障识别模块","现场作业终端外设-采集故障识别模块:无,计量故障识别模块:单相,超高频RFID模块:无,蓝牙打印模块:无","个","30","2017-12-30","买方指定仓库地面交货"]
[null,"吉林省电力有限公司","","计量现场作业终端","现场作业终端-屏幕尺寸范围:(4.0～7.0)英寸,购电卡接口:有","台","2","2017-12-30","买方指定仓库地面交货"]
[null,"辽宁省电力有限公司","","1级三相表本地通信单元（窄带）","通信单元-通信单元类别:本地,适用终端/表类型:1级三相表,通信方式:窄带载波,频率范围/中心频率:270kHz,调制方式:BFSK","只","3900","2017-08-31","买方指定仓库地面交货"]
[null,"辽宁省电力有限公司","","1级三相表本地通信单元（窄带）","通信单元-通信单元类别:本地,适用终端/表类型:1级三相表,通信方式:窄带载波,频率范围/中心频率:421kHz,调制方式:BFSK","只","5540","2017-08-31","买方指定仓库地面交货"]
[null,"辽宁省电力有限公司","","1级三相表远程通信单元（4G）","通信单元-通信单元类别:远程,适用终端/表类型:1级三相表,通信方式:无线公网4G,频率范围/中心频率:无,调制方式:无","只","200","2017-08-31","买方指定仓库地面交货"]
[null,"辽宁省电力有限公司","","1级三相表本地通信单元（宽带）","通信单元-通信单元类别:本地,适用终端/表类型:1级三相表,通信方式:宽带载波,频率范围/中心频率:2～12MHz,调制方式:OFDM","只","1710","2017-08-31","买方指定仓库地面交货"]
[null,"辽宁省电力有限公司","","1级三相表本地通信单元（窄带）","通信单元-通信单元类别:本地,适用终端/表类型:1级三相表,通信方式:窄带载波,频率范围/中心频率:270kHz,调制方式:BFSK","只","2605","2017-07-24","买方指定仓库地面交货"]
[null,"辽宁省电力有限公司","","1级三相表远程通信单元（4G）","通信单元-通信单元类别:远程,适用终端/表类型:1级三相表,通信方式:无线公网4G,频率范围/中心频率:无,调制方式:无","只","2000","2017-09-18","买方指定仓库地面交货"]
[null,"辽宁省电力有限公司","","1级三相表本地通信单元（窄带）","通信单元-通信单元类别:本地,适用终端/表类型:1级三相表,通信方式:窄带载波,频率范围/中心频率:270kHz,调制方式:BFSK","只","4000","2017-09-18","买方指定仓库地面交货"]
[null,"辽宁省电力有限公司","","1级三相表本地通信单元（窄带）","通信单元-通信单元类别:本地,适用终端/表类型:1级三相表,通信方式:窄带载波,频率范围/中心频率:270kHz,调制方式:BFSK","只","500","2017-08-20","买方指定仓库地面交货"]
[null,"辽宁省电力有限公司","","1级三相表远程通信单元（4G）","通信单元-通信单元类别:远程,适用终端/表类型:1级三相表,通信方式:无线公网4G,频率范围/中心频率:无,调制方式:无","只","500","2017-08-23","买方指定仓库地面交货"]
[null,"辽宁省电力有限公司","","1级三相表本地通信单元（窄带）","通信单元-通信单元类别:本地,适用终端/表类型:1级三相表,通信方式:窄带载波,频率范围/中心频率:270kHz,调制方式:BFSK","只","500","2017-08-23","买方指定仓库地面交货"]
[null,"辽宁省电力有限公司","","1级三相表本地通信单元（窄带）","通信单元-通信单元类别:本地,适用终端/表类型:1级三相表,通信方式:窄带载波,频率范围/中心频率:421kHz,调制方式:BFSK","只","2000","2017-08-22","买方指定仓库地面交货"]
[null,"辽宁省电力有限公司","","1级三相表本地通信单元（窄带）","通信单元-通信单元类别:本地,适用终端/表类型:1级三相表,通信方式:窄带载波,频率范围/中心频率:270kHz,调制方式:BFSK","只","7300","2017-07-25","买方指定仓库地面交货"]
[null,"辽宁省电力有限公司","","1级三相表本地通信单元（窄带）","通信单元-通信单元类别:本地,适用终端/表类型:1级三相表,通信方式:窄带载波,频率范围/中心频率:421kHz,调制方式:BFSK","只","2000","2017-07-25","买方指定仓库地面交货"]
[null,"辽宁省电力有限公司","","1级三相表本地通信单元（窄带）","通信单元-通信单元类别:本地,适用终端/表类型:1级三相表,通信方式:窄带载波,频率范围/中心频率:270kHz,调制方式:BFSK","只","4000","2017-09-15","买方指定仓库地面交货"]
[null,"辽宁省电力有限公司","","1级三相表本地通信单元（窄带）","通信单元-通信单元类别:本地,适用终端/表类型:1级三相表,通信方式:窄带载波,频率范围/中心频率:421kHz,调制方式:BFSK","只","150","2017-07-20","买方指定仓库地面交货"]
[null,"辽宁省电力有限公司","","1级三相费控智能电能表（模块-CPU卡-开关外置）","三相智能电能表-准确度等级:1级,费控方式:本地,负荷开关:外置,通信模块接口:有,电压规格:3×220/380V,电流规格:5A","只","8000","2017-08-31","买方指定仓库地面交货"]
[null,"辽宁省电力有限公司","","1级三相费控智能电能表（模块-CPU卡-开关外置）","三相智能电能表-准确度等级:1级,费控方式:本地,负荷开关:外置,通信模块接口:有,电压规格:3×220/380V,电流规格:5A","只","2000","2017-08-25","买方指定仓库地面交货"]
[null,"辽宁省电力有限公司","","1级三相费控智能电能表（模块-CPU卡-开关外置）","三相智能电能表-准确度等级:1级,费控方式:本地,负荷开关:外置,通信模块接口:有,电压规格:3×220/380V,电流规格:5A","只","1000","2017-08-25","买方指定仓库地面交货"]
[null,"辽宁省电力有限公司","","1级三相费控智能电能表（模块-CPU卡-开关外置）","三相智能电能表-准确度等级:1级,费控方式:本地,负荷开关:外置,通信模块接口:有,电压规格:3×220/380V,电流规格:5A","只","2000","2017-08-25","买方指定仓库地面交货"]
[null,"辽宁省电力有限公司","","1级三相费控智能电能表（模块-CPU卡-开关外置）","三相智能电能表-准确度等级:1级,费控方式:本地,负荷开关:外置,通信模块接口:有,电压规格:3×220/380V,电流规格:10A","只","1000","2017-07-24","买方指定仓库地面交货"]
["包25GW1","安徽省电力公司","","1级三相费控智能电能表（远程-开关内置）","三相智能电能表-准确度等级:1级,费控方式:远程,负荷开关:内置,通信模块接口:无,电压规格:3×220/380V,电流规格:5A","只","11200","2017-07-10","买方指定仓库地面交货"]
[null,"江苏省电力公司","","1级三相费控智能电能表（远程-开关内置）","三相智能电能表-准确度等级:1级,费控方式:远程,负荷开关:内置,通信模块接口:无,电压规格:3×220/380V,电流规格:5A","只","28000","2018-04-15","买方指定仓库地面交货"]
[null,"江苏省电力公司","","1级三相费控智能电能表（远程-开关内置）","三相智能电能表-准确度等级:1级,费控方式:远程,负荷开关:内置,通信模块接口:无,电压规格:3×220/380V,电流规格:5A","只","25000","2018-04-15","买方指定仓库地面交货"]
[null,"江苏省电力公司","","1级三相费控智能电能表（远程-开关内置）","三相智能电能表-准确度等级:1级,费控方式:远程,负荷开关:内置,通信模块接口:无,电压规格:3×220/380V,电流规格:5A","只","12000","2018-04-15","买方指定仓库地面交货"]
[null,"江苏省电力公司","","1级三相费控智能电能表（远程-开关内置）","三相智能电能表-准确度等级:1级,费控方式:远程,负荷开关:内置,通信模块接口:无,电压规格:3×220/380V,电流规格:5A","只","10000","2018-04-15","买方指定仓库地面交货"]
["包25JS1","江苏省电力公司","","1级三相费控智能电能表（远程-开关内置）","三相智能电能表-准确度等级:1级,费控方式:远程,负荷开关:内置,通信模块接口:无,电压规格:3×220/380V,电流规格:5A","只","40000","2018-04-15","买方指定仓库地面交货"]
[null,"江苏省电力公司","","1级三相费控智能电能表（远程-开关内置）","三相智能电能表-准确度等级:1级,费控方式:远程,负荷开关:内置,通信模块接口:无,电压规格:3×220/380V,电流规格:5A","只","35000","2018-04-15","买方指定仓库地面交货"]
[null,"江苏省电力公司","","1级三相费控智能电能表（远程-开关内置）","三相智能电能表-准确度等级:1级,费控方式:远程,负荷开关:内置,通信模块接口:无,电压规格:3×220/380V,电流规格:5A","只","20000","2018-04-15","买方指定仓库地面交货"]
["包25ZJ1","浙江省电力公司","","1级三相费控智能电能表（远程-开关内置）","三相智能电能表-准确度等级:1级,费控方式:远程,负荷开关:内置,通信模块接口:无,电压规格:3×220/380V,电流规格:5A","只","155000","2019-03-31","买方指定仓库地面交货"]
["包25ZJ2","浙江省电力公司","","1级三相费控智能电能表（远程-开关内置）","三相智能电能表-准确度等级:1级,费控方式:远程,负荷开关:内置,通信模块接口:无,电压规格:3×220/380V,电流规格:5A","只","150000","2019-03-31","买方指定仓库地面交货"]
["包25ZJ3","浙江省电力公司","","1级三相费控智能电能表（远程-开关内置）","三相智能电能表-准确度等级:1级,费控方式:远程,负荷开关:内置,通信模块接口:无,电压规格:3×220/380V,电流规格:5A","只","100000","2019-03-31","买方指定仓库地面交货"]
["包25ZJ4","浙江省电力公司","","1级三相费控智能电能表（远程-开关内置）","三相智能电能表-准确度等级:1级,费控方式:远程,负荷开关:内置,通信模块接口:无,电压规格:3×220/380V,电流规格:5A","只","50000","2019-03-31","买方指定仓库地面交货"]
["包28GW1","内蒙古东部电力有限公司","","1级三相智能电能表","三相智能电能表-准确度等级:1级,费控方式:无,负荷开关:无控,通信模块接口:无,电压规格:3×220/380V,电流规格:1.5A","只","208","2017-12-31","买方指定仓库地面交货"]
[null,"内蒙古东部电力有限公司","","1级三相智能电能表","三相智能电能表-准确度等级:1级,费控方式:无,负荷开关:无控,通信模块接口:无,电压规格:3×220/380V,电流规格:1.5A","只","32","2017-12-31","买方指定仓库地面交货"]
[null,"内蒙古东部电力有限公司","","1级三相智能电能表","三相智能电能表-准确度等级:1级,费控方式:无,负荷开关:无控,通信模块接口:无,电压规格:3×220/380V,电流规格:1.5A","只","16","2017-12-29","买方指定仓库地面交货"]
[null,"内蒙古东部电力有限公司","","1级三相智能电能表","三相智能电能表-准确度等级:1级,费控方式:无,负荷开关:无控,通信模块接口:无,电压规格:3×220/380V,电流规格:1.5A","只","246","2017-12-31","买方指定仓库地面交货"]
[null,"内蒙古东部电力有限公司","","1级三相智能电能表","三相智能电能表-准确度等级:1级,费控方式:无,负荷开关:无控,通信模块接口:无,电压规格:3×220/380V,电流规格:1.5A","只","192","2017-12-31","买方指定仓库地面交货"]
[null,"安徽省电力公司","","1级三相智能电能表","三相智能电能表-准确度等级:1级,费控方式:无,负荷开关:无控,通信模块接口:无,电压规格:3×220/380V,电流规格:1.5A","只","9700","2017-07-10","买方指定仓库地面交货"]
[null,"西藏电力有限公司","国网西藏电力有限公司各供电公司营销专项、电网基建/户表","1级三相费控智能电能表（远程-开关外置）","三相智能电能表-准确度等级:1级,费控方式:远程,负荷开关:外置,通信模块接口:无,电压规格:3×57.7/100V,电流规格:1.5A","只","170","2017-06-30","买方指定仓库地面交货"]
[null,"陕西省电力公司","","超高频RFID模块","现场作业终端外设-采集故障识别模块:无,计量故障识别模块:无,超高频RFID模块:有,蓝牙打印模块:无","个","145","2018-06-30","买方指定仓库地面交货"]
[null,"陕西省电力公司","","单相计量故障识别模块","现场作业终端外设-采集故障识别模块:无,计量故障识别模块:单相,超高频RFID模块:无,蓝牙打印模块:无","个","145","2018-06-30","买方指定仓库地面交货"]
[null,"陕西省电力公司","","1级三相智能电能表","三相智能电能表-准确度等级:1级,费控方式:无,负荷开关:无控,通信模块接口:无,电压规格:3×220/380V,电流规格:1.5A","只","3943","2018-06-30","买方指定仓库地面交货"]
[null,"内蒙古东部电力有限公司","","1级三相智能电能表","三相智能电能表-准确度等级:1级,费控方式:无,负荷开关:无控,通信模块接口:无,电压规格:3×220/380V,电流规格:1.5A","只","45","2017-12-31","买方指定仓库地面交货"]
[null,"内蒙古东部电力有限公司","","1级三相智能电能表","三相智能电能表-准确度等级:1级,费控方式:无,负荷开关:无控,通信模块接口:无,电压规格:3×220/380V,电流规格:1.5A","只","308","2017-12-31","买方指定仓库地面交货"]
[null,"陕西省电力公司","","采集故障识别模块","现场作业终端外设-采集故障识别模块:有,计量故障识别模块:无,超高频RFID模块:无,蓝牙打印模块:无","个","145","2018-06-30","买方指定仓库地面交货"]
[null,"陕西省电力公司","","计量现场作业终端与外设收纳箱","现场作业终端与外设收纳箱-存放外设个数:3","个","145","2018-06-30","买方指定仓库地面交货"]
[null,"陕西省电力公司","","计量现场作业终端","现场作业终端-屏幕尺寸范围:≤4.0英寸,购电卡接口:有","台","26","2018-06-30","买方指定仓库地面交货"]
[null,"陕西省电力公司","","计量现场作业终端","现场作业终端-屏幕尺寸范围:≤4.0英寸,购电卡接口:无","台","119","2018-06-30","买方指定仓库地面交货"]
[null,"浙江省电力公司","","1级三相费控智能电能表（远程-开关外置）","三相智能电能表-准确度等级:1级,费控方式:远程,负荷开关:外置,通信模块接口:无,电压规格:3×220/380V,电流规格:1.5A","只","124000","2019-03-31","买方指定仓库地面交货"]
[null,"内蒙古东部电力有限公司","","1级三相表本地通信单元（宽带）","通信单元-通信单元类别:本地,适用终端/表类型:1级三相表,通信方式:宽带载波,频率范围/中心频率:2～12MHz,调制方式:OFDM","只","500","2017-12-31","买方指定仓库地面交货"]
[null,"内蒙古东部电力有限公司","","1级三相表本地通信单元（窄带）","通信单元-通信单元类别:本地,适用终端/表类型:1级三相表,通信方式:窄带载波,频率范围/中心频率:270kHz,调制方式:BFSK","只","294","2017-12-31","买方指定仓库地面交货"]
[null,"内蒙古东部电力有限公司","","1级三相智能电能表","三相智能电能表-准确度等级:1级,费控方式:无,负荷开关:无控,通信模块接口:无,电压规格:3×220/380V,电流规格:1.5A","只","153","2017-12-31","买方指定仓库地面交货"]
[null,"陕西省电力公司","","三相计量故障识别模块","现场作业终端外设-采集故障识别模块:无,计量故障识别模块:三相,超高频RFID模块:无,蓝牙打印模块:无","个","145","2018-06-30","买方指定仓库地面交货"]
[null,"内蒙古东部电力有限公司","","1级三相表本地通信单元（窄带）","通信单元-通信单元类别:本地,适用终端/表类型:1级三相表,通信方式:窄带载波,频率范围/中心频率:421kHz,调制方式:BFSK","只","1178","2017-12-31","买方指定仓库地面交货"]
["包28JS1","江苏省电力公司","","1级三相费控智能电能表（远程-开关外置）","三相智能电能表-准确度等级:1级,费控方式:远程,负荷开关:外置,通信模块接口:无,电压规格:3×220/380V,电流规格:10A","只","23000","2018-04-15","买方指定仓库地面交货"]
[null,"江苏省电力公司","","1级三相费控智能电能表（远程-开关外置）","三相智能电能表-准确度等级:1级,费控方式:远程,负荷开关:外置,通信模块接口:无,电压规格:3×220/380V,电流规格:10A","只","17000","2018-04-15","买方指定仓库地面交货"]
["包28SD1","山东电力集团公司","","1级三相费控智能电能表（远程-开关外置）","三相智能电能表-准确度等级:1级,费控方式:远程,负荷开关:外置,通信模块接口:无,电压规格:3×220/380V,电流规格:10A","只","24240","2018-06-30","买方指定仓库地面交货"]
[null,"山东电力集团公司","","1级三相费控智能电能表（远程-开关外置）","三相智能电能表-准确度等级:1级,费控方式:远程,负荷开关:外置,通信模块接口:无,电压规格:3×220/380V,电流规格:1.5A","只","125760","2018-06-30","买方指定仓库地面交货"]
["包28SD2","山东电力集团公司","","1级三相费控智能电能表（远程-开关外置）","三相智能电能表-准确度等级:1级,费控方式:远程,负荷开关:外置,通信模块接口:无,电压规格:3×220/380V,电流规格:10A","只","150000","2018-06-30","买方指定仓库地面交货"]
["包28SD3","山东电力集团公司","","1级三相费控智能电能表（远程-开关外置）","三相智能电能表-准确度等级:1级,费控方式:远程,负荷开关:外置,通信模块接口:无,电压规格:3×220/380V,电流规格:10A","只","79230","2018-06-30","买方指定仓库地面交货"]

{"sheet":"0.5S级三相智能电能表","index":2,"n_rows":122,"n_cols":9,"rows_kept":122,"merged":[[0,0,0,8],[1,0,1,8],[3,0,26,0],[27,0,40,0],[41,0,47,0],[48,0,54,0],[55,0,110,0],[111,0,114,0],[115,0,116,0],[117,0,119,0]],"flags":["formulas_cached_only"]}
["国家电网公司2017年第一次电能表及用电信息采集设备招标活动\n货物需求一览表\n(0.5S级三相智能电能表)"]
["分标编号:0711-17OTL03922000-3"]
["包号","项目单位","项目名称","招标货物","物资描述","单位","行数量","交货日期","交货地点"]
["包32GW1","上海市电力公司","国网上海公司2017年第一次电能表（含用电信息采集）项目","0.5S级三相费控智能电能表（模块-远程-开关外置）","三相智能电能表-准确度等级:0.5S级,费控方式:远程,负荷开关:外置,通信模块接口:有,电压规格:3×220/380V,电流规格:1.5A","只","5000","2018-04-30","买方指定仓库车板交货"]
[null,"西藏电力有限公司","国网西藏电力有限公司各供电公司营销专项、电网基建/户表","0.5S级三相费控智能电能表（模块-远程-开关外置）","三相智能电能表-准确度等级:0.5S级,费控方式:远程,负荷开关:外置,通信模块接口:有,电压规格:3×220/380V,电流规格:1.5A","只","75","2017-06-30","买方指定仓库地面交货"]
[null,"辽宁省电力有限公司","","0.5S级三相费控智能电能表（模块-远程-开关外置）","三相智能电能表-准确度等级:0.5S级,费控方式:远程,负荷开关:外置,通信模块接口:有,电压规格:3×220/380V,电流规格:1.5A","只","800","2017-09-21","买方指定仓库地面交货"]
[null,"辽宁省电力有限公司","","0.5S级三相表远程通信单元（4G）","通信单元-通信单元类别:远程,适用终端/表类型:0.5S级三相表,通信方式:无线公网4G,频率范围/中心频率:无,调制方式:无","只","800","2017-09-21","买方指定仓库地面交货"]
[null,"辽宁省电力有限公司","","0.5S级三相费控智能电能表（模块-远程-开关外置）","三相智能电能表-准确度等级:0.5S级,费控方式:远程,负荷开关:外置,通信模块接口:有,电压规格:3×100V,电流规格:1.5A","只","300","2017-09-21","买方指定仓库地面交货"]
[null,"上海市电力公司","国网上海公司2017年第一次电能表（含用电信息采集）项目","0.5S级三相表远程通信单元（4G）","通信单元-通信单元类别:远程,适用终端/表类型:0.5S级三相表,通信方式:无线公网4G,频率范围/中心频率:无,调制方式:无","只","5000","2018-04-30","买方指定仓库车板交货"]
[null,"辽宁省电力有限公司","","0.5S级三相费控智能电能表（模块-远程-开关外置）","三相智能电能表-准确度等级:0.5S级,费控方式:远程,负荷开关:外置,通信模块接口:有,电压规格:3×220/380V,电流规格:1.5A","只","3550","2017-08-31","买方指定仓库地面交货"]
[null,"辽宁省电力有限公司","","0.5S级三相表远程通信单元（4G）","通信单元-通信单元类别:远程,适用终端/表类型:0.5S级三相表,通信方式:无线公网4G,频率范围/中心频率:无,调制方式:无","只","4800","2017-08-31","买方指定仓库地面交货"]
[null,"辽宁省电力有限公司","","0.5S级三相费控智能电能表（模块-远程-开关外置）","三相智能电能表-准确度等级:0.5S级,费控方式:远程,负荷开关:外置,通信模块接口:有,电压规格:3×100V,电流规格:1.5A","只","2700","2017-08-31","买方指定仓库地面交货"]
[null,"辽宁省电力有限公司","","0.5S级三相费控智能电能表（模块-远程-开关外置）","三相智能电能表-准确度等级:0.5S级,费控方式:远程,负荷开关:外置,通信模块接口:有,电压规格:3×220/380V,电流规格:1.5A","只","3000","2017-08-23","买方指定仓库地面交货"]
[null,"辽宁省电力有限公司","","0.5S级三相表远程通信单元（4G）","通信单元-通信单元类别:远程,适用终端/表类型:0.5S级三相表,通信方式:无线公网4G,频率范围/中心频率:无,调制方式:无","只","3000","2017-08-23","买方指定仓库地面交货"]
[null,"辽宁省电力有限公司","","0.5S级三相表远程通信单元（4G）","通信单元-通信单元类别:远程,适用终端/表类型:0.5S级三相表,通信方式:无线公网4G,频率范围/中心频率:无,调制方式:无","只","400","2017-08-20","买方指定仓库地面交货"]
[null,"辽宁省电力有限公司","","0.5S级三相表远程通信单元（4G）","通信单元-通信单元类别:远程,适用终端/表类型:0.5S级三相表,通信方式:无线公网4G,频率范围/中心频率:无,调制方式:无","只","300","2017-09-21","买方指定仓库地面交货"]
[null,"辽宁省电力有限公司","","0.5S级三相费控智能电能表（模块-远程-开关外置）","三相智能电能表-准确度等级:0.5S级,费控方式:远程,负荷开关:外置,通信模块接口:有,电压规格:3×220/380V,电流规格:1.5A","只","400","2017-08-20","买方指定仓库地面交货"]
[null,"辽宁省电力有限公司","","0.5S级三相费控智能电能表（模块-远程-开关外置）","三相智能电能表-准确度等级:0.5S级,费控方式:远程,负荷开关:外置,通信模块接口:有,电压规格:3×220/380V,电流规格:1.5A","只","100","2017-07-20","买方指定仓库地面交货"]
[null,"辽宁省电力有限公司","","0.5S级三相表远程通信单元（4G）","通信单元-通信单元类别:远程,适用终端/表类型:0.5S级三相表,通信方式:无线公网4G,频率范围/中心频率:无,调制方式:无","只","100","2017-07-20","买方指定仓库地面交货"]
[null,"辽宁省电力有限公司","","0.5S级三相表远程通信单元（4G）","通信单元-通信单元类别:远程,适用终端/表类型:0.5S级三相表,通信方式:无线公网4G,频率范围/中心频率:无,调制方式:无","只","2000","2017-09-15","买方指定仓库地面交货"]
[null,"辽宁省电力有限公司","","0.5S级三相费控智能电能表（模块-远程-开关外置）","三相智能电能表-准确度等级:0.5S级,费控方式:远程,负荷开关:外置,通信模块接口:有,电压规格:3×220/380V,电流规格:1.5A","只","2000","2017-09-15","买方指定仓库地面交货"]
[null,"辽宁省电力有限公司","","0.5S级三相费控智能电能表（模块-远程-开关外置）","三相智能电能表-准确度等级:0.5S级,费控方式:远程,负荷开关:外置,通信模块接口:有,电压规格:3×220/380V,电流规格:1.5A","只","500","2017-08-20","买方指定仓库地面交货"]
[null,"辽宁省电力有限公司","","0.5S级三相表远程通信单元（4G）","通信单元-通信单元类别:远程,适用终端/表类型:0.5S级三相表,通信方式:无线公网4G,频率范围/中心频率:无,调制方式:无","只","700","2017-08-20","买方指定仓库地面交货"]
[null,"辽宁省电力有限公司","","0.5S级三相费控智能电能表（模块-远程-开关外置）","三相智能电能表-准确度等级:0.5S级,费控方式:远程,负荷开关:外置,通信模块接口:有,电压规格:3×57.7/100V,电流规格:1.5A","只","500","2017-09-18","买方指定仓库地面交货"]
[null,"辽宁省电力有限公司","","0.5S级三相表远程通信单元（4G）","通信单元-通信单元类别:远程,适用终端/表类型:0.5S级三相表,通信方式:无线公网4G,频率范围/中心频率:无,调制方式:无","只","500","2017-09-18","买方指定仓库地面交货"]
[null,"西藏电力有限公司","国网西藏电力有限公司各供电公司营销专项、电网基建/户表","0.5S级三相费控智能电能表（模块-远程-开关外置）","三相智能电能表-准确度等级:0.5S级,费控方式:远程,负荷开关:外置,通信模块接口:有,电压规格:3×100V,电流规格:1.5A","只","20","2017-07-30","买方指定仓库地面交货"]
[null,"辽宁省电力有限公司","","0.5S级三相费控智能电能表（模块-远程-开关外置）","三相智能电能表-准确度等级:0.5S级,费控方式:远程,负荷开关:外置,通信模块接口:有,电压规格:3×100V,电流规格:1.5A","只","200","2017-08-20","买方指定仓库地面交货"]
["包33GW1","天津市电力公司","","0.5S级三相表本地通信单元（窄带）","通信单元-通信单元类别:本地,适用终端/表类型:0.5S级三相表,通信方式:窄带载波,频率范围/中心频率:270kHz,调制方式:BFSK","只","4000","2017-12-31","买方指定仓库地面交货"]
[null,"天津市电力公司","","0.5S级三相费控智能电能表（模块-CPU卡-开关外置）","三相智能电能表-准确度等级:0.5S级,费控方式:本地,负荷开关:外置,通信模块接口:有,电压规格:3×220/380V,电流规格:1.5A","只","10000","2017-12-31","买方指定仓库地面交货"]
[null,"天津市电力公司","","0.5S级三相表本地通信单元（宽带）","通信单元-通信单元类别:本地,适用终端/表类型:0.5S级三相表,通信方式:宽带载波,频率范围/中心频率:2～12MHz,调制方式:OFDM","只","1000","2017-12-31","买方指定仓库地面交货"]
[null,"辽宁省电力有限公司","","0.5S级三相费控智能电能表（模块-CPU卡-开关外置）","三相智能电能表-准确度等级:0.5S级,费控方式:本地,负荷开关:外置,通信模块接口:有,电压规格:3×220/380V,电流规格:1.5A","只","1900","2017-08-31","买方指定仓库地面交货"]
[null,"辽宁省电力有限公司","","0.5S级三相费控智能电能表（模块-CPU卡-开关外置）","三相智能电能表-准确度等级:0.5S级,费控方式:本地,负荷开关:外置,通信模块接口:有,电压规格:3×220/380V,电流规格:1.5A","只","1068","2017-07-24","买方指定仓库地面交货"]
[null,"辽宁省电力有限公司","","0.5S级三相费控智能电能表（模块-CPU卡-开关外置）","三相智能电能表-准确度等级:0.5S级,费控方式:本地,负荷开关:外置,通信模块接口:有,电压规格:3×220/380V,电流规格:1.5A","只","800","2017-09-15","买方指定仓库地面交货"]
[null,"辽宁省电力有限公司","","0.5S级三相表远程通信单元（4G）","通信单元-通信单元类别:远程,适用终端/表类型:0.5S级三相表,通信方式:无线公网4G,频率范围/中心频率:无,调制方式:无","只","800","2017-09-15","买方指定仓库地面交货"]
[null,"辽宁省电力有限公司","","0.5S级三相费控智能电能表（模块-CPU卡-开关外置）","三相智能电能表-准确度等级:0.5S级,费控方式:本地,负荷开关:外置,通信模块接口:有,电压规格:3×220/380V,电流规格:1.5A","只","50","2017-07-20","买方指定仓库地面交货"]
[null,"天津市电力公司","","0.5S级三相表本地通信单元（窄带）","通信单元-通信单元类别:本地,适用终端/表类型:0.5S级三相表,通信方式:窄带载波,频率范围/中心频率:其他,调制方式:其他","只","2000","2017-12-31","买方指定仓库地面交货"]
[null,"天津市电力公司","","0.5S级三相表本地通信单元（窄带）","通信单元-通信单元类别:本地,适用终端/表类型:0.5S级三相表,通信方式:窄带载波,频率范围/中心频率:421kHz,调制方式:BFSK","只","3000","2017-12-31","买方指定仓库地面交货"]
[null,"辽宁省电力有限公司","","0.5S级三相费控智能电能表（模块-CPU卡-开关外置）","三相智能电能表-准确度等级:0.5S级,费控方式:本地,负荷开关:外置,通信模块接口:有,电压规格:3×220/380V,电流规格:1.5A","只","300","2017-08-20","买方指定仓库地面交货"]
[null,"辽宁省电力有限公司","","0.5S级三相表远程通信单元（4G）","通信单元-通信单元类别:远程,适用终端/表类型:0.5S级三相表,通信方式:无线公网4G,频率范围/中心频率:无,调制方式:无","只","300","2017-08-20","买方指定仓库地面交货"]
[null,"辽宁省电力有限公司","","0.5S级三相表远程通信单元（4G）","通信单元-通信单元类别:远程,适用终端/表类型:0.5S级三相表,通信方式:无线公网4G,频率范围/中心频率:无,调制方式:无","只","1200","2017-07-20","买方指定仓库地面交货"]
[null,"辽宁省电力有限公司","","0.5S级三相费控智能电能表（模块-CPU卡-开关外置）","三相智能电能表-准确度等级:0.5S级,费控方式:本地,负荷开关:外置,通信模块接口:有,电压规格:3×220/380V,电流规格:1.5A","只","1200","2017-07-20","买方指定仓库地面交货"]
["包35GW1","福建省电力有限公司","国网福建省电力有限公司采购","0.5S级三相智能电能表","三相智能电能表-准确度等级:0.5S级,费控方式:无,负荷开关:无控,通信模块接口:无,电压规格:3×100V,电流规格:0.3A","只","210","2018-06-30","买方指定仓库地面交货"]
[null,"福建省电力有限公司","国网福建省电力有限公司采购","0.5S级三相智能电能表","三相智能电能表-准确度等级:0.5S级,费控方式:无,负荷开关:无控,通信模块接口:无,电压规格:3×100V,电流规格:1.5A","只","7740","2018-06-30","买方指定仓库地面交货"]
[null,"福建省电力有限公司","国网福建省电力有限公司采购","0.5S级三相智能电能表","三相智能电能表-准确度等级:0.5S级,费控方式:无,负荷开关:无控,通信模块接口:无,电压规格:3×57.7/100V,电流规格:1.5A","只","630","2018-06-30","买方指定仓库地面交货"]
[null,"福建省电力有限公司","国网福建省电力有限公司采购","0.5S级三相智能电能表","三相智能电能表-准确度等级:0.5S级,费控方式:无,负荷开关:无控,通信模块接口:无,电压规格:3×220/380V,电流规格:1.5A","只","1300","2018-06-30","买方指定仓库地面交货"]
[null,"安徽省电力公司","","0.5S级三相智能电能表","三相智能电能表-准确度等级:0.5S级,费控方式:无,负荷开关:无控,通信模块接口:无,电压规格:3×220/380V,电流规格:1.5A","只","10600","2017-07-10","买方指定仓库地面交货"]
[null,"山东电力集团公司","","0.5S级三相智能电能表","三相智能电能表-准确度等级:0.5S级,费控方式:无,负荷开关:无控,通信模块接口:无,电压规格:3×57.7/100V,电流规格:1.5A","只","4020","2018-06-30","买方指定仓库地面交货"]
[null,"山东电力集团公司","","0.5S级三相智能电能表","三相智能电能表-准确度等级:0.5S级,费控方式:无,负荷开关:无控,通信模块接口:无,电压规格:3×100V,电流规格:1.5A","只","13510","2018-06-30","买方指定仓库地面交货"]
["包35GW2","北京市电力公司","北京协议库存","0.5S级三相智能电能表","三相智能电能表-准确度等级:0.5S级,费控方式:无,负荷开关:无控,通信模块接口:无,电压规格:3×100V,电流规格:1.5A","只","2639","2018-04-14","买方指定仓库地面交货"]
[null,"天津市电力公司","","0.5S级三相智能电能表","三相智能电能表-准确度等级:0.5S级,费控方式:无,负荷开关:无控,通信模块接口:无,电压规格:3×220/380V,电流规格:1.5A","只","3000","2017-12-31","买方指定仓库地面交货"]
[null,"山西省电力公司","","0.5S级三相智能电能表","三相智能电能表-准确度等级:0.5S级,费控方式:无,负荷开关:无控,通信模块接口:无,电压规格:3×57.7/100V,电流规格:0.3A","只","350","2018-04-30","买方指定仓库地面交货"]
[null,"山西省电力公司","","0.5S级三相智能电能表","三相智能电能表-准确度等级:0.5S级,费控方式:无,负荷开关:无控,通信模块接口:无,电压规格:3×100V,电流规格:0.3A","只","350","2018-04-30","买方指定仓库地面交货"]
[null,"山西省电力公司","","0.5S级三相智能电能表","三相智能电能表-准确度等级:0.5S级,费控方式:无,负荷开关:无控,通信模块接口:无,电压规格:3×100V,电流规格:1.5A","只","3700","2018-04-30","买方指定仓库地面交货"]
[null,"山西省电力公司","","0.5S级三相智能电能表","三相智能电能表-准确度等级:0.5S级,费控方式:无,负荷开关:无控,通信模块接口:无,电压规格:3×57.7/100V,电流规格:1.5A","只","775","2018-04-30","买方指定仓库地面交货"]
[null,"山西省电力公司","","0.5S级三相智能电能表","三相智能电能表-准确度等级:0.5S级,费控方式:无,负荷开关:无控,通信模块接口:无,电压规格:3×220/380V,电流规格:1.5A","只","26617","2018-04-30","买方指定仓库地面交货"]
["包35GW3","内蒙古东部电力有限公司","","0.5S级三相智能电能表","三相智能电能表-准确度等级:0.5S级,费控方式:无,负荷开关:无控,通信模块接口:无,电压规格:3×100V,电流规格:1.5A","只","164","2017-12-31","买方指定仓库地面交货"]
[null,"辽宁省电力有限公司","","0.5S级三相智能电能表","三相智能电能表-准确度等级:0.5S级,费控方式:无,负荷开关:无控,通信模块接口:无,电压规格:3×100V,电流规格:1.5A","只","500","2017-08-23","买方指定仓库地面交货"]
[null,"辽宁省电力有限公司","","0.5S级三相智能电能表","三相智能电能表-准确度等级:0.5S级,费控方式:无,负荷开关:无控,通信模块接口:无,电压规格:3×220/380V,电流规格:1.5A","只","6100","2017-08-31","买方指定仓库地面交货"]
[null,"辽宁省电力有限公司","","0.5S级三相智能电能表","三相智能电能表-准确度等级:0.5S级,费控方式:无,负荷开关:无控,通信模块接口:无,电压规格:3×220/380V,电流规格:1.5A","只","2000","2017-08-25","买方指定仓库地面交货"]
[null,"辽宁省电力有限公司","","0.5S级三相智能电能表","三相智能电能表-准确度等级:0.5S级,费控方式:无,负荷开关:无控,通信模块接口:无,电压规格:3×100V,电流规格:1.5A","只","200","2017-09-15","买方指定仓库地面交货"]
[null,"辽宁省电力有限公司","","0.5S级三相智能电能表","三相智能电能表-准确度等级:0.5S级,费控方式:无,负荷开关:无控,通信模块接口:无,电压规格:3×220/380V,电流规格:1.5A","只","1000","2017-08-20","买方指定仓库地面交货"]
[null,"辽宁省电力有限公司","","0.5S级三相智能电能表","三相智能电能表-准确度等级:0.5S级,费控方式:无,负荷开关:无控,通信模块接口:无,电压规格:3×220/380V,电流规格:1.5A","只","96","2017-08-20","买方指定仓库地面交货"]
[null,"黑龙江省电力有限公司","","0.5S级三相智能电能表","三相智能电能表-准确度等级:0.5S级,费控方式:无,负荷开关:无控,通信模块接口:无,电压规格:3×100V,电流规格:1.5A","只","2155","2018-04-20","买方指定仓库地面交货"]
[null,"内蒙古东部电力有限公司","","0.5S级三相智能电能表","三相智能电能表-准确度等级:0.5S级,费控方式:无,负荷开关:无控,通信模块接口:无,电压规格:3×100V,电流规格:1.5A","只","30","2017-12-31","买方指定仓库地面交货"]
[null,"内蒙古东部电力有限公司","","0.5S级三相智能电能表","三相智能电能表-准确度等级:0.5S级,费控方式:无,负荷开关:无控,通信模块接口:无,电压规格:3×100V,电流规格:1.5A","只","12","2017-12-31","买方指定仓库地面交货"]
[null,"内蒙古东部电力有限公司","","0.5S级三相智能电能表","三相智能电能表-准确度等级:0.5S级,费控方式:无,负荷开关:无控,通信模块接口:无,电压规格:3×220/380V,电流规格:1.5A","只","230","2017-12-31","买方指定仓库地面交货"]
[null,"内蒙古东部电力有限公司","","0.5S级三相智能电能表","三相智能电能表-准确度等级:0.5S级,费控方式:无,负荷开关:无控,通信模块接口:无,电压规格:3×100V,电流规格:1.5A","只","6","2017-12-31","买方指定仓库地面交货"]
[null,"内蒙古东部电力有限公司","","0.5S级三相智能电能表","三相智能电能表-准确度等级:0.5S级,费控方式:无,负荷开关:无控,通信模块接口:无,电压规格:3×220/380V,电流规格:1.5A","只","199","2017-12-31","买方指定仓库地面交货"]
[null,"内蒙古东部电力有限公司","","0.5S级三相智能电能表","三相智能电能表-准确度等级:0.5S级,费控方式:无,负荷开关:无控,通信模块接口:无,电压规格:3×57.7/100V,电流规格:1.5A","只","19","2017-12-31","买方指定仓库地面交货"]
[null,"内蒙古东部电力有限公司","","0.5S级三相智能电能表","三相智能电能表-准确度等级:0.5S级,费控方式:无,负荷开关:无控,通信模块接口:无,电压规格:3×220/380V,电流规格:1.5A","只","47","2017-12-31","买方指定仓库地面交货"]
[null,"内蒙古东部电力有限公司","","0.5S级三相智能电能表","三相智能电能表-准确度等级:0.5S级,费控方式:无,负荷开关:无控,通信模块接口:无,电压规格:3×100V,电流规格:1.5A","只","2","2017-12-31","施工现场地面交货"]
[null,"内蒙古东部电力有限公司","","0.5S级三相智能电能表","三相智能电能表-准确度等级:0.5S级,费控方式:无,负荷开关:无控,通信模块接口:无,电压规格:3×100V,电流规格:1.5A","只","26","2017-12-31","买方指定仓库地面交货"]
[null,"内蒙古东部电力有限公司","","0.5S级三相智能电能表","三相智能电能表-准确度等级:0.5S级,费控方式:无,负荷开关:无控,通信模块接口:无,电压规格:3×100V,电流规格:1.5A","只","48","2017-12-31","买方指定仓库地面交货"]
[null,"内蒙古东部电力有限公司","","0.5S级三相智能电能表","三相智能电能表-准确度等级:0.5S级,费控方式:无,负荷开关:无控,通信模块接口:无,电压规格:3×220/380V,电流规格:1.5A","只","7","2017-12-31","买方指定仓库地面交货"]
[null,"内蒙古东部电力有限公司","","0.5S级三相智能电能表","三相智能电能表-准确度等级:0.5S级,费控方式:无,负荷开关:无控,通信模块接口:无,电压规格:3×100V,电流规格:1.5A","只","3","2017-12-31","买方指定仓库地面交货"]
[null,"内蒙古东部电力有限公司","","0.5S级三相智能电能表","三相智能电能表-准确度等级:0.5S级,费控方式:无,负荷开关:无控,通信模块接口:无,电压规格:3×220/380V,电流规格:1.5A","只","328","2017-12-31","买方指定仓库地面交货"]
[null,"内蒙古东部电力有限公司","","0.5S级三相智能电能表","三相智能电能表-准确度等级:0.5S级,费控方式:无,负荷开关:无控,通信模块接口:无,电压规格:3×100V,电流规格:1.5A","只","21","2017-12-31","买方指定仓库地面交货"]
[null,"内蒙古东部电力有限公司","","0.5S级三相智能电能表","三相智能电能表-准确度等级:0.5S级,费控方式:无,负荷开关:无控,通信模块接口:无,电压规格:3×100V,电流规格:1.5A","只","1","2017-12-31","买方指定仓库地面交货"]
[null,"内蒙古东部电力有限公司","","0.5S级三相智能电能表","三相智能电能表-准确度等级:0.5S级,费控方式:无,负荷开关:无控,通信模块接口:无,电压规格:3×100V,电流规格:1.5A","只","1","2017-12-31","买方指定仓库地面交货"]
[null,"内蒙古东部电力有限公司","","0.5S级三相智能电能表","三相智能电能表-准确度等级:0.5S级,费控方式:无,负荷开关:无控,通信模块接口:无,电压规格:3×100V,电流规格:1.5A","只","7","2017-12-31","买方指定仓库地面交货"]
[null,"内蒙古东部电力有限公司","","0.5S级三相智能电能表","三相智能电能表-准确度等级:0.5S级,费控方式:无,负荷开关:无控,通信模块接口:无,电压规格:3×100V,电流规格:1.5A","只","54","2017-12-31","买方指定仓库地面交货"]
[null,"内蒙古东部电力有限公司","","0.5S级三相智能电能表","三相智能电能表-准确度等级:0.5S级,费控方式:无,负荷开关:无控,通信模块接口:无,电压规格:3×100V,电流规格:1.5A","只","4","2017-12-31","买方指定仓库地面交货"]
[null,"内蒙古东部电力有限公司","","0.5S级三相智能电能表","三相智能电能表-准确度等级:0.5S级,费控方式:无,负荷开关:无控,通信模块接口:无,电压规格:3×220/380V,电流规格:1.5A","只","70","2017-12-31","买方指定仓库地面交货"]
[null,"内蒙古东部电力有限公司","","0.5S级三相智能电能表","三相智能电能表-准确度等级:0.5S级,费控方式:无,负荷开关:无控,通信模块接口:无,电压规格:3×220/380V,电流规格:1.5A","只","158","2017-12-31","买方指定仓库地面交货"]
[null,"内蒙古东部电力有限公司","","0.5S级三相智能电能表","三相智能电能表-准确度等级:0.5S级,费控方式:无,负荷开关:无控,通信模块接口:无,电压规格:3×220/380V,电流规格:1.5A","只","438","2017-12-31","买方指定仓库地面交货"]
[null,"内蒙古东部电力有限公司","","0.5S级三相智能电能表","三相智能电能表-准确度等级:0.5S级,费控方式:无,负荷开关:无控,通信模块接口:无,电压规格:3×220/380V,电流规格:1.5A","只","19","2017-12-31","买方指定仓库地面交货"]
[null,"内蒙古东部电力有限公司","","0.5S级三相智能电能表","三相智能电能表-准确度等级:0.5S级,费控方式:无,负荷开关:无控,通信模块接口:无,电压规格:3×100V,电流规格:1.5A","只","1","2017-12-31","买方指定仓库地面交货"]
[null,"内蒙古东部电力有限公司","","0.5S级三相智能电能表","三相智能电能表-准确度等级:0.5S级,费控方式:无,负荷开关:无控,通信模块接口:无,电压规格:3×220/380V,电流规格:1.5A","只","100","2017-12-31","买方指定仓库地面交货"]
[null,"内蒙古东部电力有限公司","","0.5S级三相智能电能表","三相智能电能表-准确度等级:0.5S级,费控方式:无,负荷开关:无控,通信模块接口:无,电压规格:3×220/380V,电流规格:1.5A","只","2","2017-12-31","买方指定仓库地面交货"]
[null,"内蒙古东部电力有限公司","","0.5S级三相智能电能表","三相智能电能表-准确度等级:0.5S级,费控方式:无,负荷开关:无控,通信模块接口:无,电压规格:3×220/380V,电流规格:1.5A","只","2150","2017-12-31","买方指定仓库地面交货"]
[null,"内蒙古东部电力有限公司","","0.5S级三相智能电能表","三相智能电能表-准确度等级:0.5S级,费控方式:无,负荷开关:无控,通信模块接口:无,电压规格:3×57.7/100V,电流规格:1.5A","只","276","2017-12-31","买方指定仓库地面交货"]
[null,"内蒙古东部电力有限公司","","0.5S级三相智能电能表","三相智能电能表-准确度等级:0.5S级,费控方式:无,负荷开关:无控,通信模块接口:无,电压规格:3×100V,电流规格:1.5A","只","90","2017-12-31","买方指定仓库地面交货"]
[null,"内蒙古东部电力有限公司","","0.5S级三相智能电能表","三相智能电能表-准确度等级:0.5S级,费控方式:无,负荷开关:无控,通信模块接口:无,电压规格:3×220/380V,电流规格:1.5A","只","1045","2017-12-31","买方指定仓库地面交货"]
[null,"内蒙古东部电力有限公司","","0.5S级三相智能电能表","三相智能电能表-准确度等级:0.5S级,费控方式:无,负荷开关:无控,通信模块接口:无,电压规格:3×220/380V,电流规格:1.5A","只","150","2017-12-31","买方指定仓库地面交货"]
[null,"辽宁省电力有限公司","","0.5S级三相智能电能表","三相智能电能表-准确度等级:0.5S级,费控方式:无,负荷开关:无控,通信模块接口:无,电压规格:3×100V,电流规格:1.5A","只","300","2017-07-24","买方指定仓库地面交货"]
[null,"辽宁省电力有限公司","","0.5S级三相智能电能表","三相智能电能表-准确度等级:0.5S级,费控方式:无,负荷开关:无控,通信模块接口:无,电压规格:3×100V,电流规格:1.5A","只","350","2017-08-22","买方指定仓库地面交货"]
[null,"辽宁省电力有限公司","","0.5S级三相智能电能表","三相智能电能表-准确度等级:0.5S级,费控方式:无,负荷开关:无控,通信模块接口:无,电压规格:3×220/380V,电流规格:1.5A","只","200","2017-09-15","买方指定仓库地面交货"]
[null,"内蒙古东部电力有限公司","","0.5S级三相表本地通信单元（窄带）","通信单元-通信单元类别:本地,适用终端/表类型:0.5S级三相表,通信方式:窄带载波,频率范围/中心频率:其他,调制方式:其他","只","21","2017-12-31","买方指定仓库地面交货"]
[null,"内蒙古东部电力有限公司","","0.5S级三相表本地通信单元（窄带）","通信单元-通信单元类别:本地,适用终端/表类型:0.5S级三相表,通信方式:窄带载波,频率范围/中心频率:421kHz,调制方式:BFSK","只","460","2017-12-31","买方指定仓库地面交货"]
[null,"内蒙古东部电力有限公司","","0.5S级三相表本地通信单元（窄带）","通信单元-通信单元类别:本地,适用终端/表类型:0.5S级三相表,通信方式:窄带载波,频率范围/中心频率:421kHz,调制方式:BFSK","只","53","2017-12-31","买方指定仓库地面交货"]
[null,"内蒙古东部电力有限公司","","0.5S级三相智能电能表","三相智能电能表-准确度等级:0.5S级,费控方式:无,负荷开关:无控,通信模块接口:无,电压规格:3×220/380V,电流规格:1.5A","只","22","2017-12-31","买方指定仓库地面交货"]
[null,"内蒙古东部电力有限公司","","0.5S级三相智能电能表","三相智能电能表-准确度等级:0.5S级,费控方式:无,负荷开关:无控,通信模块接口:无,电压规格:3×100V,电流规格:1.5A","只","12","2017-12-31","买方指定仓库地面交货"]
[null,"内蒙古东部电力有限公司","","0.5S级三相智能电能表","三相智能电能表-准确度等级:0.5S级,费控方式:无,负荷开关:无控,通信模块接口:无,电压规格:3×100V,电流规格:1.5A","只","16","2017-12-31","买方指定仓库地面交货"]
[null,"内蒙古东部电力有限公司","","0.5S级三相智能电能表","三相智能电能表-准确度等级:0.5S级,费控方式:无,负荷开关:无控,通信模块接口:无,电压规格:3×100V,电流规格:1.5A","只","205","2017-12-31","买方指定仓库地面交货"]
[null,"内蒙古东部电力有限公司","","0.5S级三相智能电能表","三相智能电能表-准确度等级:0.5S级,费控方式:无,负荷开关:无控,通信模块接口:无,电压规格:3×57.7/100V,电流规格:1.5A","只","40","2017-12-31","买方指定仓库地面交货"]
[null,"内蒙古东部电力有限公司","","0.5S级三相智能电能表","三相智能电能表-准确度等级:0.5S级,费控方式:无,负荷开关:无控,通信模块接口:无,电压规格:3×100V,电流规格:1.5A","只","45","2017-12-31","买方指定仓库地面交货"]
[null,"内蒙古东部电力有限公司","","0.5S级三相智能电能表","三相智能电能表-准确度等级:0.5S级,费控方式:无,负荷开关:无控,通信模块接口:无,电压规格:3×220/380V,电流规格:1.5A","只","11","2017-12-31","买方指定仓库地面交货"]
[null,"内蒙古东部电力有限公司","","0.5S级三相智能电能表","三相智能电能表-准确度等级:0.5S级,费控方式:无,负荷开关:无控,通信模块接口:无,电压规格:3×220/380V,电流规格:1.5A","只","400","2017-12-31","买方指定仓库地面交货"]
[null,"内蒙古东部电力有限公司","","0.5S级三相智能电能表","三相智能电能表-准确度等级:0.5S级,费控方式:无,负荷开关:无控,通信模块接口:无,电压规格:3×100V,电流规格:1.5A","只","556","2017-12-31","买方指定仓库地面交货"]
[null,"内蒙古东部电力有限公司","","0.5S级三相智能电能表","三相智能电能表-准确度等级:0.5S级,费控方式:无,负荷开关:无控,通信模块接口:无,电压规格:3×57.7/100V,电流规格:1.5A","只","129","2017-12-31","买方指定仓库地面交货"]
[null,"内蒙古东部电力有限公司","","0.5S级三相智能电能表","三相智能电能表-准确度等级:0.5S级,费控方式:无,负荷开关:无控,通信模块接口:无,电压规格:3×100V,电流规格:1.5A","只","15","2017-12-31","买方指定仓库地面交货"]
["包35GW4","上海市电力公司","国网上海公司2017年第一次电能表（含用电信息采集）项目","0.5S级三相智能电能表","三相智能电能表-准确度等级:0.5S级,费控方式:无,负荷开关:无控,通信模块接口:无,电压规格:3×220/380V,电流规格:1.5A","只","6000","2018-04-30","买方指定仓库车板交货"]
[null,"上海市电力公司","国网上海公司2017年第一次电能表（含用电信息采集）项目","0.5S级三相智能电能表","三相智能电能表-准确度等级:0.5S级,费控方式:无,负荷开关:无控,通信模块接口:无,电压规格:3×100V,电流规格:1.5A","只","6000","2018-04-30","买方指定仓库车板交货"]
[null,"上海市电力公司","国网上海公司2017年第一次电能表（含用电信息采集）项目","0.5S级三相智能电能表","三相智能电能表-准确度等级:0.5S级,费控方式:无,负荷开关:无控,通信模块接口:无,电压规格:3×57.7/100V,电流规格:1.5A","只","5000","2018-04-30","买方指定仓库车板交货"]
[null,"新疆电力公司","国家电网公司2017年第一次电能表（含用电信息采集）","0.5S级三相智能电能表","三相智能电能表-准确度等级:0.5S级,费控方式:无,负荷开关:无控,通信模块接口:无,电压规格:3×100V,电流规格:1.5A","只","3700","2017-10-30","买方指定仓库车板交货"]
["包35GW5","西藏电力有限公司","国网西藏电力有限公司各供电公司营销专项、电网基建/户表","0.5S级三相智能电能表","三相智能电能表-准确度等级:0.5S级,费控方式:无,负荷开关:无控,通信模块接口:无,电压规格:3×57.7/100V,电流规格:1.5A","只","31","2017-06-30","买方指定仓库地面交货"]
[null,"浙江省电力公司","","0.5S级三相智能电能表","三相智能电能表-准确度等级:0.5S级,费控方式:无,负荷开关:无控,通信模块接口:无,电压规格:3×100V,电流规格:1.5A","只","41000","2019-03-31","买方指定仓库地面交货"]
["包35CQ1","重庆市电力公司","国网重庆公司2017年营销类物资协议库存招标采购","0.5S级三相智能电能表","三相智能电能表-准确度等级:0.5S级,费控方式:无,负荷开关:无控,通信模块接口:无,电压规格:3×57.7/100V,电流规格:1.5A","只","1000","2018-06-16","买方指定仓库地面交货"]
[null,"重庆市电力公司","国网重庆公司2017年营销类物资协议库存招标采购","0.5S级三相智能电能表","三相智能电能表-准确度等级:0.5S级,费控方式:无,负荷开关:无控,通信模块接口:无,电压规格:3×220/380V,电流规格:1.5A","只","10000","2018-06-16","买方指定仓库地面交货"]
[null,"重庆市电力公司","国网重庆公司2017年营销类物资协议库存招标采购","0.5S级三相智能电能表","三相智能电能表-准确度等级:0.5S级,费控方式:无,负荷开关:无控,通信模块接口:无,电压规格:3×100V,电流规格:1.5A","只","13000","2018-06-16","买方指定仓库地面交货"]
["包35JX1","江西省电力公司","","0.5S级三相智能电能表","三相智能电能表-准确度等级:0.5S级,费控方式:无,负荷开关:无控,通信模块接口:无,电压规格:3×100V,电流规格:1.5A","只","30000","2017-09-15","买方指定仓库地面交货"]
["包35JX2","江西省电力公司","","0.5S级三相智能电能表","三相智能电能表-准确度等级:0.5S级,费控方式:无,负荷开关:无控,通信模块接口:无,电压规格:3×100V,电流规格:1.5A","只","20000","2017-09-15","买方指定仓库地面交货"]

{"sheet":"0.2S级三相智能电能表","index":3,"n_rows":15,"n_cols":9,"rows_kept":15,"merged":[[0,0,0,8],[1,0,1,8],[3,0,6,0],[7,0,10,0],[11,0,13,0]],"flags":["formulas_cached_only"]}
["国家电网公司2017年第一次电能表及用电信息采集设备招标活动\n货物需求一览表\n(0.2S级三相智能电能表)"]
["分标编号:0711-17OTL03922000-4"]
["包号","项目单位","项目名称","招标货物","物资描述","单位","行数量","交货日期","交货地点"]
["包36GW1","江西省电力公司","","0.2S级三相智能电能表","三相智能电能表-准确度等级:0.2S级,费控方式:无,负荷开关:无控,通信模块接口:无,电压规格:3×100V,电流规格:1.5A","只","1000","2017-09-15","买方指定仓库地面交货"]
[null,"安徽省电力公司","","0.2S级三相智能电能表","三相智能电能表-准确度等级:0.2S级,费控方式:无,负荷开关:无控,通信模块接口:无,电压规格:3×100V,电流规格:1.5A","只","400","2017-07-10","买方指定仓库地面交货"]
[null,"重庆市电力公司","国网重庆公司2017年营销类物资协议库存招标采购","0.2S级三相智能电能表","三相智能电能表-准确度等级:0.2S级,费控方式:无,负荷开关:无控,通信模块接口:无,电压规格:3×57.7/100V,电流规格:1.5A","只","400","2018-06-16","买方指定仓库地面交货"]
[null,"重庆市电力公司","国网重庆公司2017年营销类物资协议库存招标采购","0.2S级三相智能电能表","三相智能电能表-准确度等级:0.2S级,费控方式:无,负荷开关:无控,通信模块接口:无,电压规格:3×100V,电流规格:1.5A","只","200","2018-06-16","买方指定仓库地面交货"]
["包36GW2","黑龙江省电力有限公司","","0.2S级三相智能电能表","三相智能电能表-准确度等级:0.2S级,费控方式:无,负荷开关:无控,通信模块接口:无,电压规格:3×100V,电流规格:1.5A","只","209","2018-04-20","买方指定仓库地面交货"]
[null,"辽宁省电力有限公司","","0.2S级三相智能电能表","三相智能电能表-准确度等级:0.2S级,费控方式:无,负荷开关:无控,通信模块接口:无,电压规格:3×100V,电流规格:1.5A","只","100","2017-08-23","买方指定仓库地面交货"]
[null,"辽宁省电力有限公司","","0.2S级三相智能电能表","三相智能电能表-准确度等级:0.2S级,费控方式:无,负荷开关:无控,通信模块接口:无,电压规格:3×57.7/100V,电流规格:0.3A","只","20","2017-09-21","买方指定仓库地面交货"]
[null,"辽宁省电力有限公司","","0.2S级三相智能电能表","三相智能电能表-准确度等级:0.2S级,费控方式:无,负荷开关:无控,通信模块接口:无,电压规格:3×100V,电流规格:1.5A","只","480","2017-09-21","买方指定仓库地面交货"]
["包36FJ1","福建省电力有限公司","国网福建省电力有限公司采购","0.2S级三相智能电能表","三相智能电能表-准确度等级:0.2S级,费控方式:无,负荷开关:无控,通信模块接口:无,电压规格:3×57.7/100V,电流规格:1.5A","只","1780","2018-06-30","买方指定仓库地面交货"]
[null,"福建省电力有限公司","国网福建省电力有限公司采购","0.2S级三相智能电能表","三相智能电能表-准确度等级:0.2S级,费控方式:无,负荷开关:无控,通信模块接口:无,电压规格:3×57.7/100V,电流规格:0.3A","只","240","2018-06-30","买方指定仓库地面交货"]
[null,"福建省电力有限公司","国网福建省电力有限公司采购","0.2S级三相智能电能表","三相智能电能表-准确度等级:0.2S级,费控方式:无,负荷开关:无控,通信模块接口:无,电压规格:3×100V,电流规格:1.5A","只","2160","2018-06-30","买方指定仓库地面交货"]
["包36ZJ1","浙江省电力公司","","0.2S级三相智能电能表","三相智能电能表-准确度等级:0.2S级,费控方式:无,负荷开关:无控,通信模块接口:无,电压规格:3×100V,电流规格:1.5A","只","1300","2019-03-31","买方指定仓库地面交货"]

{"sheet":"集中器、采集器","index":4,"n_rows":419,"n_cols":9,"rows_kept":419,"merged":[[0,0,0,8],[1,0,1,8],[3,0,16,0],[17,0,23,0],[24,0,27,0],[28,0,29,0],[30,0,31,0],[32,0,33,0],[34,0,35,0],[36,0,37,0],[38,0,39,0],[40,0,41,0],[42,0,43,0],[44,0,58,0],[59,0,160,0],[161,0,178,0],[179,0,206,0],[207,0,228,0],[229,0,233,0],[234,0,237,0],[238,0,241,0],[242,0,249,0],[250,0,255,0],[256,0,276,0],[277,0,288,0],[289,0,302,0],[303,0,316,0],[317,0,351,0],[352,0,358,0],[359,0,365,0],[366,0,372,0],[373,0,379,0],[380,0,386,0],[387,0,393,0],[394,0,400,0],[401,0,407,0],[408,0,418,0]],"flags":["formulas_cached_only"]}
["国家电网公司2017年第一次电能表及用电信息采集设备招标活动\n货物需求一览表\n(集中器、采集器)"]
["分标编号:0711-17OTL03922000-5"]
["包号","项目单位","项目名称","招标货物","物资描述","单位","行数量","交货日期","交货地点"]
["包J1GW1","内蒙古东部电力有限公司","","集中器I型（无线公网GPRS/窄带载波）","集中器-设备类别:I型,远程通信:GPRS,本地通信:电力线窄带载波,交采功能:有,温度等级:C3","台","4","2017-12-31","买方指定仓库地面交货"]
[null,"内蒙古东部电力有限公司","","集中器I型（无线公网GPRS/窄带载波）","集中器-设备类别:I型,远程通信:GPRS,本地通信:电力线窄带载波,交采功能:有,温度等级:C3","台","47","2017-12-31","买方指定仓库地面交货"]
[null,"山东电力集团公司","","采集器II型（窄带载波）","采集器-设备类别:II型,采集器与集中器通信方式:电力线窄带载波,交采功能:无,温度等级:C3","台","184310","2018-06-30","买方指定仓库地面交货"]
[null,"山东电力集团公司","","集中器I型远程通信单元（4G）","通信单元-通信单元类别:远程,适用终端/表类型:集中器I型,通信方式:无线公网4G,频率范围/中心频率:无,调制方式:无","只","4060","2018-06-30","买方指定仓库地面交货"]
[null,"内蒙古东部电力有限公司","","集中器I型远程通信单元（GPRS）","通信单元-通信单元类别:远程,适用终端/表类型:集中器I型,通信方式:无线公网GPRS,频率范围/中心频率:无,调制方式:无","只","47","2017-12-31","买方指定仓库地面交货"]
[null,"内蒙古东部电力有限公司","","集中器I型远程通信单元（GPRS）","通信单元-通信单元类别:远程,适用终端/表类型:集中器I型,通信方式:无线公网GPRS,频率范围/中心频率:无,调制方式:无","只","4935","2017-12-31","买方指定仓库地面交货"]
[null,"内蒙古东部电力有限公司","","集中器I型远程通信单元（GPRS）","通信单元-通信单元类别:远程,适用终端/表类型:集中器I型,通信方式:无线公网GPRS,频率范围/中心频率:无,调制方式:无","只","22","2017-12-31","买方指定仓库地面交货"]
[null,"内蒙古东部电力有限公司","","集中器I型（无线公网GPRS/窄带载波）","集中器-设备类别:I型,远程通信:GPRS,本地通信:电力线窄带载波,交采功能:有,温度等级:C3","台","153","2017-12-31","买方指定仓库地面交货"]
[null,"内蒙古东部电力有限公司","","集中器I型（无线公网GPRS/窄带载波）","集中器-设备类别:I型,远程通信:GPRS,本地通信:电力线窄带载波,交采功能:有,温度等级:C3","台","4935","2017-12-31","买方指定仓库地面交货"]
[null,"山东电力集团公司","","采集器II型本地通信单元（窄带）","通信单元-通信单元类别:本地,适用终端/表类型:采集器II型,通信方式:窄带载波,频率范围/中心频率:其他,调制方式:其他","只","68080","2018-06-30","买方指定仓库地面交货"]
[null,"山东电力集团公司","","采集器II型本地通信单元（窄带）","通信单元-通信单元类别:本地,适用终端/表类型:采集器II型,通信方式:窄带载波,频率范围/中心频率:421kHz,调制方式:BFSK","只","116230","2018-06-30","买方指定仓库地面交货"]
[null,"山东电力集团公司","","集中器I型（无线公网GPRS/窄带载波）","集中器-设备类别:I型,远程通信:GPRS,本地通信:电力线窄带载波,交采功能:有,温度等级:C3","台","4060","2018-06-30","买方指定仓库地面交货"]
[null,"山东电力集团公司","","集中器I型本地通信单元（窄带）","通信单元-通信单元类别:本地,适用终端/表类型:集中器I型,通信方式:窄带载波,频率范围/中心频率:421kHz,调制方式:BFSK","只","4466","2018-06-30","买方指定仓库地面交货"]
[null,"山东电力集团公司","","集中器I型本地通信单元（窄带）","通信单元-通信单元类别:本地,适用终端/表类型:集中器I型,通信方式:窄带载波,频率范围/中心频率:其他,调制方式:其他","只","4466","2018-06-30","买方指定仓库地面交货"]
["包J1SD1","山东电力集团公司","","采集器II型本地通信单元（窄带）","通信单元-通信单元类别:本地,适用终端/表类型:采集器II型,通信方式:窄带载波,频率范围/中心频率:其他,调制方式:其他","只","68080","2018-06-30","买方指定仓库地面交货"]
[null,"山东电力集团公司","","采集器II型（窄带载波）","采集器-设备类别:II型,采集器与集中器通信方式:电力线窄带载波,交采功能:无,温度等级:C3","台","184310","2018-06-30","买方指定仓库地面交货"]
[null,"山东电力集团公司","","集中器I型本地通信单元（窄带）","通信单元-通信单元类别:本地,适用终端/表类型:集中器I型,通信方式:窄带载波,频率范围/中心频率:其他,调制方式:其他","只","2420","2018-06-30","买方指定仓库地面交货"]
[null,"山东电力集团公司","","采集器II型本地通信单元（窄带）","通信单元-通信单元类别:本地,适用终端/表类型:采集器II型,通信方式:窄带载波,频率范围/中心频率:421kHz,调制方式:BFSK","只","116230","2018-06-30","买方指定仓库地面交货"]
[null,"山东电力集团公司","","集中器I型远程通信单元（4G）","通信单元-通信单元类别:远程,适用终端/表类型:集中器I型,通信方式:无线公网4G,频率范围/中心频率:无,调制方式:无","只","14380","2018-06-30","买方指定仓库地面交货"]
[null,"山东电力集团公司","","集中器I型（无线公网GPRS/窄带载波）","集中器-设备类别:I型,远程通信:GPRS,本地通信:电力线窄带载波,交采功能:有,温度等级:C3","台","14380","2018-06-30","买方指定仓库地面交货"]
[null,"山东电力集团公司","","集中器I型本地通信单元（窄带）","通信单元-通信单元类别:本地,适用终端/表类型:集中器I型,通信方式:窄带载波,频率范围/中心频率:421kHz,调制方式:BFSK","只","8932","2018-06-30","买方指定仓库地面交货"]
["包J7GW1","天津市电力公司","","集中器II型（无线公网GPRS）","集中器-设备类别:II型,远程通信:GPRS,本地通信:RS-485,交采功能:无,温度等级:C3","台","3000","2017-12-31","买方指定仓库地面交货"]
[null,"天津市电力公司","","集中器II型远程通信单元（GPRS）","通信单元-通信单元类别:远程,适用终端/表类型:集中器II型,通信方式:无线公网GPRS,频率范围/中心频率:无,调制方式:无","只","3000","2017-12-31","买方指定仓库地面交货"]
[null,"山东电力集团公司","","集中器II型远程通信单元（4G）","通信单元-通信单元类别:远程,适用终端/表类型:集中器II型,通信方式:无线公网4G,频率范围/中心频率:无,调制方式:无","只","74370","2018-06-30","买方指定仓库地面交货"]
[null,"山东电力集团公司","","集中器II型（无线公网GPRS）","集中器-设备类别:II型,远程通信:GPRS,本地通信:RS-485,交采功能:无,温度等级:C3","台","74370","2018-06-30","买方指定仓库地面交货"]
["包J7SD1","山东电力集团公司","","集中器II型远程通信单元（4G）","通信单元-通信单元类别:远程,适用终端/表类型:集中器II型,通信方式:无线公网4G,频率范围/中心频率:无,调制方式:无","只","77000","2018-06-30","买方指定仓库地面交货"]
[null,"山东电力集团公司","","集中器II型（无线公网GPRS）","集中器-设备类别:II型,远程通信:GPRS,本地通信:RS-485,交采功能:无,温度等级:C3","台","77000","2018-06-30","买方指定仓库地面交货"]
["包J7SD2","山东电力集团公司","","集中器II型远程通信单元（4G）","通信单元-通信单元类别:远程,适用终端/表类型:集中器II型,通信方式:无线公网4G,频率范围/中心频率:无,调制方式:无","只","77000","2018-06-30","买方指定仓库地面交货"]
[null,"山东电力集团公司","","集中器II型（无线公网GPRS）","集中器-设备类别:II型,远程通信:GPRS,本地通信:RS-485,交采功能:无,温度等级:C3","台","77000","2018-06-30","买方指定仓库地面交货"]
["包J7SD3","山东电力集团公司","","集中器II型远程通信单元（4G）","通信单元-通信单元类别:远程,适用终端/表类型:集中器II型,通信方式:无线公网4G,频率范围/中心频率:无,调制方式:无","只","77000","2018-06-30","买方指定仓库地面交货"]
[null,"山东电力集团公司","","集中器II型（无线公网GPRS）","集中器-设备类别:II型,远程通信:GPRS,本地通信:RS-485,交采功能:无,温度等级:C3","台","77000","2018-06-30","买方指定仓库地面交货"]
["包J7SD4","山东电力集团公司","","集中器II型远程通信单元（4G）","通信单元-通信单元类别:远程,适用终端/表类型:集中器II型,通信方式:无线公网4G,频率范围/中心频率:无,调制方式:无","只","77000","2018-06-30","买方指定仓库地面交货"]
[null,"山东电力集团公司","","集中器II型（无线公网GPRS）","集中器-设备类别:II型,远程通信:GPRS,本地通信:RS-485,交采功能:无,温度等级:C3","台","77000","2018-06-30","买方指定仓库地面交货"]
["包J7SD5","山东电力集团公司","","集中器II型（无线公网GPRS）","集中器-设备类别:II型,远程通信:GPRS,本地通信:RS-485,交采功能:无,温度等级:C3","台","77000","2018-06-30","买方指定仓库地面交货"]
[null,"山东电力集团公司","","集中器II型远程通信单元（4G）","通信单元-通信单元类别:远程,适用终端/表类型:集中器II型,通信方式:无线公网4G,频率范围/中心频率:无,调制方式:无","只","77000","2018-06-30","买方指定仓库地面交货"]
["包J7SD6","山东电力集团公司","","集中器II型（无线公网GPRS）","集中器-设备类别:II型,远程通信:GPRS,本地通信:RS-485,交采功能:无,温度等级:C3","台","77000","2018-06-30","买方指定仓库地面交货"]
[null,"山东电力集团公司","","集中器II型远程通信单元（4G）","通信单元-通信单元类别:远程,适用终端/表类型:集中器II型,通信方式:无线公网4G,频率范围/中心频率:无,调制方式:无","只","77000","2018-06-30","买方指定仓库地面交货"]
["包J7SD7","山东电力集团公司","","集中器II型（无线公网GPRS）","集中器-设备类别:II型,远程通信:GPRS,本地通信:RS-485,交采功能:无,温度等级:C3","台","77000","2018-06-30","买方指定仓库地面交货"]
[null,"山东电力集团公司","","集中器II型远程通信单元（4G）","通信单元-通信单元类别:远程,适用终端/表类型:集中器II型,通信方式:无线公网4G,频率范围/中心频率:无,调制方式:无","只","77000","2018-06-30","买方指定仓库地面交货"]
["包J7SD8","山东电力集团公司","","集中器II型远程通信单元（4G）","通信单元-通信单元类别:远程,适用终端/表类型:集中器II型,通信方式:无线公网4G,频率范围/中心频率:无,调制方式:无","只","77000","2018-06-30","买方指定仓库地面交货"]
[null,"山东电力集团公司","","集中器II型（无线公网GPRS）","集中器-设备类别:II型,远程通信:GPRS,本地通信:RS-485,交采功能:无,温度等级:C3","台","77000","2018-06-30","买方指定仓库地面交货"]
["包J14GW1","安徽省电力公司","","集中器I型远程通信单元（4G）","通信单元-通信单元类别:远程,适用终端/表类型:集中器I型,通信方式:无线公网4G,频率范围/中心频率:无,调制方式:无","只","15400","2017-07-10","买方指定仓库地面交货"]
[null,"安徽省电力公司","","采集器II型本地通信单元（窄带）","通信单元-通信单元类别:本地,适用终端/表类型:采集器II型,通信方式:窄带载波,频率范围/中心频率:132kHz,调制方式:BPSK","只","6200","2017-07-10","买方指定仓库地面交货"]
[null,"安徽省电力公司","","采集器II型（窄带载波）","采集器-设备类别:II型,采集器与集中器通信方式:电力线窄带载波,交采功能:无,温度等级:C3","台","36900","2017-07-10","买方指定仓库地面交货"]
[null,"福建省电力有限公司","国网福建省电力有限公司采购","集中器I型（无线公网4G/窄带载波）","集中器-设备类别:I型,远程通信:4G,本地通信:电力线窄带载波,交采功能:有,温度等级:C3","台","1500","2018-06-30","买方指定仓库地面交货"]
[null,"福建省电力有限公司","国网福建省电力有限公司采购","采集器II型本地通信单元（窄带）","通信单元-通信单元类别:本地,适用终端/表类型:采集器II型,通信方式:窄带载波,频率范围/中心频率:421kHz,调制方式:BFSK","只","250","2018-06-30","买方指定仓库地面交货"]
[null,"福建省电力有限公司","国网福建省电力有限公司采购","采集器II型（窄带载波）","采集器-设备类别:II型,采集器与集中器通信方式:电力线窄带载波,交采功能:无,温度等级:C3","台","250","2018-06-30","买方指定仓库地面交货"]
[null,"福建省电力有限公司","国网福建省电力有限公司采购","集中器I型远程通信单元（4G）","通信单元-通信单元类别:远程,适用终端/表类型:集中器I型,通信方式:无线公网4G,频率范围/中心频率:无,调制方式:无","只","2250","2018-06-30","买方指定仓库地面交货"]
[null,"福建省电力有限公司","国网福建省电力有限公司采购","专变III型远程通信单元（4G）","通信单元-通信单元类别:远程,适用终端/表类型:专变III型,通信方式:无线公网4G,频率范围/中心频率:无,调制方式:无","只","3798","2018-06-30","买方指定仓库地面交货"]
[null,"福建省电力有限公司","国网福建省电力有限公司采购","集中器I型本地通信单元（窄带）","通信单元-通信单元类别:本地,适用终端/表类型:集中器I型,通信方式:窄带载波,频率范围/中心频率:270kHz,调制方式:BFSK","只","1180","2018-06-30","买方指定仓库地面交货"]
[null,"福建省电力有限公司","国网福建省电力有限公司采购","集中器I型本地通信单元（窄带）","通信单元-通信单元类别:本地,适用终端/表类型:集中器I型,通信方式:窄带载波,频率范围/中心频率:其他,调制方式:其他","只","1500","2018-06-30","买方指定仓库地面交货"]
[null,"安徽省电力公司","","集中器I型本地通信单元（窄带）","通信单元-通信单元类别:本地,适用终端/表类型:集中器I型,通信方式:窄带载波,频率范围/中心频率:421kHz,调制方式:BFSK","只","12710","2017-07-10","买方指定仓库地面交货"]
[null,"安徽省电力公司","","集中器I型（无线公网4G/窄带载波）","集中器-设备类别:I型,远程通信:4G,本地通信:电力线窄带载波,交采功能:有,温度等级:C3","台","15400","2017-07-10","买方指定仓库地面交货"]
[null,"安徽省电力公司","","集中器I型本地通信单元（窄带）","通信单元-通信单元类别:本地,适用终端/表类型:集中器I型,通信方式:窄带载波,频率范围/中心频率:其他,调制方式:其他","只","30","2017-07-10","买方指定仓库地面交货"]
[null,"安徽省电力公司","","集中器I型本地通信单元（窄带）","通信单元-通信单元类别:本地,适用终端/表类型:集中器I型,通信方式:窄带载波,频率范围/中心频率:132kHz,调制方式:BPSK","只","2660","2017-07-10","买方指定仓库地面交货"]
[null,"安徽省电力公司","","采集器II型本地通信单元（窄带）","通信单元-通信单元类别:本地,适用终端/表类型:采集器II型,通信方式:窄带载波,频率范围/中心频率:421kHz,调制方式:BFSK","只","30700","2017-07-10","买方指定仓库地面交货"]
["包J14GW2","辽宁省电力有限公司","","集中器I型本地通信单元（窄带）","通信单元-通信单元类别:本地,适用终端/表类型:集中器I型,通信方式:窄带载波,频率范围/中心频率:270kHz,调制方式:BFSK","只","730","2017-07-24","买方指定仓库地面交货"]
[null,"辽宁省电力有限公司","","集中器I型（无线公网4G/窄带载波）","集中器-设备类别:I型,远程通信:4G,本地通信:电力线窄带载波,交采功能:有,温度等级:C3","台","730","2017-07-24","买方指定仓库地面交货"]
[null,"辽宁省电力有限公司","","集中器I型（无线公网4G/窄带载波）","集中器-设备类别:I型,远程通信:4G,本地通信:电力线窄带载波,交采功能:有,温度等级:C3","台","860","2017-09-22","买方指定仓库地面交货"]
[null,"辽宁省电力有限公司","","集中器I型（无线公网4G/窄带载波）","集中器-设备类别:I型,远程通信:4G,本地通信:电力线窄带载波,交采功能:有,温度等级:C3","台","450","2017-09-22","买方指定仓库地面交货"]
[null,"辽宁省电力有限公司","","集中器I型远程通信单元（4G）","通信单元-通信单元类别:远程,适用终端/表类型:集中器I型,通信方式:无线公网4G,频率范围/中心频率:无,调制方式:无","只","420","2017-07-25","买方指定仓库地面交货"]
[null,"辽宁省电力有限公司","","集中器I型远程通信单元（4G）","通信单元-通信单元类别:远程,适用终端/表类型:集中器I型,通信方式:无线公网4G,频率范围/中心频率:无,调制方式:无","只","196","2017-08-20","买方指定仓库地面交货"]
[null,"辽宁省电力有限公司","","集中器I型本地通信单元（窄带）","通信单元-通信单元类别:本地,适用终端/表类型:集中器I型,通信方式:窄带载波,频率范围/中心频率:其他,调制方式:其他","只","4000","2017-07-20","买方指定仓库地面交货"]
[null,"辽宁省电力有限公司","","集中器I型远程通信单元（4G）","通信单元-通信单元类别:远程,适用终端/表类型:集中器I型,通信方式:无线公网4G,频率范围/中心频率:无,调制方式:无","只","4000","2017-07-20","买方指定仓库地面交货"]
[null,"辽宁省电力有限公司","","集中器I型本地通信单元（窄带）","通信单元-通信单元类别:本地,适用终端/表类型:集中器I型,通信方式:窄带载波,频率范围/中心频率:270kHz,调制方式:BFSK","只","200","2017-08-23","买方指定仓库地面交货"]
[null,"辽宁省电力有限公司","","集中器I型远程通信单元（4G）","通信单元-通信单元类别:远程,适用终端/表类型:集中器I型,通信方式:无线公网4G,频率范围/中心频率:无,调制方式:无","只","200","2017-08-23","买方指定仓库地面交货"]
[null,"辽宁省电力有限公司","","集中器I型（无线公网4G/窄带载波）","集中器-设备类别:I型,远程通信:4G,本地通信:电力线窄带载波,交采功能:有,温度等级:C3","台","200","2017-08-23","买方指定仓库地面交货"]
[null,"辽宁省电力有限公司","","集中器I型（无线公网4G/窄带载波）","集中器-设备类别:I型,远程通信:4G,本地通信:电力线窄带载波,交采功能:有,温度等级:C3","台","4000","2017-07-20","买方指定仓库地面交货"]
[null,"辽宁省电力有限公司","","集中器I型远程通信单元（4G）","通信单元-通信单元类别:远程,适用终端/表类型:集中器I型,通信方式:无线公网4G,频率范围/中心频率:无,调制方式:无","只","4750","2017-08-20","买方指定仓库地面交货"]
[null,"辽宁省电力有限公司","","集中器I型（无线公网4G/窄带载波）","集中器-设备类别:I型,远程通信:4G,本地通信:电力线窄带载波,交采功能:有,温度等级:C3","台","4750","2017-08-20","买方指定仓库地面交货"]
[null,"辽宁省电力有限公司","","集中器I型本地通信单元（窄带）","通信单元-通信单元类别:本地,适用终端/表类型:集中器I型,通信方式:窄带载波,频率范围/中心频率:270kHz,调制方式:BFSK","只","3000","2017-08-20","买方指定仓库地面交货"]
[null,"内蒙古东部电力有限公司","","集中器I型（无线公网4G/窄带载波）","集中器-设备类别:I型,远程通信:4G,本地通信:电力线窄带载波,交采功能:有,温度等级:C3","台","29","2017-12-31","买方指定仓库地面交货"]
[null,"内蒙古东部电力有限公司","","集中器I型（无线公网4G/窄带载波）","集中器-设备类别:I型,远程通信:4G,本地通信:电力线窄带载波,交采功能:有,温度等级:C3","台","10","2017-12-31","买方指定仓库地面交货"]
[null,"内蒙古东部电力有限公司","","集中器I型（无线公网4G/窄带载波）","集中器-设备类别:I型,远程通信:4G,本地通信:电力线窄带载波,交采功能:有,温度等级:C3","台","30","2017-12-31","买方指定仓库地面交货"]
[null,"内蒙古东部电力有限公司","","集中器I型（无线公网4G/窄带载波）","集中器-设备类别:I型,远程通信:4G,本地通信:电力线窄带载波,交采功能:有,温度等级:C3","台","301","2017-12-31","买方指定仓库地面交货"]
[null,"内蒙古东部电力有限公司","","集中器I型（无线公网4G/窄带载波）","集中器-设备类别:I型,远程通信:4G,本地通信:电力线窄带载波,交采功能:有,温度等级:C3","台","1392","2017-12-31","买方指定仓库地面交货"]
[null,"内蒙古东部电力有限公司","","集中器I型（无线公网4G/窄带载波）","集中器-设备类别:I型,远程通信:4G,本地通信:电力线窄带载波,交采功能:有,温度等级:C3","台","330","2017-12-31","买方指定仓库地面交货"]
[null,"内蒙古东部电力有限公司","","集中器I型（无线公网4G/窄带载波）","集中器-设备类别:I型,远程通信:4G,本地通信:电力线窄带载波,交采功能:有,温度等级:C3","台","45","2017-12-31","买方指定仓库地面交货"]
[null,"内蒙古东部电力有限公司","","集中器I型（无线公网4G/窄带载波）","集中器-设备类别:I型,远程通信:4G,本地通信:电力线窄带载波,交采功能:有,温度等级:C3","台","328","2017-12-31","买方指定仓库地面交货"]
[null,"内蒙古东部电力有限公司","","集中器I型（无线公网4G/窄带载波）","集中器-设备类别:I型,远程通信:4G,本地通信:电力线窄带载波,交采功能:有,温度等级:C3","台","524","2017-12-31","买方指定仓库地面交货"]
[null,"辽宁省电力有限公司","","集中器I型（无线公网4G/窄带载波）","集中器-设备类别:I型,远程通信:4G,本地通信:电力线窄带载波,交采功能:有,温度等级:C3","台","2100","2017-09-21","买方指定仓库地面交货"]
[null,"辽宁省电力有限公司","","集中器I型远程通信单元（4G）","通信单元-通信单元类别:远程,适用终端/表类型:集中器I型,通信方式:无线公网4G,频率范围/中心频率:无,调制方式:无","只","2350","2017-09-21","买方指定仓库地面交货"]
[null,"辽宁省电力有限公司","","集中器I型本地通信单元（宽带）","通信单元-通信单元类别:本地,适用终端/表类型:集中器I型,通信方式:宽带载波,频率范围/中心频率:2～12MHz,调制方式:OFDM","只","2100","2017-09-21","买方指定仓库地面交货"]
[null,"辽宁省电力有限公司","","集中器I型本地通信单元（窄带）","通信单元-通信单元类别:本地,适用终端/表类型:集中器I型,通信方式:窄带载波,频率范围/中心频率:270kHz,调制方式:BFSK","只","3000","2017-09-15","买方指定仓库地面交货"]
[null,"辽宁省电力有限公司","","集中器I型本地通信单元（窄带）","通信单元-通信单元类别:本地,适用终端/表类型:集中器I型,通信方式:窄带载波,频率范围/中心频率:270kHz,调制方式:BFSK","只","723","2017-07-20","买方指定仓库地面交货"]
[null,"辽宁省电力有限公司","","集中器I型远程通信单元（4G）","通信单元-通信单元类别:远程,适用终端/表类型:集中器I型,通信方式:无线公网4G,频率范围/中心频率:无,调制方式:无","只","1446","2017-07-20","买方指定仓库地面交货"]
[null,"辽宁省电力有限公司","","集中器I型（无线公网4G/窄带载波）","集中器-设备类别:I型,远程通信:4G,本地通信:电力线窄带载波,交采功能:有,温度等级:C3","台","1446","2017-07-20","买方指定仓库地面交货"]
[null,"辽宁省电力有限公司","","集中器I型远程通信单元（4G）","通信单元-通信单元类别:远程,适用终端/表类型:集中器I型,通信方式:无线公网4G,频率范围/中心频率:无,调制方式:无","只","3000","2017-09-15","买方指定仓库地面交货"]
[null,"辽宁省电力有限公司","","集中器I型本地通信单元（窄带）","通信单元-通信单元类别:本地,适用终端/表类型:集中器I型,通信方式:窄带载波,频率范围/中心频率:421kHz,调制方式:BFSK","只","1750","2017-08-20","买方指定仓库地面交货"]
[null,"内蒙古东部电力有限公司","","集中器I型本地通信单元（窄带）","通信单元-通信单元类别:本地,适用终端/表类型:集中器I型,通信方式:窄带载波,频率范围/中心频率:270kHz,调制方式:BFSK","只","143","2017-12-31","买方指定仓库地面交货"]
[null,"内蒙古东部电力有限公司","","集中器I型本地通信单元（窄带）","通信单元-通信单元类别:本地,适用终端/表类型:集中器I型,通信方式:窄带载波,频率范围/中心频率:132kHz,调制方式:BPSK","只","11","2017-12-31","买方指定仓库地面交货"]
[null,"内蒙古东部电力有限公司","","集中器I型远程通信单元（4G）","通信单元-通信单元类别:远程,适用终端/表类型:集中器I型,通信方式:无线公网4G,频率范围/中心频率:无,调制方式:无","只","50","2017-12-31","买方指定仓库地面交货"]
[null,"内蒙古东部电力有限公司","","集中器I型远程通信单元（4G）","通信单元-通信单元类别:远程,适用终端/表类型:集中器I型,通信方式:无线公网4G,频率范围/中心频率:无,调制方式:无","只","69","2017-12-31","买方指定仓库地面交货"]
[null,"内蒙古东部电力有限公司","","集中器I型远程通信单元（4G）","通信单元-通信单元类别:远程,适用终端/表类型:集中器I型,通信方式:无线公网4G,频率范围/中心频率:无,调制方式:无","只","110","2017-12-31","买方指定仓库地面交货"]
[null,"内蒙古东部电力有限公司","","集中器I型远程通信单元（4G）","通信单元-通信单元类别:远程,适用终端/表类型:集中器I型,通信方式:无线公网4G,频率范围/中心频率:无,调制方式:无","只","100","2017-12-31","买方指定仓库地面交货"]
[null,"辽宁省电力有限公司","","集中器I型本地通信单元（窄带）","通信单元-通信单元类别:本地,适用终端/表类型:集中器I型,通信方式:窄带载波,频率范围/中心频率:270kHz,调制方式:BFSK","只","860","2017-08-31","买方指定仓库地面交货"]
[null,"辽宁省电力有限公司","","集中器I型远程通信单元（4G）","通信单元-通信单元类别:远程,适用终端/表类型:集中器I型,通信方式:无线公网4G,频率范围/中心频率:无,调制方式:无","只","1310","2017-08-31","买方指定仓库地面交货"]
[null,"辽宁省电力有限公司","","集中器I型本地通信单元（宽带）","通信单元-通信单元类别:本地,适用终端/表类型:集中器I型,通信方式:宽带载波,频率范围/中心频率:2～12MHz,调制方式:OFDM","只","450","2017-08-31","买方指定仓库地面交货"]
[null,"辽宁省电力有限公司","","集中器I型远程通信单元（4G）","通信单元-通信单元类别:远程,适用终端/表类型:集中器I型,通信方式:无线公网4G,频率范围/中心频率:无,调制方式:无","只","4480","2017-08-25","买方指定仓库地面交货"]
[null,"辽宁省电力有限公司","","集中器I型远程通信单元（4G）","通信单元-通信单元类别:远程,适用终端/表类型:集中器I型,通信方式:无线公网4G,频率范围/中心频率:无,调制方式:无","只","530","2017-08-20","买方指定仓库地面交货"]
[null,"辽宁省电力有限公司","","集中器I型远程通信单元（4G）","通信单元-通信单元类别:远程,适用终端/表类型:集中器I型,通信方式:无线公网4G,频率范围/中心频率:无,调制方式:无","只","730","2017-07-24","买方指定仓库地面交货"]
[null,"辽宁省电力有限公司","","集中器I型远程通信单元（4G）","通信单元-通信单元类别:远程,适用终端/表类型:集中器I型,通信方式:无线公网4G,频率范围/中心频率:无,调制方式:无","只","2750","2017-08-22","买方指定仓库地面交货"]
[null,"辽宁省电力有限公司","","集中器I型本地通信单元（窄带）","通信单元-通信单元类别:本地,适用终端/表类型:集中器I型,通信方式:窄带载波,频率范围/中心频率:421kHz,调制方式:BFSK","只","530","2017-08-20","买方指定仓库地面交货"]
[null,"辽宁省电力有限公司","","集中器I型（无线公网4G/窄带载波）","集中器-设备类别:I型,远程通信:4G,本地通信:电力线窄带载波,交采功能:有,温度等级:C3","台","530","2017-08-20","买方指定仓库地面交货"]
[null,"辽宁省电力有限公司","","集中器I型（无线公网4G/窄带载波）","集中器-设备类别:I型,远程通信:4G,本地通信:电力线窄带载波,交采功能:有,温度等级:C3","台","2750","2017-08-22","买方指定仓库地面交货"]
[null,"辽宁省电力有限公司","","集中器I型本地通信单元（窄带）","通信单元-通信单元类别:本地,适用终端/表类型:集中器I型,通信方式:窄带载波,频率范围/中心频率:270kHz,调制方式:BFSK","只","1750","2017-08-22","买方指定仓库地面交货"]
[null,"辽宁省电力有限公司","","集中器I型本地通信单元（窄带）","通信单元-通信单元类别:本地,适用终端/表类型:集中器I型,通信方式:窄带载波,频率范围/中心频率:421kHz,调制方式:BFSK","只","1000","2017-08-22","买方指定仓库地面交货"]
[null,"辽宁省电力有限公司","","集中器I型（无线公网4G/窄带载波）","集中器-设备类别:I型,远程通信:4G,本地通信:电力线窄带载波,交采功能:有,温度等级:C3","台","420","2017-07-25","买方指定仓库地面交货"]
[null,"辽宁省电力有限公司","","集中器I型本地通信单元（窄带）","通信单元-通信单元类别:本地,适用终端/表类型:集中器I型,通信方式:窄带载波,频率范围/中心频率:421kHz,调制方式:BFSK","只","420","2017-07-25","买方指定仓库地面交货"]
[null,"辽宁省电力有限公司","","集中器I型本地通信单元（窄带）","通信单元-通信单元类别:本地,适用终端/表类型:集中器I型,通信方式:窄带载波,频率范围/中心频率:421kHz,调制方式:BFSK","只","723","2017-07-20","买方指定仓库地面交货"]
[null,"辽宁省电力有限公司","","集中器I型（无线公网4G/窄带载波）","集中器-设备类别:I型,远程通信:4G,本地通信:电力线窄带载波,交采功能:有,温度等级:C3","台","3000","2017-09-15","买方指定仓库地面交货"]
[null,"辽宁省电力有限公司","","集中器I型（无线公网4G/窄带载波）","集中器-设备类别:I型,远程通信:4G,本地通信:电力线窄带载波,交采功能:有,温度等级:C3","台","96","2017-08-20","买方指定仓库地面交货"]
[null,"辽宁省电力有限公司","","集中器I型（无线公网4G/窄带载波）","集中器-设备类别:I型,远程通信:4G,本地通信:电力线窄带载波,交采功能:有,温度等级:C3","台","100","2017-08-20","买方指定仓库地面交货"]
[null,"辽宁省电力有限公司","","集中器I型本地通信单元（窄带）","通信单元-通信单元类别:本地,适用终端/表类型:集中器I型,通信方式:窄带载波,频率范围/中心频率:其他,调制方式:其他","只","96","2017-08-20","买方指定仓库地面交货"]
[null,"辽宁省电力有限公司","","集中器I型本地通信单元（窄带）","通信单元-通信单元类别:本地,适用终端/表类型:集中器I型,通信方式:窄带载波,频率范围/中心频率:其他,调制方式:其他","只","100","2017-08-20","买方指定仓库地面交货"]
[null,"内蒙古东部电力有限公司","","集中器I型本地通信单元（窄带）","通信单元-通信单元类别:本地,适用终端/表类型:集中器I型,通信方式:窄带载波,频率范围/中心频率:421kHz,调制方式:BFSK","只","29","2017-12-31","买方指定仓库地面交货"]
[null,"内蒙古东部电力有限公司","","集中器I型本地通信单元（窄带）","通信单元-通信单元类别:本地,适用终端/表类型:集中器I型,通信方式:窄带载波,频率范围/中心频率:421kHz,调制方式:BFSK","只","10","2017-12-31","买方指定仓库地面交货"]
[null,"内蒙古东部电力有限公司","","集中器I型本地通信单元（窄带）","通信单元-通信单元类别:本地,适用终端/表类型:集中器I型,通信方式:窄带载波,频率范围/中心频率:421kHz,调制方式:BFSK","只","100","2017-12-31","买方指定仓库地面交货"]
[null,"内蒙古东部电力有限公司","","集中器I型本地通信单元（窄带）","通信单元-通信单元类别:本地,适用终端/表类型:集中器I型,通信方式:窄带载波,频率范围/中心频率:270kHz,调制方式:BFSK","只","20","2017-12-31","买方指定仓库地面交货"]
[null,"内蒙古东部电力有限公司","","集中器I型本地通信单元（窄带）","通信单元-通信单元类别:本地,适用终端/表类型:集中器I型,通信方式:窄带载波,频率范围/中心频率:421kHz,调制方式:BFSK","只","32","2017-12-31","买方指定仓库地面交货"]
[null,"内蒙古东部电力有限公司","","集中器I型本地通信单元（窄带）","通信单元-通信单元类别:本地,适用终端/表类型:集中器I型,通信方式:窄带载波,频率范围/中心频率:其他,调制方式:其他","只","4935","2017-12-31","买方指定仓库地面交货"]
[null,"内蒙古东部电力有限公司","","集中器I型本地通信单元（窄带）","通信单元-通信单元类别:本地,适用终端/表类型:集中器I型,通信方式:窄带载波,频率范围/中心频率:421kHz,调制方式:BFSK","只","50","2017-12-31","买方指定仓库地面交货"]
[null,"内蒙古东部电力有限公司","","集中器I型本地通信单元（窄带）","通信单元-通信单元类别:本地,适用终端/表类型:集中器I型,通信方式:窄带载波,频率范围/中心频率:421kHz,调制方式:BFSK","只","417","2017-12-31","买方指定仓库地面交货"]
[null,"内蒙古东部电力有限公司","","集中器I型本地通信单元（窄带）","通信单元-通信单元类别:本地,适用终端/表类型:集中器I型,通信方式:窄带载波,频率范围/中心频率:270kHz,调制方式:BFSK","只","10","2017-12-31","买方指定仓库地面交货"]
[null,"内蒙古东部电力有限公司","","集中器I型本地通信单元（窄带）","通信单元-通信单元类别:本地,适用终端/表类型:集中器I型,通信方式:窄带载波,频率范围/中心频率:421kHz,调制方式:BFSK","只","50","2017-12-31","买方指定仓库地面交货"]
[null,"内蒙古东部电力有限公司","","集中器I型本地通信单元（窄带）","通信单元-通信单元类别:本地,适用终端/表类型:集中器I型,通信方式:窄带载波,频率范围/中心频率:其他,调制方式:其他","只","517","2017-12-31","买方指定仓库地面交货"]
[null,"内蒙古东部电力有限公司","","集中器I型本地通信单元（窄带）","通信单元-通信单元类别:本地,适用终端/表类型:集中器I型,通信方式:窄带载波,频率范围/中心频率:300kHz,调制方式:BPSK","只","945","2017-12-31","买方指定仓库地面交货"]
[null,"内蒙古东部电力有限公司","","集中器I型本地通信单元（窄带）","通信单元-通信单元类别:本地,适用终端/表类型:集中器I型,通信方式:窄带载波,频率范围/中心频率:其他,调制方式:其他","只","153","2017-12-31","买方指定仓库地面交货"]
[null,"内蒙古东部电力有限公司","","集中器I型本地通信单元（窄带）","通信单元-通信单元类别:本地,适用终端/表类型:集中器I型,通信方式:窄带载波,频率范围/中心频率:421kHz,调制方式:BFSK","只","347","2017-12-31","买方指定仓库地面交货"]
[null,"内蒙古东部电力有限公司","","集中器I型本地通信单元（窄带）","通信单元-通信单元类别:本地,适用终端/表类型:集中器I型,通信方式:窄带载波,频率范围/中心频率:421kHz,调制方式:BFSK","只","150","2017-12-31","买方指定仓库地面交货"]
[null,"内蒙古东部电力有限公司","","集中器I型本地通信单元（窄带）","通信单元-通信单元类别:本地,适用终端/表类型:集中器I型,通信方式:窄带载波,频率范围/中心频率:其他,调制方式:其他","只","47","2017-12-31","买方指定仓库地面交货"]
[null,"内蒙古东部电力有限公司","","集中器I型本地通信单元（窄带）","通信单元-通信单元类别:本地,适用终端/表类型:集中器I型,通信方式:窄带载波,频率范围/中心频率:270kHz,调制方式:BFSK","只","45","2017-12-31","买方指定仓库地面交货"]
[null,"内蒙古东部电力有限公司","","集中器I型本地通信单元（窄带）","通信单元-通信单元类别:本地,适用终端/表类型:集中器I型,通信方式:窄带载波,频率范围/中心频率:270kHz,调制方式:BFSK","只","4","2017-12-31","买方指定仓库地面交货"]
[null,"内蒙古东部电力有限公司","","集中器I型本地通信单元（窄带）","通信单元-通信单元类别:本地,适用终端/表类型:集中器I型,通信方式:窄带载波,频率范围/中心频率:421kHz,调制方式:BFSK","只","100","2017-12-31","买方指定仓库地面交货"]
[null,"内蒙古东部电力有限公司","","集中器I型本地通信单元（窄带）","通信单元-通信单元类别:本地,适用终端/表类型:集中器I型,通信方式:窄带载波,频率范围/中心频率:421kHz,调制方式:BFSK","只","328","2017-12-31","买方指定仓库地面交货"]
[null,"内蒙古东部电力有限公司","","集中器I型本地通信单元（窄带）","通信单元-通信单元类别:本地,适用终端/表类型:集中器I型,通信方式:窄带载波,频率范围/中心频率:421kHz,调制方式:BFSK","只","100","2017-12-31","买方指定仓库地面交货"]
[null,"内蒙古东部电力有限公司","","集中器I型本地通信单元（窄带）","通信单元-通信单元类别:本地,适用终端/表类型:集中器I型,通信方式:窄带载波,频率范围/中心频率:270kHz,调制方式:BFSK","只","50","2017-12-31","买方指定仓库地面交货"]
[null,"内蒙古东部电力有限公司","","集中器I型本地通信单元（窄带）","通信单元-通信单元类别:本地,适用终端/表类型:集中器I型,通信方式:窄带载波,频率范围/中心频率:421kHz,调制方式:BFSK","只","397","2017-12-31","买方指定仓库地面交货"]
[null,"内蒙古东部电力有限公司","","集中器I型远程通信单元（4G）","通信单元-通信单元类别:远程,适用终端/表类型:集中器I型,通信方式:无线公网4G,频率范围/中心频率:无,调制方式:无","只","32","2017-12-31","买方指定仓库地面交货"]
[null,"内蒙古东部电力有限公司","","集中器I型远程通信单元（4G）","通信单元-通信单元类别:远程,适用终端/表类型:集中器I型,通信方式:无线公网4G,频率范围/中心频率:无,调制方式:无","只","29","2017-12-31","买方指定仓库地面交货"]
[null,"内蒙古东部电力有限公司","","集中器I型远程通信单元（4G）","通信单元-通信单元类别:远程,适用终端/表类型:集中器I型,通信方式:无线公网4G,频率范围/中心频率:无,调制方式:无","只","100","2017-12-31","买方指定仓库地面交货"]
[null,"内蒙古东部电力有限公司","","集中器I型远程通信单元（4G）","通信单元-通信单元类别:远程,适用终端/表类型:集中器I型,通信方式:无线公网4G,频率范围/中心频率:无,调制方式:无","只","50","2017-12-31","买方指定仓库地面交货"]
[null,"内蒙古东部电力有限公司","","集中器I型远程通信单元（4G）","通信单元-通信单元类别:远程,适用终端/表类型:集中器I型,通信方式:无线公网4G,频率范围/中心频率:无,调制方式:无","只","32","2017-12-31","买方指定仓库地面交货"]
[null,"内蒙古东部电力有限公司","","集中器I型远程通信单元（4G）","通信单元-通信单元类别:远程,适用终端/表类型:集中器I型,通信方式:无线公网4G,频率范围/中心频率:无,调制方式:无","只","200","2017-12-31","买方指定仓库地面交货"]
[null,"内蒙古东部电力有限公司","","集中器I型远程通信单元（4G）","通信单元-通信单元类别:远程,适用终端/表类型:集中器I型,通信方式:无线公网4G,频率范围/中心频率:无,调制方式:无","只","4883","2017-12-31","买方指定仓库地面交货"]
[null,"内蒙古东部电力有限公司","","集中器I型远程通信单元（4G）","通信单元-通信单元类别:远程,适用终端/表类型:集中器I型,通信方式:无线公网4G,频率范围/中心频率:无,调制方式:无","只","1791","2017-12-31","买方指定仓库地面交货"]
[null,"内蒙古东部电力有限公司","","集中器I型远程通信单元（4G）","通信单元-通信单元类别:远程,适用终端/表类型:集中器I型,通信方式:无线公网4G,频率范围/中心频率:无,调制方式:无","只","2232","2017-12-31","买方指定仓库地面交货"]
[null,"内蒙古东部电力有限公司","","集中器I型远程通信单元（4G）","通信单元-通信单元类别:远程,适用终端/表类型:集中器I型,通信方式:无线公网4G,频率范围/中心频率:无,调制方式:无","只","244","2017-12-31","买方指定仓库地面交货"]
[null,"内蒙古东部电力有限公司","","集中器I型远程通信单元（4G）","通信单元-通信单元类别:远程,适用终端/表类型:集中器I型,通信方式:无线公网4G,频率范围/中心频率:无,调制方式:无","只","347","2017-12-31","买方指定仓库地面交货"]
[null,"内蒙古东部电力有限公司","","集中器I型远程通信单元（4G）","通信单元-通信单元类别:远程,适用终端/表类型:集中器I型,通信方式:无线公网4G,频率范围/中心频率:无,调制方式:无","只","209","2017-12-31","买方指定仓库地面交货"]
[null,"内蒙古东部电力有限公司","","集中器I型远程通信单元（4G）","通信单元-通信单元类别:远程,适用终端/表类型:集中器I型,通信方式:无线公网4G,频率范围/中心频率:无,调制方式:无","只","45","2017-12-31","买方指定仓库地面交货"]
[null,"内蒙古东部电力有限公司","","集中器I型远程通信单元（4G）","通信单元-通信单元类别:远程,适用终端/表类型:集中器I型,通信方式:无线公网4G,频率范围/中心频率:无,调制方式:无","只","50","2017-12-31","买方指定仓库地面交货"]
[null,"内蒙古东部电力有限公司","","集中器I型远程通信单元（4G）","通信单元-通信单元类别:远程,适用终端/表类型:集中器I型,通信方式:无线公网4G,频率范围/中心频率:无,调制方式:无","只","328","2017-12-31","买方指定仓库地面交货"]
[null,"内蒙古东部电力有限公司","","集中器I型远程通信单元（4G）","通信单元-通信单元类别:远程,适用终端/表类型:集中器I型,通信方式:无线公网4G,频率范围/中心频率:无,调制方式:无","只","300","2017-12-31","买方指定仓库地面交货"]
[null,"内蒙古东部电力有限公司","","集中器I型远程通信单元（4G）","通信单元-通信单元类别:远程,适用终端/表类型:集中器I型,通信方式:无线公网4G,频率范围/中心频率:无,调制方式:无","只","487","2017-12-31","买方指定仓库地面交货"]
[null,"内蒙古东部电力有限公司","","集中器I型远程通信单元（4G）","通信单元-通信单元类别:远程,适用终端/表类型:集中器I型,通信方式:无线公网4G,频率范围/中心频率:无,调制方式:无","只","551","2017-12-31","买方指定仓库地面交货"]
[null,"辽宁省电力有限公司","","集中器I型（无线公网4G/窄带载波）","集中器-设备类别:I型,远程通信:4G,本地通信:电力线窄带载波,交采功能:有,温度等级:C3","台","4480","2017-08-25","买方指定仓库地面交货"]
[null,"辽宁省电力有限公司","","集中器I型本地通信单元（窄带）","通信单元-通信单元类别:本地,适用终端/表类型:集中器I型,通信方式:窄带载波,频率范围/中心频率:270kHz,调制方式:BFSK","只","4480","2017-08-25","买方指定仓库地面交货"]
["包J14GW3","陕西省电力公司","","集中器I型（无线公网4G/窄带载波）","集中器-设备类别:I型,远程通信:4G,本地通信:电力线窄带载波,交采功能:有,温度等级:C3","台","2960","2018-06-30","买方指定仓库地面交货"]
[null,"重庆市电力公司","国网重庆公司2017年营销类物资协议库存招标采购","采集器II型本地通信单元（窄带）","通信单元-通信单元类别:本地,适用终端/表类型:采集器II型,通信方式:窄带载波,频率范围/中心频率:其他,调制方式:其他","只","8000","2018-06-16","买方指定仓库地面交货"]
[null,"陕西省电力公司","","集中器I型本地通信单元（宽带）","通信单元-通信单元类别:本地,适用终端/表类型:集中器I型,通信方式:宽带载波,频率范围/中心频率:2～12MHz,调制方式:OFDM","只","63","2018-06-30","买方指定仓库地面交货"]
[null,"陕西省电力公司","","集中器I型本地通信单元（窄带）","通信单元-通信单元类别:本地,适用终端/表类型:集中器I型,通信方式:窄带载波,频率范围/中心频率:132kHz,调制方式:BPSK","只","620","2018-06-30","买方指定仓库地面交货"]
[null,"陕西省电力公司","","集中器I型本地通信单元（窄带）","通信单元-通信单元类别:本地,适用终端/表类型:集中器I型,通信方式:窄带载波,频率范围/中心频率:270kHz,调制方式:BFSK","只","455","2018-06-30","买方指定仓库地面交货"]
[null,"陕西省电力公司","","集中器I型本地通信单元（窄带）","通信单元-通信单元类别:本地,适用终端/表类型:集中器I型,通信方式:窄带载波,频率范围/中心频率:421kHz,调制方式:BFSK","只","1600","2018-06-30","买方指定仓库地面交货"]
[null,"陕西省电力公司","","集中器I型本地通信单元（窄带）","通信单元-通信单元类别:本地,适用终端/表类型:集中器I型,通信方式:窄带载波,频率范围/中心频率:其他,调制方式:其他","只","220","2018-06-30","买方指定仓库地面交货"]
[null,"重庆市电力公司","国网重庆公司2017年营销类物资协议库存招标采购","集中器I型（无线公网4G/窄带载波）","集中器-设备类别:I型,远程通信:4G,本地通信:电力线窄带载波,交采功能:有,温度等级:C3","台","21000","2018-06-16","买方指定仓库地面交货"]
[null,"重庆市电力公司","国网重庆公司2017年营销类物资协议库存招标采购","集中器I型本地通信单元（窄带）","通信单元-通信单元类别:本地,适用终端/表类型:集中器I型,通信方式:窄带载波,频率范围/中心频率:270kHz,调制方式:BFSK","只","2000","2018-06-16","买方指定仓库地面交货"]
[null,"重庆市电力公司","国网重庆公司2017年营销类物资协议库存招标采购","集中器I型本地通信单元（窄带）","通信单元-通信单元类别:本地,适用终端/表类型:集中器I型,通信方式:窄带载波,频率范围/中心频率:其他,调制方式:其他","只","5000","2018-06-16","买方指定仓库地面交货"]
[null,"重庆市电力公司","国网重庆公司2017年营销类物资协议库存招标采购","集中器I型本地通信单元（窄带）","通信单元-通信单元类别:本地,适用终端/表类型:集中器I型,通信方式:窄带载波,频率范围/中心频率:421kHz,调制方式:BFSK","只","14000","2018-06-16","买方指定仓库地面交货"]
[null,"重庆市电力公司","国网重庆公司2017年营销类物资协议库存招标采购","集中器I型远程通信单元（4G）","通信单元-通信单元类别:远程,适用终端/表类型:集中器I型,通信方式:无线公网4G,频率范围/中心频率:无,调制方式:无","只","21000","2018-06-16","买方指定仓库地面交货"]
[null,"重庆市电力公司","国网重庆公司2017年营销类物资协议库存招标采购","采集器I型本地通信单元（窄带）","通信单元-通信单元类别:本地,适用终端/表类型:采集器I型,通信方式:窄带载波,频率范围/中心频率:421kHz,调制方式:BFSK","只","2000","2018-06-16","买方指定仓库地面交货"]
[null,"重庆市电力公司","国网重庆公司2017年营销类物资协议库存招标采购","采集器I型（窄带载波）","采集器-设备类别:I型,采集器与集中器通信方式:电力线窄带载波,交采功能:无,温度等级:C3","台","2000","2018-06-16","买方指定仓库地面交货"]
[null,"重庆市电力公司","国网重庆公司2017年营销类物资协议库存招标采购","采集器II型（窄带载波）","采集器-设备类别:II型,采集器与集中器通信方式:电力线窄带载波,交采功能:无,温度等级:C3","台","20000","2018-06-16","买方指定仓库地面交货"]
[null,"重庆市电力公司","国网重庆公司2017年营销类物资协议库存招标采购","采集器II型本地通信单元（窄带）","通信单元-通信单元类别:本地,适用终端/表类型:采集器II型,通信方式:窄带载波,频率范围/中心频率:421kHz,调制方式:BFSK","只","8000","2018-06-16","买方指定仓库地面交货"]
[null,"重庆市电力公司","国网重庆公司2017年营销类物资协议库存招标采购","采集器II型本地通信单元（窄带）","通信单元-通信单元类别:本地,适用终端/表类型:采集器II型,通信方式:窄带载波,频率范围/中心频率:270kHz,调制方式:BFSK","只","4000","2018-06-16","买方指定仓库地面交货"]
[null,"陕西省电力公司","","集中器I型远程通信单元（4G）","通信单元-通信单元类别:远程,适用终端/表类型:集中器I型,通信方式:无线公网4G,频率范围/中心频率:无,调制方式:无","只","3943","2018-06-30","买方指定仓库地面交货"]
["包J14GW4","西藏电力有限公司","国网西藏电力有限公司各供电公司营销专项、电网基建/户表","集中器I型（无线公网CDMA/窄带载波）","集中器-设备类别:I型,远程通信:CDMA,本地通信:电力线窄带载波,交采功能:有,温度等级:C3","台","1268","2017-06-30","买方指定仓库地面交货"]
[null,"江苏省电力公司","","集中器I型（无线公网4G/窄带载波）","集中器-设备类别:I型,远程通信:4G,本地通信:电力线窄带载波,交采功能:有,温度等级:C3","台","1800","2018-04-15","买方指定仓库地面交货"]
[null,"江苏省电力公司","","集中器I型（无线公网4G/窄带载波）","集中器-设备类别:I型,远程通信:4G,本地通信:电力线窄带载波,交采功能:有,温度等级:C3","台","3000","2018-04-15","买方指定仓库地面交货"]
[null,"江苏省电力公司","","集中器I型（无线公网4G/窄带载波）","集中器-设备类别:I型,远程通信:4G,本地通信:电力线窄带载波,交采功能:有,温度等级:C3","台","2200","2018-04-15","买方指定仓库地面交货"]
[null,"江苏省电力公司","","集中器I型（无线公网4G/窄带载波）","集中器-设备类别:I型,远程通信:4G,本地通信:电力线窄带载波,交采功能:有,温度等级:C3","台","4000","2018-04-15","买方指定仓库地面交货"]
[null,"江苏省电力公司","","集中器I型本地通信单元（窄带）","通信单元-通信单元类别:本地,适用终端/表类型:集中器I型,通信方式:窄带载波,频率范围/中心频率:421kHz,调制方式:BFSK","只","3300","2018-04-15","买方指定仓库地面交货"]
[null,"江苏省电力公司","","集中器I型本地通信单元（窄带）","通信单元-通信单元类别:本地,适用终端/表类型:集中器I型,通信方式:窄带载波,频率范围/中心频率:421kHz,调制方式:BFSK","只","2420","2018-04-15","买方指定仓库地面交货"]
[null,"江苏省电力公司","","集中器I型本地通信单元（窄带）","通信单元-通信单元类别:本地,适用终端/表类型:集中器I型,通信方式:窄带载波,频率范围/中心频率:421kHz,调制方式:BFSK","只","1980","2018-04-15","买方指定仓库地面交货"]
[null,"江苏省电力公司","","集中器I型远程通信单元（4G）","通信单元-通信单元类别:远程,适用终端/表类型:集中器I型,通信方式:无线公网4G,频率范围/中心频率:无,调制方式:无","只","1980","2018-04-15","买方指定仓库地面交货"]
[null,"江苏省电力公司","","集中器I型远程通信单元（4G）","通信单元-通信单元类别:远程,适用终端/表类型:集中器I型,通信方式:无线公网4G,频率范围/中心频率:无,调制方式:无","只","3300","2018-04-15","买方指定仓库地面交货"]
[null,"江苏省电力公司","","集中器I型远程通信单元（4G）","通信单元-通信单元类别:远程,适用终端/表类型:集中器I型,通信方式:无线公网4G,频率范围/中心频率:无,调制方式:无","只","2420","2018-04-15","买方指定仓库地面交货"]
[null,"江苏省电力公司","","集中器I型远程通信单元（4G）","通信单元-通信单元类别:远程,适用终端/表类型:集中器I型,通信方式:无线公网4G,频率范围/中心频率:无,调制方式:无","只","4400","2018-04-15","买方指定仓库地面交货"]
[null,"江苏省电力公司","","采集器II型（窄带载波）","采集器-设备类别:II型,采集器与集中器通信方式:电力线窄带载波,交采功能:无,温度等级:C3","台","60000","2018-04-15","买方指定仓库地面交货"]
[null,"江苏省电力公司","","采集器II型（窄带载波）","采集器-设备类别:II型,采集器与集中器通信方式:电力线窄带载波,交采功能:无,温度等级:C3","台","55000","2018-04-15","买方指定仓库地面交货"]
[null,"江苏省电力公司","","采集器II型（窄带载波）","采集器-设备类别:II型,采集器与集中器通信方式:电力线窄带载波,交采功能:无,温度等级:C3","台","45000","2018-04-15","买方指定仓库地面交货"]
[null,"江苏省电力公司","","采集器II型（窄带载波）","采集器-设备类别:II型,采集器与集中器通信方式:电力线窄带载波,交采功能:无,温度等级:C3","台","40000","2018-04-15","买方指定仓库地面交货"]
[null,"江苏省电力公司","","采集器II型（窄带载波）","采集器-设备类别:II型,采集器与集中器通信方式:电力线窄带载波,交采功能:无,温度等级:C3","台","30000","2018-04-15","买方指定仓库地面交货"]
[null,"江苏省电力公司","","采集器II型本地通信单元（窄带）","通信单元-通信单元类别:本地,适用终端/表类型:采集器II型,通信方式:窄带载波,频率范围/中心频率:421kHz,调制方式:BFSK","只","60000","2018-04-15","买方指定仓库地面交货"]
[null,"江苏省电力公司","","采集器II型本地通信单元（窄带）","通信单元-通信单元类别:本地,适用终端/表类型:采集器II型,通信方式:窄带载波,频率范围/中心频率:421kHz,调制方式:BFSK","只","45000","2018-04-15","买方指定仓库地面交货"]
[null,"江苏省电力公司","","采集器II型本地通信单元（窄带）","通信单元-通信单元类别:本地,适用终端/表类型:采集器II型,通信方式:窄带载波,频率范围/中心频率:421kHz,调制方式:BFSK","只","55000","2018-04-15","买方指定仓库地面交货"]
[null,"江苏省电力公司","","采集器II型本地通信单元（窄带）","通信单元-通信单元类别:本地,适用终端/表类型:采集器II型,通信方式:窄带载波,频率范围/中心频率:其他,调制方式:其他","只","40000","2018-04-15","买方指定仓库地面交货"]
[null,"江苏省电力公司","","采集器II型本地通信单元（窄带）","通信单元-通信单元类别:本地,适用终端/表类型:采集器II型,通信方式:窄带载波,频率范围/中心频率:其他,调制方式:其他","只","30000","2018-04-15","买方指定仓库地面交货"]
[null,"江苏省电力公司","","集中器I型本地通信单元（窄带）","通信单元-通信单元类别:本地,适用终端/表类型:集中器I型,通信方式:窄带载波,频率范围/中心频率:其他,调制方式:其他","只","4400","2018-04-15","买方指定仓库地面交货"]
[null,"西藏电力有限公司","国网西藏电力有限公司各供电公司营销专项、电网基建/户表","采集器II型（窄带载波）","采集器-设备类别:II型,采集器与集中器通信方式:电力线窄带载波,交采功能:无,温度等级:C3","台","711","2017-06-30","买方指定仓库地面交货"]
[null,"西藏电力有限公司","国网西藏电力有限公司各供电公司营销专项、电网基建/户表","集中器I型本地通信单元（窄带）","通信单元-通信单元类别:本地,适用终端/表类型:集中器I型,通信方式:窄带载波,频率范围/中心频率:421kHz,调制方式:BFSK","只","1278","2017-07-30","买方指定仓库地面交货"]
[null,"西藏电力有限公司","国网西藏电力有限公司各供电公司营销专项、电网基建/户表","集中器I型远程通信单元（CDMA）","通信单元-通信单元类别:远程,适用终端/表类型:集中器I型,通信方式:无线公网CDMA,频率范围/中心频率:无,调制方式:无","只","1268","2017-07-30","买方指定仓库地面交货"]
[null,"西藏电力有限公司","国网西藏电力有限公司各供电公司营销专项、电网基建/户表","采集器II型本地通信单元（窄带）","通信单元-通信单元类别:本地,适用终端/表类型:采集器II型,通信方式:窄带载波,频率范围/中心频率:421kHz,调制方式:BFSK","只","711","2017-06-30","买方指定仓库地面交货"]
[null,"西藏电力有限公司","国网西藏电力有限公司各供电公司营销专项、电网基建/户表","采集器I型本地通信单元（窄带）","通信单元-通信单元类别:本地,适用终端/表类型:采集器I型,通信方式:窄带载波,频率范围/中心频率:421kHz,调制方式:BFSK","只","556","2017-07-30","买方指定仓库地面交货"]
["包J14GW5","江西省电力公司","","集中器I型（无线公网GPRS/窄带载波）","集中器-设备类别:I型,远程通信:GPRS,本地通信:电力线窄带载波,交采功能:有,温度等级:C3","台","12000","2017-09-15","买方指定仓库地面交货"]
[null,"江苏省电力公司","","集中器I型本地通信单元（窄带）","通信单元-通信单元类别:本地,适用终端/表类型:集中器I型,通信方式:窄带载波,频率范围/中心频率:132kHz,调制方式:BPSK","只","495","2018-04-15","买方指定仓库地面交货"]
[null,"江苏省电力公司","","集中器I型本地通信单元（窄带）","通信单元-通信单元类别:本地,适用终端/表类型:集中器I型,通信方式:窄带载波,频率范围/中心频率:其他,调制方式:其他","只","4950","2018-04-15","买方指定仓库地面交货"]
[null,"江苏省电力公司","","集中器I型本地通信单元（窄带）","通信单元-通信单元类别:本地,适用终端/表类型:集中器I型,通信方式:窄带载波,频率范围/中心频率:270kHz,调制方式:BFSK","只","660","2018-04-15","买方指定仓库地面交货"]
[null,"江西省电力公司","","集中器I型（无线公网CDMA/窄带载波）","集中器-设备类别:I型,远程通信:CDMA,本地通信:电力线窄带载波,交采功能:有,温度等级:C3","台","3000","2017-09-15","买方指定仓库地面交货"]
[null,"江西省电力公司","","集中器I型本地通信单元（窄带）","通信单元-通信单元类别:本地,适用终端/表类型:集中器I型,通信方式:窄带载波,频率范围/中心频率:270kHz,调制方式:BFSK","只","7840","2017-09-15","买方指定仓库地面交货"]
[null,"江西省电力公司","","集中器I型本地通信单元（窄带）","通信单元-通信单元类别:本地,适用终端/表类型:集中器I型,通信方式:窄带载波,频率范围/中心频率:其他,调制方式:其他","只","5360","2017-09-15","买方指定仓库地面交货"]
[null,"江苏省电力公司","","集中器I型（无线公网4G/窄带载波）","集中器-设备类别:I型,远程通信:4G,本地通信:电力线窄带载波,交采功能:有,温度等级:C3","台","4500","2018-04-15","买方指定仓库地面交货"]
[null,"江苏省电力公司","","集中器I型（无线公网4G/窄带载波）","集中器-设备类别:I型,远程通信:4G,本地通信:电力线窄带载波,交采功能:有,温度等级:C3","台","600","2018-04-15","买方指定仓库地面交货"]
[null,"江苏省电力公司","","集中器I型（无线公网4G/窄带载波）","集中器-设备类别:I型,远程通信:4G,本地通信:电力线窄带载波,交采功能:有,温度等级:C3","台","450","2018-04-15","买方指定仓库地面交货"]
[null,"江苏省电力公司","","集中器I型远程通信单元（4G）","通信单元-通信单元类别:远程,适用终端/表类型:集中器I型,通信方式:无线公网4G,频率范围/中心频率:无,调制方式:无","只","660","2018-04-15","买方指定仓库地面交货"]
[null,"江苏省电力公司","","集中器I型远程通信单元（4G）","通信单元-通信单元类别:远程,适用终端/表类型:集中器I型,通信方式:无线公网4G,频率范围/中心频率:无,调制方式:无","只","495","2018-04-15","买方指定仓库地面交货"]
[null,"江苏省电力公司","","采集器II型（窄带载波）","采集器-设备类别:II型,采集器与集中器通信方式:电力线窄带载波,交采功能:无,温度等级:C3","台","50000","2018-04-15","买方指定仓库地面交货"]
[null,"江苏省电力公司","","采集器II型（窄带载波）","采集器-设备类别:II型,采集器与集中器通信方式:电力线窄带载波,交采功能:无,温度等级:C3","台","20000","2018-04-15","买方指定仓库地面交货"]
[null,"江苏省电力公司","","采集器II型（窄带载波）","采集器-设备类别:II型,采集器与集中器通信方式:电力线窄带载波,交采功能:无,温度等级:C3","台","10000","2018-04-15","买方指定仓库地面交货"]
[null,"江苏省电力公司","","采集器II型本地通信单元（窄带）","通信单元-通信单元类别:本地,适用终端/表类型:采集器II型,通信方式:窄带载波,频率范围/中心频率:132kHz,调制方式:BPSK","只","10000","2018-04-15","买方指定仓库地面交货"]
[null,"江苏省电力公司","","采集器II型本地通信单元（窄带）","通信单元-通信单元类别:本地,适用终端/表类型:采集器II型,通信方式:窄带载波,频率范围/中心频率:270kHz,调制方式:BFSK","只","20000","2018-04-15","买方指定仓库地面交货"]
[null,"江苏省电力公司","","采集器II型本地通信单元（窄带）","通信单元-通信单元类别:本地,适用终端/表类型:采集器II型,通信方式:窄带载波,频率范围/中心频率:其他,调制方式:其他","只","50000","2018-04-15","买方指定仓库地面交货"]
[null,"江西省电力公司","","集中器I型本地通信单元（窄带）","通信单元-通信单元类别:本地,适用终端/表类型:集中器I型,通信方式:窄带载波,频率范围/中心频率:421kHz,调制方式:BFSK","只","1800","2017-09-15","买方指定仓库地面交货"]
[null,"江西省电力公司","","集中器I型远程通信单元（GPRS）","通信单元-通信单元类别:远程,适用终端/表类型:集中器I型,通信方式:无线公网GPRS,频率范围/中心频率:无,调制方式:无","只","12000","2017-09-15","买方指定仓库地面交货"]
[null,"江西省电力公司","","集中器I型远程通信单元（CDMA）","通信单元-通信单元类别:远程,适用终端/表类型:集中器I型,通信方式:无线公网CDMA,频率范围/中心频率:无,调制方式:无","只","3000","2017-09-15","买方指定仓库地面交货"]
[null,"江苏省电力公司","","集中器I型远程通信单元（4G）","通信单元-通信单元类别:远程,适用终端/表类型:集中器I型,通信方式:无线公网4G,频率范围/中心频率:无,调制方式:无","只","4950","2018-04-15","买方指定仓库地面交货"]
["包J14HA1","河南省电力公司","","集中器I型远程通信单元（4G）","通信单元-通信单元类别:远程,适用终端/表类型:集中器I型,通信方式:无线公网4G,频率范围/中心频率:无,调制方式:无","只","24750","2018-04-10","买方指定仓库地面交货"]
[null,"河南省电力公司","","集中器I型本地通信单元（窄带）","通信单元-通信单元类别:本地,适用终端/表类型:集中器I型,通信方式:窄带载波,频率范围/中心频率:421kHz,调制方式:BFSK","只","17292","2018-04-10","买方指定仓库地面交货"]
[null,"河南省电力公司","","集中器I型本地通信单元（窄带）","通信单元-通信单元类别:本地,适用终端/表类型:集中器I型,通信方式:窄带载波,频率范围/中心频率:270kHz,调制方式:BFSK","只","2343","2018-04-10","买方指定仓库地面交货"]
[null,"河南省电力公司","","集中器I型（无线公网4G/窄带载波）","集中器-设备类别:I型,远程通信:4G,本地通信:电力线窄带载波,交采功能:有,温度等级:C3","台","22500","2018-04-10","买方指定仓库地面交货"]
[null,"河南省电力公司","","集中器I型本地通信单元（窄带）","通信单元-通信单元类别:本地,适用终端/表类型:集中器I型,通信方式:窄带载波,频率范围/中心频率:132kHz,调制方式:BPSK","只","5115","2018-04-10","买方指定仓库地面交货"]
["包J14HA2","河南省电力公司","","集中器I型本地通信单元（窄带）","通信单元-通信单元类别:本地,适用终端/表类型:集中器I型,通信方式:窄带载波,频率范围/中心频率:132kHz,调制方式:BPSK","只","6105","2018-04-10","买方指定仓库地面交货"]
[null,"河南省电力公司","","集中器I型远程通信单元（4G）","通信单元-通信单元类别:远程,适用终端/表类型:集中器I型,通信方式:无线公网4G,频率范围/中心频率:无,调制方式:无","只","22000","2018-04-10","买方指定仓库地面交货"]
[null,"河南省电力公司","","集中器I型本地通信单元（窄带）","通信单元-通信单元类别:本地,适用终端/表类型:集中器I型,通信方式:窄带载波,频率范围/中心频率:其他,调制方式:其他","只","15895","2018-04-10","买方指定仓库地面交货"]
[null,"河南省电力公司","","集中器I型（无线公网4G/窄带载波）","集中器-设备类别:I型,远程通信:4G,本地通信:电力线窄带载波,交采功能:有,温度等级:C3","台","20000","2018-04-10","买方指定仓库地面交货"]
["包J14HE1","河北省电力公司","","集中器I型远程通信单元（4G）","通信单元-通信单元类别:远程,适用终端/表类型:集中器I型,通信方式:无线公网4G,频率范围/中心频率:无,调制方式:无","只","32000","2018-03-31","买方指定仓库地面交货"]
[null,"河北省电力公司","","集中器I型本地通信单元（窄带）","通信单元-通信单元类别:本地,适用终端/表类型:集中器I型,通信方式:窄带载波,频率范围/中心频率:300kHz,调制方式:BPSK","只","22000","2018-03-31","买方指定仓库地面交货"]
[null,"河北省电力公司","","集中器I型本地通信单元（窄带）","通信单元-通信单元类别:本地,适用终端/表类型:集中器I型,通信方式:窄带载波,频率范围/中心频率:132kHz,调制方式:BPSK","只","10000","2018-03-31","买方指定仓库地面交货"]
[null,"河北省电力公司","","集中器I型（无线公网4G/窄带载波）","集中器-设备类别:I型,远程通信:4G,本地通信:电力线窄带载波,交采功能:有,温度等级:C3","台","32000","2018-03-31","买方指定仓库地面交货"]
["包J14HE2","河北省电力公司","","集中器I型本地通信单元（窄带）","通信单元-通信单元类别:本地,适用终端/表类型:集中器I型,通信方式:窄带载波,频率范围/中心频率:300kHz,调制方式:QPSK","只","5500","2018-03-31","买方指定仓库地面交货"]
[null,"河北省电力公司","","集中器I型本地通信单元（窄带）","通信单元-通信单元类别:本地,适用终端/表类型:集中器I型,通信方式:窄带载波,频率范围/中心频率:270kHz,调制方式:BFSK","只","7300","2018-03-31","买方指定仓库地面交货"]
[null,"河北省电力公司","","集中器I型本地通信单元（窄带）","通信单元-通信单元类别:本地,适用终端/表类型:集中器I型,通信方式:窄带载波,频率范围/中心频率:421kHz,调制方式:BFSK","只","1000","2018-03-31","买方指定仓库地面交货"]
[null,"河北省电力公司","","集中器I型本地通信单元（窄带）","通信单元-通信单元类别:本地,适用终端/表类型:集中器I型,通信方式:窄带载波,频率范围/中心频率:421kHz,调制方式:BFSK","只","3200","2018-03-31","买方指定仓库地面交货"]
[null,"河北省电力公司","","集中器I型本地通信单元（窄带）","通信单元-通信单元类别:本地,适用终端/表类型:集中器I型,通信方式:窄带载波,频率范围/中心频率:421kHz,调制方式:BFSK","只","6000","2018-03-31","买方指定仓库地面交货"]
[null,"河北省电力公司","","集中器I型远程通信单元（4G）","通信单元-通信单元类别:远程,适用终端/表类型:集中器I型,通信方式:无线公网4G,频率范围/中心频率:无,调制方式:无","只","32000","2018-03-31","买方指定仓库地面交货"]
[null,"河北省电力公司","","集中器I型本地通信单元（窄带）","通信单元-通信单元类别:本地,适用终端/表类型:集中器I型,通信方式:窄带载波,频率范围/中心频率:132kHz,调制方式:BPSK","只","9000","2018-03-31","买方指定仓库地面交货"]
[null,"河北省电力公司","","集中器I型（无线公网4G/窄带载波）","集中器-设备类别:I型,远程通信:4G,本地通信:电力线窄带载波,交采功能:有,温度等级:C3","台","32000","2018-03-31","买方指定仓库地面交货"]
["包J14JX1","江西省电力公司","","集中器I型（无线公网4G/窄带载波）","集中器-设备类别:I型,远程通信:4G,本地通信:电力线窄带载波,交采功能:有,温度等级:C3","台","20000","2017-09-15","买方指定仓库地面交货"]
[null,"江西省电力公司","","集中器I型本地通信单元（窄带）","通信单元-通信单元类别:本地,适用终端/表类型:集中器I型,通信方式:窄带载波,频率范围/中心频率:270kHz,调制方式:BFSK","只","16000","2017-09-15","买方指定仓库地面交货"]
[null,"江西省电力公司","","集中器I型本地通信单元（窄带）","通信单元-通信单元类别:本地,适用终端/表类型:集中器I型,通信方式:窄带载波,频率范围/中心频率:132kHz,调制方式:BPSK","只","500","2017-09-15","买方指定仓库地面交货"]
[null,"江西省电力公司","","集中器I型本地通信单元（窄带）","通信单元-通信单元类别:本地,适用终端/表类型:集中器I型,通信方式:窄带载波,频率范围/中心频率:其他,调制方式:其他","只","3000","2017-09-15","买方指定仓库地面交货"]
[null,"江西省电力公司","","集中器I型远程通信单元（4G）","通信单元-通信单元类别:远程,适用终端/表类型:集中器I型,通信方式:无线公网4G,频率范围/中心频率:无,调制方式:无","只","20000","2017-09-15","买方指定仓库地面交货"]
[null,"江西省电力公司","","集中器I型本地通信单元（窄带）","通信单元-通信单元类别:本地,适用终端/表类型:集中器I型,通信方式:窄带载波,频率范围/中心频率:421kHz,调制方式:BFSK","只","500","2017-09-15","买方指定仓库地面交货"]
["包J15GW1","河北省电力公司","","集中器I型本地通信单元（微功率）","通信单元-通信单元类别:本地,适用终端/表类型:集中器I型,通信方式:微功率,频率范围/中心频率:470～510MHz,调制方式:GFSK","只","6000","2018-03-31","买方指定仓库地面交货"]
[null,"北京市电力公司","北京协议库存","1级三相表远程通信单元（4G）","通信单元-通信单元类别:远程,适用终端/表类型:1级三相表,通信方式:无线公网4G,频率范围/中心频率:无,调制方式:无","只","7000","2018-04-14","买方指定仓库地面交货"]
[null,"河南省电力公司","","集中器I型（无线公网4G/微功率无线）","集中器-设备类别:I型,远程通信:4G,本地通信:微功率无线,交采功能:有,温度等级:C3","台","7500","2018-04-10","买方指定仓库地面交货"]
[null,"西藏电力有限公司","国网西藏电力有限公司各供电公司营销专项、电网基建/户表","集中器I型（无线公网CDMA/微功率无线）","集中器-设备类别:I型,远程通信:CDMA,本地通信:微功率无线,交采功能:有,温度等级:C3","台","290","2017-06-30","买方指定仓库地面交货"]
[null,"河北省电力公司","","集中器I型本地通信单元（窄带）","通信单元-通信单元类别:本地,适用终端/表类型:集中器I型,通信方式:窄带载波,频率范围/中心频率:300kHz,调制方式:BPSK","只","8000","2018-03-31","买方指定仓库地面交货"]
[null,"西藏电力有限公司","国网西藏电力有限公司各供电公司营销专项、电网基建/户表","集中器I型本地通信单元（微功率）","通信单元-通信单元类别:本地,适用终端/表类型:集中器I型,通信方式:微功率,频率范围/中心频率:470～510MHz,调制方式:GFSK","只","290","2017-07-30","买方指定仓库地面交货"]
[null,"西藏电力有限公司","国网西藏电力有限公司各供电公司营销专项、电网基建/户表","采集器II型本地通信单元（微功率）","通信单元-通信单元类别:本地,适用终端/表类型:采集器II型,通信方式:微功率,频率范围/中心频率:470～510MHz,调制方式:GFSK","只","600","2017-07-30","买方指定仓库地面交货"]
[null,"江西省电力公司","","集中器I型（无线公网GPRS/微功率无线）","集中器-设备类别:I型,远程通信:GPRS,本地通信:微功率无线,交采功能:有,温度等级:C3","台","400","2017-09-15","买方指定仓库地面交货"]
[null,"江西省电力公司","","集中器I型远程通信单元（GPRS）","通信单元-通信单元类别:远程,适用终端/表类型:集中器I型,通信方式:无线公网GPRS,频率范围/中心频率:无,调制方式:无","只","400","2017-09-15","买方指定仓库地面交货"]
[null,"江西省电力公司","","集中器I型本地通信单元（微功率）","通信单元-通信单元类别:本地,适用终端/表类型:集中器I型,通信方式:微功率,频率范围/中心频率:470～510MHz,调制方式:GFSK","只","400","2017-09-15","买方指定仓库地面交货"]
[null,"河南省电力公司","","集中器I型本地通信单元（微功率）","通信单元-通信单元类别:本地,适用终端/表类型:集中器I型,通信方式:微功率,频率范围/中心频率:470～510MHz,调制方式:GFSK","只","8250","2018-04-10","买方指定仓库地面交货"]
[null,"陕西省电力公司","","集中器I型（无线公网4G/微功率无线）","集中器-设备类别:I型,远程通信:4G,本地通信:微功率无线,交采功能:有,温度等级:C3","台","983","2018-06-30","买方指定仓库地面交货"]
[null,"陕西省电力公司","","集中器I型本地通信单元（微功率）","通信单元-通信单元类别:本地,适用终端/表类型:集中器I型,通信方式:微功率,频率范围/中心频率:470～510MHz,调制方式:GFSK","只","985","2018-06-30","买方指定仓库地面交货"]
[null,"西藏电力有限公司","国网西藏电力有限公司各供电公司营销专项、电网基建/户表","采集器II型（微功率无线）","采集器-设备类别:II型,采集器与集中器通信方式:微功率无线,交采功能:无,温度等级:C3","台","600","2017-07-30","买方指定仓库地面交货"]
[null,"西藏电力有限公司","国网西藏电力有限公司各供电公司营销专项、电网基建/户表","采集器I型（窄带载波）","采集器-设备类别:I型,采集器与集中器通信方式:电力线窄带载波,交采功能:无,温度等级:C3","台","556","2017-07-30","买方指定仓库地面交货"]
[null,"西藏电力有限公司","国网西藏电力有限公司各供电公司营销专项、电网基建/户表","集中器I型远程通信单元（CDMA）","通信单元-通信单元类别:远程,适用终端/表类型:集中器I型,通信方式:无线公网CDMA,频率范围/中心频率:无,调制方式:无","只","290","2017-07-30","买方指定仓库地面交货"]
[null,"北京市电力公司","北京协议库存","2级单相表本地通信单元（微功率）","通信单元-通信单元类别:本地,适用终端/表类型:2级单相表,通信方式:微功率,频率范围/中心频率:470～510MHz,调制方式:GFSK","只","320000","2018-04-14","买方指定仓库地面交货"]
[null,"北京市电力公司","北京协议库存","1级三相表本地通信单元（微功率）","通信单元-通信单元类别:本地,适用终端/表类型:1级三相表,通信方式:微功率,频率范围/中心频率:470～510MHz,调制方式:GFSK","只","15000","2018-04-14","买方指定仓库地面交货"]
[null,"河北省电力公司","","集中器I型远程通信单元（4G）","通信单元-通信单元类别:远程,适用终端/表类型:集中器I型,通信方式:无线公网4G,频率范围/中心频率:无,调制方式:无","只","14000","2018-03-31","买方指定仓库地面交货"]
[null,"河南省电力公司","","集中器I型远程通信单元（4G）","通信单元-通信单元类别:远程,适用终端/表类型:集中器I型,通信方式:无线公网4G,频率范围/中心频率:无,调制方式:无","只","8250","2018-04-10","买方指定仓库地面交货"]
[null,"河北省电力公司","","集中器I型（无线公网4G/微功率无线）","集中器-设备类别:I型,远程通信:4G,本地通信:微功率无线,交采功能:有,温度等级:C3","台","14000","2018-03-31","买方指定仓库地面交货"]
["包J16GW1","江苏省电力公司","","采集器I型本地通信单元（宽带）","通信单元-通信单元类别:本地,适用终端/表类型:采集器I型,通信方式:宽带载波,频率范围/中心频率:2～12MHz,调制方式:OFDM","只","66000","2018-04-15","买方指定仓库地面交货"]
[null,"江苏省电力公司","","集中器I型（无线公网4G/宽带载波）","集中器-设备类别:I型,远程通信:4G,本地通信:电力线宽带载波,交采功能:有,温度等级:C3","台","9000","2018-04-15","买方指定仓库地面交货"]
[null,"江苏省电力公司","","集中器I型远程通信单元（4G）","通信单元-通信单元类别:远程,适用终端/表类型:集中器I型,通信方式:无线公网4G,频率范围/中心频率:无,调制方式:无","只","9900","2018-04-15","买方指定仓库地面交货"]
[null,"江苏省电力公司","","采集器I型（宽带载波）","采集器-设备类别:I型,采集器与集中器通信方式:电力线宽带载波,交采功能:无,温度等级:C3","台","60000","2018-04-15","买方指定仓库地面交货"]
[null,"江苏省电力公司","","采集器II型（宽带载波）","采集器-设备类别:II型,采集器与集中器通信方式:电力线宽带载波,交采功能:无,温度等级:C3","台","215000","2018-04-15","买方指定仓库地面交货"]
[null,"福建省电力有限公司","国网福建省电力有限公司采购","集中器I型本地通信单元（宽带）","通信单元-通信单元类别:本地,适用终端/表类型:集中器I型,通信方式:宽带载波,频率范围/中心频率:2～12MHz,调制方式:OFDM","只","4500","2018-06-30","买方指定仓库地面交货"]
[null,"江苏省电力公司","","集中器I型本地通信单元（宽带）","通信单元-通信单元类别:本地,适用终端/表类型:集中器I型,通信方式:宽带载波,频率范围/中心频率:2～12MHz,调制方式:OFDM","只","9900","2018-04-15","买方指定仓库地面交货"]
[null,"江苏省电力公司","","采集器II型本地通信单元（宽带）","通信单元-通信单元类别:本地,适用终端/表类型:采集器II型,通信方式:宽带载波,频率范围/中心频率:2～12MHz,调制方式:OFDM","只","70000","2018-04-15","买方指定仓库地面交货"]
[null,"江苏省电力公司","","采集器II型本地通信单元（宽带）","通信单元-通信单元类别:本地,适用终端/表类型:采集器II型,通信方式:宽带载波,频率范围/中心频率:2～12MHz,调制方式:OFDM","只","215000","2018-04-15","买方指定仓库地面交货"]
[null,"福建省电力有限公司","国网福建省电力有限公司采购","集中器I型远程通信单元（4G）","通信单元-通信单元类别:远程,适用终端/表类型:集中器I型,通信方式:无线公网4G,频率范围/中心频率:无,调制方式:无","只","4500","2018-06-30","买方指定仓库地面交货"]
[null,"福建省电力有限公司","国网福建省电力有限公司采购","集中器I型（无线公网4G/宽带载波）","集中器-设备类别:I型,远程通信:4G,本地通信:电力线宽带载波,交采功能:有,温度等级:C3","台","4500","2018-06-30","买方指定仓库地面交货"]
[null,"江苏省电力公司","","采集器II型（宽带载波）","采集器-设备类别:II型,采集器与集中器通信方式:电力线宽带载波,交采功能:无,温度等级:C3","台","70000","2018-04-15","买方指定仓库地面交货"]
["包J16GW2","江苏省电力公司","","集中器I型本地通信单元（宽带）","通信单元-通信单元类别:本地,适用终端/表类型:集中器I型,通信方式:宽带载波,频率范围/中心频率:2～12MHz,调制方式:OFDM","只","9350","2018-04-15","买方指定仓库地面交货"]
[null,"江苏省电力公司","","集中器I型（无线公网4G/宽带载波）","集中器-设备类别:I型,远程通信:4G,本地通信:电力线宽带载波,交采功能:有,温度等级:C3","台","8500","2018-04-15","买方指定仓库地面交货"]
[null,"江苏省电力公司","","集中器I型远程通信单元（4G）","通信单元-通信单元类别:远程,适用终端/表类型:集中器I型,通信方式:无线公网4G,频率范围/中心频率:无,调制方式:无","只","9350","2018-04-15","买方指定仓库地面交货"]
[null,"江苏省电力公司","","采集器I型（宽带载波）","采集器-设备类别:I型,采集器与集中器通信方式:电力线宽带载波,交采功能:无,温度等级:C3","台","35000","2018-04-15","买方指定仓库地面交货"]
[null,"江苏省电力公司","","采集器I型（宽带载波）","采集器-设备类别:I型,采集器与集中器通信方式:电力线宽带载波,交采功能:无,温度等级:C3","台","50000","2018-04-15","买方指定仓库地面交货"]
[null,"江苏省电力公司","","采集器II型（宽带载波）","采集器-设备类别:II型,采集器与集中器通信方式:电力线宽带载波,交采功能:无,温度等级:C3","台","210000","2018-04-15","买方指定仓库地面交货"]
[null,"江西省电力公司","","集中器I型远程通信单元（4G）","通信单元-通信单元类别:远程,适用终端/表类型:集中器I型,通信方式:无线公网4G,频率范围/中心频率:无,调制方式:无","只","3000","2017-09-15","买方指定仓库地面交货"]
[null,"江苏省电力公司","","采集器I型本地通信单元（宽带）","通信单元-通信单元类别:本地,适用终端/表类型:采集器I型,通信方式:宽带载波,频率范围/中心频率:2～12MHz,调制方式:OFDM","只","55000","2018-04-15","买方指定仓库地面交货"]
[null,"江苏省电力公司","","采集器I型本地通信单元（宽带）","通信单元-通信单元类别:本地,适用终端/表类型:采集器I型,通信方式:宽带载波,频率范围/中心频率:2～12MHz,调制方式:OFDM","只","38500","2018-04-15","买方指定仓库地面交货"]
[null,"江苏省电力公司","","采集器II型本地通信单元（宽带）","通信单元-通信单元类别:本地,适用终端/表类型:采集器II型,通信方式:宽带载波,频率范围/中心频率:2～12MHz,调制方式:OFDM","只","53900","2018-04-15","买方指定仓库地面交货"]
[null,"江苏省电力公司","","采集器II型本地通信单元（宽带）","通信单元-通信单元类别:本地,适用终端/表类型:采集器II型,通信方式:宽带载波,频率范围/中心频率:2～12MHz,调制方式:OFDM","只","210000","2018-04-15","买方指定仓库地面交货"]
[null,"江西省电力公司","","集中器I型（无线公网4G/宽带载波）","集中器-设备类别:I型,远程通信:4G,本地通信:电力线宽带载波,交采功能:有,温度等级:C3","台","3000","2017-09-15","买方指定仓库地面交货"]
[null,"江西省电力公司","","集中器I型本地通信单元（宽带）","通信单元-通信单元类别:本地,适用终端/表类型:集中器I型,通信方式:宽带载波,频率范围/中心频率:2～12MHz,调制方式:OFDM","只","3000","2017-09-15","买方指定仓库地面交货"]
[null,"江苏省电力公司","","采集器II型（宽带载波）","采集器-设备类别:II型,采集器与集中器通信方式:电力线宽带载波,交采功能:无,温度等级:C3","台","53900","2018-04-15","买方指定仓库地面交货"]
["包J16GW3","江苏省电力公司","","集中器I型（无线公网4G/宽带载波）","集中器-设备类别:I型,远程通信:4G,本地通信:电力线宽带载波,交采功能:有,温度等级:C3","台","7000","2018-04-15","买方指定仓库地面交货"]
[null,"江苏省电力公司","","集中器I型本地通信单元（宽带）","通信单元-通信单元类别:本地,适用终端/表类型:集中器I型,通信方式:宽带载波,频率范围/中心频率:2～12MHz,调制方式:OFDM","只","7700","2018-04-15","买方指定仓库地面交货"]
[null,"江苏省电力公司","","集中器I型远程通信单元（4G）","通信单元-通信单元类别:远程,适用终端/表类型:集中器I型,通信方式:无线公网4G,频率范围/中心频率:无,调制方式:无","只","7700","2018-04-15","买方指定仓库地面交货"]
[null,"江苏省电力公司","","采集器II型（宽带载波）","采集器-设备类别:II型,采集器与集中器通信方式:电力线宽带载波,交采功能:无,温度等级:C3","台","205000","2018-04-15","买方指定仓库地面交货"]
[null,"江苏省电力公司","","采集器II型（宽带载波）","采集器-设备类别:II型,采集器与集中器通信方式:电力线宽带载波,交采功能:无,温度等级:C3","台","90000","2018-04-15","买方指定仓库地面交货"]
[null,"江苏省电力公司","","采集器I型（宽带载波）","采集器-设备类别:I型,采集器与集中器通信方式:电力线宽带载波,交采功能:无,温度等级:C3","台","40000","2018-04-15","买方指定仓库地面交货"]
[null,"重庆市电力公司","国网重庆公司2017年营销类物资协议库存招标采购","集中器I型（无线公网4G/宽带载波）","集中器-设备类别:I型,远程通信:4G,本地通信:电力线宽带载波,交采功能:有,温度等级:C3","台","3000","2018-06-16","买方指定仓库地面交货"]
[null,"江苏省电力公司","","采集器I型本地通信单元（宽带）","通信单元-通信单元类别:本地,适用终端/表类型:采集器I型,通信方式:宽带载波,频率范围/中心频率:2～12MHz,调制方式:OFDM","只","44000","2018-04-15","买方指定仓库地面交货"]
[null,"江苏省电力公司","","采集器I型本地通信单元（宽带）","通信单元-通信单元类别:本地,适用终端/表类型:采集器I型,通信方式:宽带载波,频率范围/中心频率:2～12MHz,调制方式:OFDM","只","33000","2018-04-15","买方指定仓库地面交货"]
[null,"江苏省电力公司","","采集器II型本地通信单元（宽带）","通信单元-通信单元类别:本地,适用终端/表类型:采集器II型,通信方式:宽带载波,频率范围/中心频率:2～12MHz,调制方式:OFDM","只","90000","2018-04-15","买方指定仓库地面交货"]
[null,"江苏省电力公司","","采集器II型本地通信单元（宽带）","通信单元-通信单元类别:本地,适用终端/表类型:采集器II型,通信方式:宽带载波,频率范围/中心频率:2～12MHz,调制方式:OFDM","只","205000","2018-04-15","买方指定仓库地面交货"]
[null,"重庆市电力公司","国网重庆公司2017年营销类物资协议库存招标采购","集中器I型远程通信单元（4G）","通信单元-通信单元类别:远程,适用终端/表类型:集中器I型,通信方式:无线公网4G,频率范围/中心频率:无,调制方式:无","只","3000","2018-06-16","买方指定仓库地面交货"]
[null,"重庆市电力公司","国网重庆公司2017年营销类物资协议库存招标采购","集中器I型本地通信单元（宽带）","通信单元-通信单元类别:本地,适用终端/表类型:集中器I型,通信方式:宽带载波,频率范围/中心频率:2～12MHz,调制方式:OFDM","只","3000","2018-06-16","买方指定仓库地面交货"]
[null,"江苏省电力公司","","采集器I型（宽带载波）","采集器-设备类别:I型,采集器与集中器通信方式:电力线宽带载波,交采功能:无,温度等级:C3","台","30000","2018-04-15","买方指定仓库地面交货"]
["包J16GW4","内蒙古东部电力有限公司","","集中器I型本地通信单元（宽带）","通信单元-通信单元类别:本地,适用终端/表类型:集中器I型,通信方式:宽带载波,频率范围/中心频率:2～12MHz,调制方式:OFDM","只","100","2017-12-31","买方指定仓库地面交货"]
[null,"内蒙古东部电力有限公司","","集中器I型本地通信单元（宽带）","通信单元-通信单元类别:本地,适用终端/表类型:集中器I型,通信方式:宽带载波,频率范围/中心频率:2～12MHz,调制方式:OFDM","只","770","2017-12-31","买方指定仓库地面交货"]
[null,"内蒙古东部电力有限公司","","集中器I型本地通信单元（宽带）","通信单元-通信单元类别:本地,适用终端/表类型:集中器I型,通信方式:宽带载波,频率范围/中心频率:2～12MHz,调制方式:OFDM","只","244","2017-12-31","买方指定仓库地面交货"]
[null,"内蒙古东部电力有限公司","","集中器I型本地通信单元（宽带）","通信单元-通信单元类别:本地,适用终端/表类型:集中器I型,通信方式:宽带载波,频率范围/中心频率:2～12MHz,调制方式:OFDM","只","209","2017-12-31","买方指定仓库地面交货"]
[null,"内蒙古东部电力有限公司","","集中器I型本地通信单元（宽带）","通信单元-通信单元类别:本地,适用终端/表类型:集中器I型,通信方式:宽带载波,频率范围/中心频率:2～12MHz,调制方式:OFDM","只","4","2017-12-31","买方指定仓库地面交货"]
[null,"内蒙古东部电力有限公司","","集中器I型（无线公网4G/宽带载波）","集中器-设备类别:I型,远程通信:4G,本地通信:电力线宽带载波,交采功能:有,温度等级:C3","台","32","2017-12-31","买方指定仓库地面交货"]
[null,"内蒙古东部电力有限公司","","集中器I型（无线公网4G/宽带载波）","集中器-设备类别:I型,远程通信:4G,本地通信:电力线宽带载波,交采功能:有,温度等级:C3","台","22","2017-12-31","买方指定仓库地面交货"]
[null,"内蒙古东部电力有限公司","","集中器I型（无线公网4G/宽带载波）","集中器-设备类别:I型,远程通信:4G,本地通信:电力线宽带载波,交采功能:有,温度等级:C3","台","46","2017-12-31","买方指定仓库地面交货"]
[null,"内蒙古东部电力有限公司","","集中器I型（无线公网4G/宽带载波）","集中器-设备类别:I型,远程通信:4G,本地通信:电力线宽带载波,交采功能:有,温度等级:C3","台","200","2017-12-31","买方指定仓库地面交货"]
[null,"内蒙古东部电力有限公司","","集中器I型（无线公网4G/宽带载波）","集中器-设备类别:I型,远程通信:4G,本地通信:电力线宽带载波,交采功能:有,温度等级:C3","台","2","2017-12-31","买方指定仓库地面交货"]
[null,"内蒙古东部电力有限公司","","集中器I型（无线公网4G/宽带载波）","集中器-设备类别:I型,远程通信:4G,本地通信:电力线宽带载波,交采功能:有,温度等级:C3","台","4883","2017-12-31","买方指定仓库地面交货"]
[null,"内蒙古东部电力有限公司","","集中器I型（无线公网4G/宽带载波）","集中器-设备类别:I型,远程通信:4G,本地通信:电力线宽带载波,交采功能:有,温度等级:C3","台","1400","2017-12-31","买方指定仓库地面交货"]
[null,"内蒙古东部电力有限公司","","集中器I型（无线公网4G/宽带载波）","集中器-设备类别:I型,远程通信:4G,本地通信:电力线宽带载波,交采功能:有,温度等级:C3","台","69","2017-12-31","买方指定仓库地面交货"]
[null,"内蒙古东部电力有限公司","","集中器I型（无线公网4G/宽带载波）","集中器-设备类别:I型,远程通信:4G,本地通信:电力线宽带载波,交采功能:有,温度等级:C3","台","733","2017-12-31","买方指定仓库地面交货"]
[null,"内蒙古东部电力有限公司","","集中器I型（无线公网4G/宽带载波）","集中器-设备类别:I型,远程通信:4G,本地通信:电力线宽带载波,交采功能:有,温度等级:C3","台","244","2017-12-31","买方指定仓库地面交货"]
[null,"内蒙古东部电力有限公司","","集中器I型（无线公网4G/宽带载波）","集中器-设备类别:I型,远程通信:4G,本地通信:电力线宽带载波,交采功能:有,温度等级:C3","台","199","2017-12-31","买方指定仓库地面交货"]
[null,"内蒙古东部电力有限公司","","集中器I型（无线公网4G/宽带载波）","集中器-设备类别:I型,远程通信:4G,本地通信:电力线宽带载波,交采功能:有,温度等级:C3","台","4","2017-12-31","买方指定仓库地面交货"]
[null,"内蒙古东部电力有限公司","","集中器I型（无线公网4G/宽带载波）","集中器-设备类别:I型,远程通信:4G,本地通信:电力线宽带载波,交采功能:有,温度等级:C3","台","463","2017-12-31","买方指定仓库地面交货"]
[null,"内蒙古东部电力有限公司","","集中器I型本地通信单元（宽带）","通信单元-通信单元类别:本地,适用终端/表类型:集中器I型,通信方式:宽带载波,频率范围/中心频率:2～12MHz,调制方式:OFDM","只","32","2017-12-31","买方指定仓库地面交货"]
[null,"内蒙古东部电力有限公司","","集中器I型本地通信单元（宽带）","通信单元-通信单元类别:本地,适用终端/表类型:集中器I型,通信方式:宽带载波,频率范围/中心频率:2～12MHz,调制方式:OFDM","只","22","2017-12-31","买方指定仓库地面交货"]
[null,"内蒙古东部电力有限公司","","集中器I型本地通信单元（宽带）","通信单元-通信单元类别:本地,适用终端/表类型:集中器I型,通信方式:宽带载波,频率范围/中心频率:2～12MHz,调制方式:OFDM","只","46","2017-12-31","买方指定仓库地面交货"]
[null,"内蒙古东部电力有限公司","","集中器I型本地通信单元（宽带）","通信单元-通信单元类别:本地,适用终端/表类型:集中器I型,通信方式:宽带载波,频率范围/中心频率:2～12MHz,调制方式:OFDM","只","100","2017-12-31","买方指定仓库地面交货"]
[null,"内蒙古东部电力有限公司","","集中器I型本地通信单元（宽带）","通信单元-通信单元类别:本地,适用终端/表类型:集中器I型,通信方式:宽带载波,频率范围/中心频率:2～12MHz,调制方式:OFDM","只","200","2017-12-31","买方指定仓库地面交货"]
[null,"内蒙古东部电力有限公司","","集中器I型本地通信单元（宽带）","通信单元-通信单元类别:本地,适用终端/表类型:集中器I型,通信方式:宽带载波,频率范围/中心频率:2～12MHz,调制方式:OFDM","只","4883","2017-12-31","买方指定仓库地面交货"]
[null,"内蒙古东部电力有限公司","","集中器I型本地通信单元（宽带）","通信单元-通信单元类别:本地,适用终端/表类型:集中器I型,通信方式:宽带载波,频率范围/中心频率:2～12MHz,调制方式:OFDM","只","1474","2017-12-31","买方指定仓库地面交货"]
[null,"内蒙古东部电力有限公司","","集中器I型本地通信单元（宽带）","通信单元-通信单元类别:本地,适用终端/表类型:集中器I型,通信方式:宽带载波,频率范围/中心频率:2～12MHz,调制方式:OFDM","只","20","2017-12-31","买方指定仓库地面交货"]
[null,"内蒙古东部电力有限公司","","集中器I型本地通信单元（宽带）","通信单元-通信单元类别:本地,适用终端/表类型:集中器I型,通信方式:宽带载波,频率范围/中心频率:2～12MHz,调制方式:OFDM","只","487","2017-12-31","买方指定仓库地面交货"]
[null,"河南省电力公司","","集中器I型本地通信单元（宽带）","通信单元-通信单元类别:本地,适用终端/表类型:集中器I型,通信方式:宽带载波,频率范围/中心频率:2～12MHz,调制方式:OFDM","只","11000","2018-04-10","买方指定仓库地面交货"]
[null,"河南省电力公司","","集中器I型远程通信单元（4G）","通信单元-通信单元类别:远程,适用终端/表类型:集中器I型,通信方式:无线公网4G,频率范围/中心频率:无,调制方式:无","只","11000","2018-04-10","买方指定仓库地面交货"]
[null,"河南省电力公司","","集中器I型（无线公网4G/宽带载波）","集中器-设备类别:I型,远程通信:4G,本地通信:电力线宽带载波,交采功能:有,温度等级:C3","台","10000","2018-04-10","买方指定仓库地面交货"]
[null,"山西省电力公司","","集中器I型（无线公网4G/宽带载波）","集中器-设备类别:I型,远程通信:4G,本地通信:电力线宽带载波,交采功能:有,温度等级:C3","台","25977","2018-04-30","买方指定仓库地面交货"]
[null,"山西省电力公司","","集中器I型远程通信单元（4G）","通信单元-通信单元类别:远程,适用终端/表类型:集中器I型,通信方式:无线公网4G,频率范围/中心频率:无,调制方式:无","只","25977","2018-04-30","买方指定仓库地面交货"]
[null,"内蒙古东部电力有限公司","","集中器I型（无线公网GPRS/宽带载波）","集中器-设备类别:I型,远程通信:GPRS,本地通信:电力线宽带载波,交采功能:有,温度等级:C3","台","308","2017-12-31","买方指定仓库地面交货"]
[null,"内蒙古东部电力有限公司","","集中器I型本地通信单元（宽带）","通信单元-通信单元类别:本地,适用终端/表类型:集中器I型,通信方式:宽带载波,频率范围/中心频率:2～12MHz,调制方式:OFDM","只","69","2017-12-31","买方指定仓库地面交货"]
[null,"内蒙古东部电力有限公司","","集中器I型本地通信单元（宽带）","通信单元-通信单元类别:本地,适用终端/表类型:集中器I型,通信方式:宽带载波,频率范围/中心频率:2～12MHz,调制方式:OFDM","只","100","2017-12-31","买方指定仓库地面交货"]
["包J16JS1","江苏省电力公司","","采集器II型本地通信单元（宽带）","通信单元-通信单元类别:本地,适用终端/表类型:采集器II型,通信方式:宽带载波,频率范围/中心频率:2～12MHz,调制方式:OFDM","只","250000","2018-04-15","买方指定仓库地面交货"]
[null,"江苏省电力公司","","集中器I型（无线公网4G/宽带载波）","集中器-设备类别:I型,远程通信:4G,本地通信:电力线宽带载波,交采功能:有,温度等级:C3","台","5000","2018-04-15","买方指定仓库地面交货"]
[null,"江苏省电力公司","","集中器I型远程通信单元（4G）","通信单元-通信单元类别:远程,适用终端/表类型:集中器I型,通信方式:无线公网4G,频率范围/中心频率:无,调制方式:无","只","5500","2018-04-15","买方指定仓库地面交货"]
[null,"江苏省电力公司","","采集器II型本地通信单元（宽带）","通信单元-通信单元类别:本地,适用终端/表类型:采集器II型,通信方式:宽带载波,频率范围/中心频率:2～12MHz,调制方式:OFDM","只","175000","2018-04-15","买方指定仓库地面交货"]
[null,"江苏省电力公司","","集中器I型本地通信单元（宽带）","通信单元-通信单元类别:本地,适用终端/表类型:集中器I型,通信方式:宽带载波,频率范围/中心频率:2～12MHz,调制方式:OFDM","只","5500","2018-04-15","买方指定仓库地面交货"]
[null,"江苏省电力公司","","采集器II型（宽带载波）","采集器-设备类别:II型,采集器与集中器通信方式:电力线宽带载波,交采功能:无,温度等级:C3","台","250000","2018-04-15","买方指定仓库地面交货"]
[null,"江苏省电力公司","","采集器II型（宽带载波）","采集器-设备类别:II型,采集器与集中器通信方式:电力线宽带载波,交采功能:无,温度等级:C3","台","175000","2018-04-15","买方指定仓库地面交货"]
["包J16JS2","江苏省电力公司","","采集器II型（宽带载波）","采集器-设备类别:II型,采集器与集中器通信方式:电力线宽带载波,交采功能:无,温度等级:C3","台","180000","2018-04-15","买方指定仓库地面交货"]
[null,"江苏省电力公司","","采集器II型（宽带载波）","采集器-设备类别:II型,采集器与集中器通信方式:电力线宽带载波,交采功能:无,温度等级:C3","台","235000","2018-04-15","买方指定仓库地面交货"]
[null,"江苏省电力公司","","集中器I型（无线公网4G/宽带载波）","集中器-设备类别:I型,远程通信:4G,本地通信:电力线宽带载波,交采功能:有,温度等级:C3","台","5500","2018-04-15","买方指定仓库地面交货"]
[null,"江苏省电力公司","","集中器I型本地通信单元（宽带）","通信单元-通信单元类别:本地,适用终端/表类型:集中器I型,通信方式:宽带载波,频率范围/中心频率:2～12MHz,调制方式:OFDM","只","6050","2018-04-15","买方指定仓库地面交货"]
[null,"江苏省电力公司","","采集器II型本地通信单元（宽带）","通信单元-通信单元类别:本地,适用终端/表类型:采集器II型,通信方式:宽带载波,频率范围/中心频率:2～12MHz,调制方式:OFDM","只","180000","2018-04-15","买方指定仓库地面交货"]
[null,"江苏省电力公司","","采集器II型本地通信单元（宽带）","通信单元-通信单元类别:本地,适用终端/表类型:采集器II型,通信方式:宽带载波,频率范围/中心频率:2～12MHz,调制方式:OFDM","只","235000","2018-04-15","买方指定仓库地面交货"]
[null,"江苏省电力公司","","集中器I型远程通信单元（4G）","通信单元-通信单元类别:远程,适用终端/表类型:集中器I型,通信方式:无线公网4G,频率范围/中心频率:无,调制方式:无","只","6050","2018-04-15","买方指定仓库地面交货"]
["包J16JS3","江苏省电力公司","","采集器II型（宽带载波）","采集器-设备类别:II型,采集器与集中器通信方式:电力线宽带载波,交采功能:无,温度等级:C3","台","200000","2018-04-15","买方指定仓库地面交货"]
[null,"江苏省电力公司","","采集器II型（宽带载波）","采集器-设备类别:II型,采集器与集中器通信方式:电力线宽带载波,交采功能:无,温度等级:C3","台","195000","2018-04-15","买方指定仓库地面交货"]
[null,"江苏省电力公司","","集中器I型（无线公网4G/宽带载波）","集中器-设备类别:I型,远程通信:4G,本地通信:电力线宽带载波,交采功能:有,温度等级:C3","台","6800","2018-04-15","买方指定仓库地面交货"]
[null,"江苏省电力公司","","集中器I型本地通信单元（宽带）","通信单元-通信单元类别:本地,适用终端/表类型:集中器I型,通信方式:宽带载波,频率范围/中心频率:2～12MHz,调制方式:OFDM","只","7480","2018-04-15","买方指定仓库地面交货"]
[null,"江苏省电力公司","","采集器II型本地通信单元（宽带）","通信单元-通信单元类别:本地,适用终端/表类型:采集器II型,通信方式:宽带载波,频率范围/中心频率:2～12MHz,调制方式:OFDM","只","195000","2018-04-15","买方指定仓库地面交货"]
[null,"江苏省电力公司","","采集器II型本地通信单元（宽带）","通信单元-通信单元类别:本地,适用终端/表类型:采集器II型,通信方式:宽带载波,频率范围/中心频率:2～12MHz,调制方式:OFDM","只","200000","2018-04-15","买方指定仓库地面交货"]
[null,"江苏省电力公司","","集中器I型远程通信单元（4G）","通信单元-通信单元类别:远程,适用终端/表类型:集中器I型,通信方式:无线公网4G,频率范围/中心频率:无,调制方式:无","只","7480","2018-04-15","买方指定仓库地面交货"]
["包J16JS4","江苏省电力公司","","集中器I型本地通信单元（宽带）","通信单元-通信单元类别:本地,适用终端/表类型:集中器I型,通信方式:宽带载波,频率范围/中心频率:2～12MHz,调制方式:OFDM","只","4400","2018-04-15","买方指定仓库地面交货"]
[null,"江苏省电力公司","","采集器II型本地通信单元（宽带）","通信单元-通信单元类别:本地,适用终端/表类型:采集器II型,通信方式:宽带载波,频率范围/中心频率:2～12MHz,调制方式:OFDM","只","245000","2018-04-15","买方指定仓库地面交货"]
[null,"江苏省电力公司","","集中器I型远程通信单元（4G）","通信单元-通信单元类别:远程,适用终端/表类型:集中器I型,通信方式:无线公网4G,频率范围/中心频率:无,调制方式:无","只","4400","2018-04-15","买方指定仓库地面交货"]
[null,"江苏省电力公司","","采集器II型（宽带载波）","采集器-设备类别:II型,采集器与集中器通信方式:电力线宽带载波,交采功能:无,温度等级:C3","台","245000","2018-04-15","买方指定仓库地面交货"]
[null,"江苏省电力公司","","采集器II型（宽带载波）","采集器-设备类别:II型,采集器与集中器通信方式:电力线宽带载波,交采功能:无,温度等级:C3","台","190000","2018-04-15","买方指定仓库地面交货"]
[null,"江苏省电力公司","","采集器II型本地通信单元（宽带）","通信单元-通信单元类别:本地,适用终端/表类型:采集器II型,通信方式:宽带载波,频率范围/中心频率:2～12MHz,调制方式:OFDM","只","190000","2018-04-15","买方指定仓库地面交货"]
[null,"江苏省电力公司","","集中器I型（无线公网4G/宽带载波）","集中器-设备类别:I型,远程通信:4G,本地通信:电力线宽带载波,交采功能:有,温度等级:C3","台","4000","2018-04-15","买方指定仓库地面交货"]
["包J16JS5","江苏省电力公司","","集中器I型远程通信单元（4G）","通信单元-通信单元类别:远程,适用终端/表类型:集中器I型,通信方式:无线公网4G,频率范围/中心频率:无,调制方式:无","只","4950","2018-04-15","买方指定仓库地面交货"]
[null,"江苏省电力公司","","集中器I型本地通信单元（宽带）","通信单元-通信单元类别:本地,适用终端/表类型:集中器I型,通信方式:宽带载波,频率范围/中心频率:2～12MHz,调制方式:OFDM","只","4950","2018-04-15","买方指定仓库地面交货"]
[null,"江苏省电力公司","","集中器I型（无线公网4G/宽带载波）","集中器-设备类别:I型,远程通信:4G,本地通信:电力线宽带载波,交采功能:有,温度等级:C3","台","4500","2018-04-15","买方指定仓库地面交货"]
[null,"江苏省电力公司","","采集器II型（宽带载波）","采集器-设备类别:II型,采集器与集中器通信方式:电力线宽带载波,交采功能:无,温度等级:C3","台","185000","2018-04-15","买方指定仓库地面交货"]
[null,"江苏省电力公司","","采集器II型（宽带载波）","采集器-设备类别:II型,采集器与集中器通信方式:电力线宽带载波,交采功能:无,温度等级:C3","台","240000","2018-04-15","买方指定仓库地面交货"]
[null,"江苏省电力公司","","采集器II型本地通信单元（宽带）","通信单元-通信单元类别:本地,适用终端/表类型:采集器II型,通信方式:宽带载波,频率范围/中心频率:2～12MHz,调制方式:OFDM","只","240000","2018-04-15","买方指定仓库地面交货"]
[null,"江苏省电力公司","","采集器II型本地通信单元（宽带）","通信单元-通信单元类别:本地,适用终端/表类型:采集器II型,通信方式:宽带载波,频率范围/中心频率:2～12MHz,调制方式:OFDM","只","185000","2018-04-15","买方指定仓库地面交货"]
["包J16JS6","江苏省电力公司","","集中器I型（无线公网4G/宽带载波）","集中器-设备类别:I型,远程通信:4G,本地通信:电力线宽带载波,交采功能:有,温度等级:C3","台","8000","2018-04-15","买方指定仓库地面交货"]
[null,"江苏省电力公司","","集中器I型本地通信单元（宽带）","通信单元-通信单元类别:本地,适用终端/表类型:集中器I型,通信方式:宽带载波,频率范围/中心频率:2～12MHz,调制方式:OFDM","只","8800","2018-04-15","买方指定仓库地面交货"]
[null,"江苏省电力公司","","集中器I型远程通信单元（4G）","通信单元-通信单元类别:远程,适用终端/表类型:集中器I型,通信方式:无线公网4G,频率范围/中心频率:无,调制方式:无","只","8800","2018-04-15","买方指定仓库地面交货"]
[null,"江苏省电力公司","","采集器II型（宽带载波）","采集器-设备类别:II型,采集器与集中器通信方式:电力线宽带载波,交采功能:无,温度等级:C3","台","225000","2018-04-15","买方指定仓库地面交货"]
[null,"江苏省电力公司","","采集器II型（宽带载波）","采集器-设备类别:II型,采集器与集中器通信方式:电力线宽带载波,交采功能:无,温度等级:C3","台","145000","2018-04-15","买方指定仓库地面交货"]
[null,"江苏省电力公司","","采集器II型本地通信单元（宽带）","通信单元-通信单元类别:本地,适用终端/表类型:采集器II型,通信方式:宽带载波,频率范围/中心频率:2～12MHz,调制方式:OFDM","只","225000","2018-04-15","买方指定仓库地面交货"]
[null,"江苏省电力公司","","采集器II型本地通信单元（宽带）","通信单元-通信单元类别:本地,适用终端/表类型:采集器II型,通信方式:宽带载波,频率范围/中心频率:2～12MHz,调制方式:OFDM","只","145000","2018-04-15","买方指定仓库地面交货"]
["包J16JS7","江苏省电力公司","","采集器II型（宽带载波）","采集器-设备类别:II型,采集器与集中器通信方式:电力线宽带载波,交采功能:无,温度等级:C3","台","170000","2018-04-15","买方指定仓库地面交货"]
[null,"江苏省电力公司","","采集器II型（宽带载波）","采集器-设备类别:II型,采集器与集中器通信方式:电力线宽带载波,交采功能:无,温度等级:C3","台","220000","2018-04-15","买方指定仓库地面交货"]
[null,"江苏省电力公司","","集中器I型远程通信单元（4G）","通信单元-通信单元类别:远程,适用终端/表类型:集中器I型,通信方式:无线公网4G,频率范围/中心频率:无,调制方式:无","只","7150","2018-04-15","买方指定仓库地面交货"]
[null,"江苏省电力公司","","集中器I型本地通信单元（宽带）","通信单元-通信单元类别:本地,适用终端/表类型:集中器I型,通信方式:宽带载波,频率范围/中心频率:2～12MHz,调制方式:OFDM","只","7150","2018-04-15","买方指定仓库地面交货"]
[null,"江苏省电力公司","","集中器I型（无线公网4G/宽带载波）","集中器-设备类别:I型,远程通信:4G,本地通信:电力线宽带载波,交采功能:有,温度等级:C3","台","6500","2018-04-15","买方指定仓库地面交货"]
[null,"江苏省电力公司","","采集器II型本地通信单元（宽带）","通信单元-通信单元类别:本地,适用终端/表类型:采集器II型,通信方式:宽带载波,频率范围/中心频率:2～12MHz,调制方式:OFDM","只","220000","2018-04-15","买方指定仓库地面交货"]
[null,"江苏省电力公司","","采集器II型本地通信单元（宽带）","通信单元-通信单元类别:本地,适用终端/表类型:采集器II型,通信方式:宽带载波,频率范围/中心频率:2～12MHz,调制方式:OFDM","只","170000","2018-04-15","买方指定仓库地面交货"]
["包J16JS8","江苏省电力公司","","采集器II型（宽带载波）","采集器-设备类别:II型,采集器与集中器通信方式:电力线宽带载波,交采功能:无,温度等级:C3","台","110000","2018-04-15","买方指定仓库地面交货"]
[null,"江苏省电力公司","","采集器II型（宽带载波）","采集器-设备类别:II型,采集器与集中器通信方式:电力线宽带载波,交采功能:无,温度等级:C3","台","230000","2018-04-15","买方指定仓库地面交货"]
[null,"江苏省电力公司","","集中器I型本地通信单元（宽带）","通信单元-通信单元类别:本地,适用终端/表类型:集中器I型,通信方式:宽带载波,频率范围/中心频率:2～12MHz,调制方式:OFDM","只","10450","2018-04-15","买方指定仓库地面交货"]
[null,"江苏省电力公司","","采集器II型本地通信单元（宽带）","通信单元-通信单元类别:本地,适用终端/表类型:采集器II型,通信方式:宽带载波,频率范围/中心频率:2～12MHz,调制方式:OFDM","只","110000","2018-04-15","买方指定仓库地面交货"]
[null,"江苏省电力公司","","采集器II型本地通信单元（宽带）","通信单元-通信单元类别:本地,适用终端/表类型:采集器II型,通信方式:宽带载波,频率范围/中心频率:2～12MHz,调制方式:OFDM","只","230000","2018-04-15","买方指定仓库地面交货"]
[null,"江苏省电力公司","","集中器I型远程通信单元（4G）","通信单元-通信单元类别:远程,适用终端/表类型:集中器I型,通信方式:无线公网4G,频率范围/中心频率:无,调制方式:无","只","10450","2018-04-15","买方指定仓库地面交货"]
[null,"江苏省电力公司","","集中器I型（无线公网4G/宽带载波）","集中器-设备类别:I型,远程通信:4G,本地通信:电力线宽带载波,交采功能:有,温度等级:C3","台","9500","2018-04-15","买方指定仓库地面交货"]
["包J16JS9","江苏省电力公司","","采集器I型（宽带载波）","采集器-设备类别:I型,采集器与集中器通信方式:电力线宽带载波,交采功能:无,温度等级:C3","台","45000","2018-04-15","买方指定仓库地面交货"]
[null,"江苏省电力公司","","采集器I型（宽带载波）","采集器-设备类别:I型,采集器与集中器通信方式:电力线宽带载波,交采功能:无,温度等级:C3","台","21600","2018-04-15","买方指定仓库地面交货"]
[null,"江苏省电力公司","","采集器II型本地通信单元（宽带）","通信单元-通信单元类别:本地,适用终端/表类型:采集器II型,通信方式:宽带载波,频率范围/中心频率:2～12MHz,调制方式:OFDM","只","165000","2018-04-15","买方指定仓库地面交货"]
[null,"江苏省电力公司","","集中器I型本地通信单元（宽带）","通信单元-通信单元类别:本地,适用终端/表类型:集中器I型,通信方式:宽带载波,频率范围/中心频率:2～12MHz,调制方式:OFDM","只","6600","2018-04-15","买方指定仓库地面交货"]
[null,"江苏省电力公司","","采集器II型（宽带载波）","采集器-设备类别:II型,采集器与集中器通信方式:电力线宽带载波,交采功能:无,温度等级:C3","台","160000","2018-04-15","买方指定仓库地面交货"]
[null,"江苏省电力公司","","采集器II型（宽带载波）","采集器-设备类别:II型,采集器与集中器通信方式:电力线宽带载波,交采功能:无,温度等级:C3","台","165000","2018-04-15","买方指定仓库地面交货"]
[null,"江苏省电力公司","","集中器I型远程通信单元（4G）","通信单元-通信单元类别:远程,适用终端/表类型:集中器I型,通信方式:无线公网4G,频率范围/中心频率:无,调制方式:无","只","6600","2018-04-15","买方指定仓库地面交货"]
[null,"江苏省电力公司","","集中器I型（无线公网4G/宽带载波）","集中器-设备类别:I型,远程通信:4G,本地通信:电力线宽带载波,交采功能:有,温度等级:C3","台","6000","2018-04-15","买方指定仓库地面交货"]
[null,"江苏省电力公司","","采集器II型本地通信单元（宽带）","通信单元-通信单元类别:本地,适用终端/表类型:采集器II型,通信方式:宽带载波,频率范围/中心频率:2～12MHz,调制方式:OFDM","只","160000","2018-04-15","买方指定仓库地面交货"]
[null,"江苏省电力公司","","采集器I型本地通信单元（宽带）","通信单元-通信单元类别:本地,适用终端/表类型:采集器I型,通信方式:宽带载波,频率范围/中心频率:2～12MHz,调制方式:OFDM","只","49500","2018-04-15","买方指定仓库地面交货"]
[null,"江苏省电力公司","","采集器I型本地通信单元（宽带）","通信单元-通信单元类别:本地,适用终端/表类型:采集器I型,通信方式:宽带载波,频率范围/中心频率:2～12MHz,调制方式:OFDM","只","23760","2018-04-15","买方指定仓库地面交货"]

{"sheet":"专变采集终端","index":5,"n_rows":154,"n_cols":9,"rows_kept":154,"merged":[[0,0,0,8],[1,0,1,8],[3,0,4,0],[5,0,12,0],[13,0,14,0],[15,0,16,0],[17,0,18,0],[19,0,22,0],[23,0,29,0],[30,0,50,0],[51,0,52,0],[53,0,54,0],[55,0,56,0],[57,0,58,0],[59,0,60,0],[61,0,62,0],[63,0,64,0],[65,0,66,0],[67,0,68,0],[69,0,70,0],[71,0,76,0],[77,0,80,0],[81,0,151,0],[152,0,153,0]],"flags":["formulas_cached_only"]}
["国家电网公司2017年第一次电能表及用电信息采集设备招标活动\n货物需求一览表\n(专变采集终端)"]
["分标编号:0711-17OTL03922000-6"]
["包号","项目单位","项目名称","招标货物","物资描述","单位","行数量","交货日期","交货地点"]
["包Z1GW1","江苏省电力公司","","专变采集终端I型（无线专网230M）","专变采集终端-设备类别:I型,远程通信:无线专网,交采功能:有,I/O配置:8,温度等级:C3","套","12000","2018-04-15","买方指定仓库地面交货"]
[null,"黑龙江省电力有限公司","","专变采集终端I型（无线专网230M）","专变采集终端-设备类别:I型,远程通信:无线专网,交采功能:有,I/O配置:8,温度等级:C3","套","1404","2018-04-20","买方指定仓库地面交货"]
["包Z1GW2","辽宁省电力有限公司","","专变采集终端I型（无线专网230M）","专变采集终端-设备类别:I型,远程通信:无线专网,交采功能:有,I/O配置:8,温度等级:C3","套","200","2017-08-31","买方指定仓库地面交货"]
[null,"辽宁省电力有限公司","","专变采集终端I型（无线专网230M）","专变采集终端-设备类别:I型,远程通信:无线专网,交采功能:有,I/O配置:8,温度等级:C3","套","100","2017-09-15","买方指定仓库地面交货"]
[null,"江苏省电力公司","","专变采集终端I型（无线专网230M）","专变采集终端-设备类别:I型,远程通信:无线专网,交采功能:有,I/O配置:8,温度等级:C3","套","11000","2018-04-15","买方指定仓库地面交货"]
[null,"辽宁省电力有限公司","","专变采集终端I型（无线专网230M）","专变采集终端-设备类别:I型,远程通信:无线专网,交采功能:有,I/O配置:8,温度等级:C3","套","100","2017-07-20","买方指定仓库地面交货"]
[null,"辽宁省电力有限公司","","专变采集终端I型（无线专网230M）","专变采集终端-设备类别:I型,远程通信:无线专网,交采功能:有,I/O配置:8,温度等级:C3","套","100","2017-07-20","买方指定仓库地面交货"]
[null,"辽宁省电力有限公司","","专变采集终端I型（无线专网230M）","专变采集终端-设备类别:I型,远程通信:无线专网,交采功能:有,I/O配置:8,温度等级:C3","套","300","2017-08-20","买方指定仓库地面交货"]
[null,"辽宁省电力有限公司","","专变采集终端I型（无线专网230M）","专变采集终端-设备类别:I型,远程通信:无线专网,交采功能:有,I/O配置:8,温度等级:C3","套","70","2017-09-21","买方指定仓库地面交货"]
[null,"辽宁省电力有限公司","","专变采集终端I型（无线专网230M）","专变采集终端-设备类别:I型,远程通信:无线专网,交采功能:有,I/O配置:8,温度等级:C3","套","175","2017-07-25","买方指定仓库地面交货"]
["包Z1GW3","陕西省电力公司","","专变采集终端I型（无线专网230M）","专变采集终端-设备类别:I型,远程通信:无线专网,交采功能:有,I/O配置:8,温度等级:C3","套","2000","2018-06-30","买方指定仓库地面交货"]
[null,"江苏省电力公司","","专变采集终端I型（无线专网230M）","专变采集终端-设备类别:I型,远程通信:无线专网,交采功能:有,I/O配置:8,温度等级:C3","套","9000","2018-04-15","买方指定仓库地面交货"]
["包Z1GW4","天津市电力公司","","专变采集终端I型（无线专网230M）","专变采集终端-设备类别:I型,远程通信:无线专网,交采功能:有,I/O配置:8,温度等级:C3","套","1500","2017-12-31","买方指定仓库地面交货"]
[null,"江苏省电力公司","","专变采集终端I型（无线专网230M）","专变采集终端-设备类别:I型,远程通信:无线专网,交采功能:有,I/O配置:8,温度等级:C3","套","8000","2018-04-15","买方指定仓库地面交货"]
["包Z1JS1","江苏省电力公司","","专变采集终端I型（无线专网230M）","专变采集终端-设备类别:I型,远程通信:无线专网,交采功能:有,I/O配置:8,温度等级:C3","套","7000","2018-04-15","买方指定仓库地面交货"]
[null,"江苏省电力公司","","专变采集终端I型（无线专网230M）","专变采集终端-设备类别:I型,远程通信:无线专网,交采功能:有,I/O配置:8,温度等级:C3","套","6000","2018-04-15","买方指定仓库地面交货"]
["包Z5JS1","江苏省电力公司","","专变采集终端II型（无线公网GPRS）","专变采集终端-设备类别:II型,远程通信:GPRS,交采功能:无,I/O配置:4,温度等级:C3","套","4500","2018-04-15","买方指定仓库地面交货"]
[null,"江苏省电力公司","","专变采集终端II型（无线公网GPRS）","专变采集终端-设备类别:II型,远程通信:GPRS,交采功能:无,I/O配置:4,温度等级:C3","套","5000","2018-04-15","买方指定仓库地面交货"]
[null,"江苏省电力公司","","专变采集终端II型（无线公网GPRS）","专变采集终端-设备类别:II型,远程通信:GPRS,交采功能:无,I/O配置:4,温度等级:C3","套","5500","2018-04-15","买方指定仓库地面交货"]
[null,"江苏省电力公司","","专变采集终端II型（无线公网GPRS）","专变采集终端-设备类别:II型,远程通信:GPRS,交采功能:无,I/O配置:4,温度等级:C3","套","4000","2018-04-15","买方指定仓库地面交货"]
["包Z7GW1","西藏电力有限公司","国网西藏电力有限公司各供电公司营销专项、电网基建/户表","专变采集终端III型（无线公网CDMA）","专变采集终端-设备类别:III型,远程通信:CDMA,交采功能:有,I/O配置:2,温度等级:C3","套","3790","2017-06-30","买方指定仓库地面交货"]
[null,"西藏电力有限公司","国网西藏电力有限公司各供电公司营销专项、电网基建/户表","专变III型远程通信单元（GPRS）","通信单元-通信单元类别:远程,适用终端/表类型:专变III型,通信方式:无线公网GPRS,频率范围/中心频率:无,调制方式:无","只","500","2017-07-30","买方指定仓库地面交货"]
[null,"江西省电力公司","","专变采集终端III型（无线公网GPRS）","专变采集终端-设备类别:III型,远程通信:GPRS,交采功能:有,I/O配置:2,温度等级:C3","套","28000","2017-09-15","买方指定仓库地面交货"]
[null,"江西省电力公司","","专变III型远程通信单元（GPRS）","通信单元-通信单元类别:远程,适用终端/表类型:专变III型,通信方式:无线公网GPRS,频率范围/中心频率:无,调制方式:无","只","28000","2017-09-15","买方指定仓库地面交货"]
[null,"江西省电力公司","","专变III型远程通信单元（CDMA）","通信单元-通信单元类别:远程,适用终端/表类型:专变III型,通信方式:无线公网CDMA,频率范围/中心频率:无,调制方式:无","只","3000","2017-09-15","买方指定仓库地面交货"]
[null,"西藏电力有限公司","国网西藏电力有限公司各供电公司营销专项、电网基建/户表","专变III型远程通信单元（CDMA）","通信单元-通信单元类别:远程,适用终端/表类型:专变III型,通信方式:无线公网CDMA,频率范围/中心频率:无,调制方式:无","只","3290","2017-07-30","买方指定仓库地面交货"]
[null,"江西省电力公司","","专变采集终端III型（无线公网CDMA）","专变采集终端-设备类别:III型,远程通信:CDMA,交采功能:有,I/O配置:2,温度等级:C3","套","3000","2017-09-15","买方指定仓库地面交货"]
["包Z7GW2","内蒙古东部电力有限公司","","专变III型远程通信单元（GPRS）","通信单元-通信单元类别:远程,适用终端/表类型:专变III型,通信方式:无线公网GPRS,频率范围/中心频率:无,调制方式:无","只","33","2017-12-31","买方指定仓库地面交货"]
[null,"内蒙古东部电力有限公司","","专变III型远程通信单元（GPRS）","通信单元-通信单元类别:远程,适用终端/表类型:专变III型,通信方式:无线公网GPRS,频率范围/中心频率:无,调制方式:无","只","6","2017-12-31","买方指定仓库地面交货"]
[null,"内蒙古东部电力有限公司","","专变III型远程通信单元（GPRS）","通信单元-通信单元类别:远程,适用终端/表类型:专变III型,通信方式:无线公网GPRS,频率范围/中心频率:无,调制方式:无","只","2","2017-12-31","施工现场地面交货"]
[null,"内蒙古东部电力有限公司","","专变III型远程通信单元（GPRS）","通信单元-通信单元类别:远程,适用终端/表类型:专变III型,通信方式:无线公网GPRS,频率范围/中心频率:无,调制方式:无","只","26","2017-12-31","买方指定仓库地面交货"]
[null,"内蒙古东部电力有限公司","","专变III型远程通信单元（GPRS）","通信单元-通信单元类别:远程,适用终端/表类型:专变III型,通信方式:无线公网GPRS,频率范围/中心频率:无,调制方式:无","只","1","2017-12-31","买方指定仓库地面交货"]
[null,"内蒙古东部电力有限公司","","专变III型远程通信单元（GPRS）","通信单元-通信单元类别:远程,适用终端/表类型:专变III型,通信方式:无线公网GPRS,频率范围/中心频率:无,调制方式:无","只","12","2017-12-31","买方指定仓库地面交货"]
[null,"山东电力集团公司","","专变III型远程通信单元（4G）","通信单元-通信单元类别:远程,适用终端/表类型:专变III型,通信方式:无线公网4G,频率范围/中心频率:无,调制方式:无","只","30990","2018-06-30","买方指定仓库地面交货"]
[null,"山东电力集团公司","","专变采集终端III型（无线公网GPRS）","专变采集终端-设备类别:III型,远程通信:GPRS,交采功能:有,I/O配置:2,温度等级:C3","套","30990","2018-06-30","买方指定仓库地面交货"]
[null,"内蒙古东部电力有限公司","","专变III型远程通信单元（GPRS）","通信单元-通信单元类别:远程,适用终端/表类型:专变III型,通信方式:无线公网GPRS,频率范围/中心频率:无,调制方式:无","只","17","2017-12-31","买方指定仓库地面交货"]
[null,"内蒙古东部电力有限公司","","专变采集终端III型（无线公网GPRS）","专变采集终端-设备类别:III型,远程通信:GPRS,交采功能:有,I/O配置:2,温度等级:C3","套","12","2017-12-31","买方指定仓库地面交货"]
[null,"内蒙古东部电力有限公司","","专变采集终端III型（无线公网GPRS）","专变采集终端-设备类别:III型,远程通信:GPRS,交采功能:有,I/O配置:2,温度等级:C3","套","54","2017-12-31","买方指定仓库地面交货"]
[null,"内蒙古东部电力有限公司","","专变采集终端III型（无线公网GPRS）","专变采集终端-设备类别:III型,远程通信:GPRS,交采功能:有,I/O配置:2,温度等级:C3","套","26","2017-12-31","买方指定仓库地面交货"]
[null,"内蒙古东部电力有限公司","","专变采集终端III型（无线公网GPRS）","专变采集终端-设备类别:III型,远程通信:GPRS,交采功能:有,I/O配置:2,温度等级:C3","套","2","2017-12-31","施工现场地面交货"]
[null,"内蒙古东部电力有限公司","","专变采集终端III型（无线公网GPRS）","专变采集终端-设备类别:III型,远程通信:GPRS,交采功能:有,I/O配置:2,温度等级:C3","套","6","2017-12-31","买方指定仓库地面交货"]
[null,"内蒙古东部电力有限公司","","专变采集终端III型（无线公网GPRS）","专变采集终端-设备类别:III型,远程通信:GPRS,交采功能:有,I/O配置:2,温度等级:C3","套","2","2017-12-31","买方指定仓库地面交货"]
[null,"内蒙古东部电力有限公司","","专变采集终端III型（无线公网GPRS）","专变采集终端-设备类别:III型,远程通信:GPRS,交采功能:有,I/O配置:2,温度等级:C3","套","33","2017-12-31","买方指定仓库地面交货"]
[null,"内蒙古东部电力有限公司","","专变采集终端III型（无线公网GPRS）","专变采集终端-设备类别:III型,远程通信:GPRS,交采功能:有,I/O配置:2,温度等级:C3","套","8","2017-12-31","买方指定仓库地面交货"]
[null,"内蒙古东部电力有限公司","","专变采集终端III型（无线公网GPRS）","专变采集终端-设备类别:III型,远程通信:GPRS,交采功能:有,I/O配置:2,温度等级:C3","套","13","2017-12-31","买方指定仓库地面交货"]
[null,"内蒙古东部电力有限公司","","专变采集终端III型（无线公网GPRS）","专变采集终端-设备类别:III型,远程通信:GPRS,交采功能:有,I/O配置:2,温度等级:C3","套","8","2017-12-31","买方指定仓库地面交货"]
[null,"内蒙古东部电力有限公司","","专变采集终端III型（无线公网GPRS）","专变采集终端-设备类别:III型,远程通信:GPRS,交采功能:有,I/O配置:2,温度等级:C3","套","17","2017-12-31","买方指定仓库地面交货"]
[null,"内蒙古东部电力有限公司","","专变III型远程通信单元（GPRS）","通信单元-通信单元类别:远程,适用终端/表类型:专变III型,通信方式:无线公网GPRS,频率范围/中心频率:无,调制方式:无","只","8","2017-12-31","买方指定仓库地面交货"]
["包Z7HL1","黑龙江省电力有限公司","","专变采集终端III型（无线公网GPRS）","专变采集终端-设备类别:III型,远程通信:GPRS,交采功能:有,I/O配置:2,温度等级:C3","套","22619","2018-04-20","买方指定仓库地面交货"]
[null,"黑龙江省电力有限公司","","专变III型远程通信单元（4G）","通信单元-通信单元类别:远程,适用终端/表类型:专变III型,通信方式:无线公网4G,频率范围/中心频率:无,调制方式:无","只","22619","2018-04-20","买方指定仓库地面交货"]
["包Z7SD1","山东电力集团公司","","专变III型远程通信单元（4G）","通信单元-通信单元类别:远程,适用终端/表类型:专变III型,通信方式:无线公网4G,频率范围/中心频率:无,调制方式:无","只","31030","2018-06-30","买方指定仓库地面交货"]
[null,"山东电力集团公司","","专变采集终端III型（无线公网GPRS）","专变采集终端-设备类别:III型,远程通信:GPRS,交采功能:有,I/O配置:2,温度等级:C3","套","31030","2018-06-30","买方指定仓库地面交货"]
["包Z7SD2","山东电力集团公司","","专变III型远程通信单元（4G）","通信单元-通信单元类别:远程,适用终端/表类型:专变III型,通信方式:无线公网4G,频率范围/中心频率:无,调制方式:无","只","31030","2018-06-30","买方指定仓库地面交货"]
[null,"山东电力集团公司","","专变采集终端III型（无线公网GPRS）","专变采集终端-设备类别:III型,远程通信:GPRS,交采功能:有,I/O配置:2,温度等级:C3","套","31030","2018-06-30","买方指定仓库地面交货"]
["包Z7SD3","山东电力集团公司","","专变III型远程通信单元（4G）","通信单元-通信单元类别:远程,适用终端/表类型:专变III型,通信方式:无线公网4G,频率范围/中心频率:无,调制方式:无","只","31030","2018-06-30","买方指定仓库地面交货"]
[null,"山东电力集团公司","","专变采集终端III型（无线公网GPRS）","专变采集终端-设备类别:III型,远程通信:GPRS,交采功能:有,I/O配置:2,温度等级:C3","套","31030","2018-06-30","买方指定仓库地面交货"]
["包Z7SD4","山东电力集团公司","","专变采集终端III型（无线公网GPRS）","专变采集终端-设备类别:III型,远程通信:GPRS,交采功能:有,I/O配置:2,温度等级:C3","套","31030","2018-06-30","买方指定仓库地面交货"]
[null,"山东电力集团公司","","专变III型远程通信单元（4G）","通信单元-通信单元类别:远程,适用终端/表类型:专变III型,通信方式:无线公网4G,频率范围/中心频率:无,调制方式:无","只","31030","2018-06-30","买方指定仓库地面交货"]
["包Z7SD5","山东电力集团公司","","专变采集终端III型（无线公网GPRS）","专变采集终端-设备类别:III型,远程通信:GPRS,交采功能:有,I/O配置:2,温度等级:C3","套","31030","2018-06-30","买方指定仓库地面交货"]
[null,"山东电力集团公司","","专变III型远程通信单元（4G）","通信单元-通信单元类别:远程,适用终端/表类型:专变III型,通信方式:无线公网4G,频率范围/中心频率:无,调制方式:无","只","31030","2018-06-30","买方指定仓库地面交货"]
["包Z7SD6","山东电力集团公司","","专变III型远程通信单元（4G）","通信单元-通信单元类别:远程,适用终端/表类型:专变III型,通信方式:无线公网4G,频率范围/中心频率:无,调制方式:无","只","31030","2018-06-30","买方指定仓库地面交货"]
[null,"山东电力集团公司","","专变采集终端III型（无线公网GPRS）","专变采集终端-设备类别:III型,远程通信:GPRS,交采功能:有,I/O配置:2,温度等级:C3","套","31030","2018-06-30","买方指定仓库地面交货"]
["包Z7SD7","山东电力集团公司","","专变采集终端III型（无线公网GPRS）","专变采集终端-设备类别:III型,远程通信:GPRS,交采功能:有,I/O配置:2,温度等级:C3","套","31030","2018-06-30","买方指定仓库地面交货"]
[null,"山东电力集团公司","","专变III型远程通信单元（4G）","通信单元-通信单元类别:远程,适用终端/表类型:专变III型,通信方式:无线公网4G,频率范围/中心频率:无,调制方式:无","只","31030","2018-06-30","买方指定仓库地面交货"]
["包Z7SD8","山东电力集团公司","","专变III型远程通信单元（4G）","通信单元-通信单元类别:远程,适用终端/表类型:专变III型,通信方式:无线公网4G,频率范围/中心频率:无,调制方式:无","只","31030","2018-06-30","买方指定仓库地面交货"]
[null,"山东电力集团公司","","专变采集终端III型（无线公网GPRS）","专变采集终端-设备类别:III型,远程通信:GPRS,交采功能:有,I/O配置:2,温度等级:C3","套","31030","2018-06-30","买方指定仓库地面交货"]
["包Z7SD9","山东电力集团公司","","专变采集终端III型（无线公网GPRS）","专变采集终端-设备类别:III型,远程通信:GPRS,交采功能:有,I/O配置:2,温度等级:C3","套","31030","2018-06-30","买方指定仓库地面交货"]
[null,"山东电力集团公司","","专变III型远程通信单元（4G）","通信单元-通信单元类别:远程,适用终端/表类型:专变III型,通信方式:无线公网4G,频率范围/中心频率:无,调制方式:无","只","31030","2018-06-30","买方指定仓库地面交货"]
["包Z11GW1","重庆市电力公司","国网重庆公司2017年营销类物资协议库存招标采购","专变采集终端III型（无线公网4G）","专变采集终端-设备类别:III型,远程通信:4G,交采功能:有,I/O配置:2,温度等级:C3","套","7500","2018-06-16","买方指定仓库地面交货"]
[null,"安徽省电力公司","","专变采集终端III型（无线公网4G）","专变采集终端-设备类别:III型,远程通信:4G,交采功能:有,I/O配置:2,温度等级:C3","套","13500","2017-07-10","买方指定仓库地面交货"]
[null,"陕西省电力公司","","专变III型远程通信单元（4G）","通信单元-通信单元类别:远程,适用终端/表类型:专变III型,通信方式:无线公网4G,频率范围/中心频率:无,调制方式:无","只","13000","2018-06-30","买方指定仓库地面交货"]
[null,"陕西省电力公司","","专变采集终端III型（无线公网4G）","专变采集终端-设备类别:III型,远程通信:4G,交采功能:有,I/O配置:2,温度等级:C3","套","13000","2018-06-30","买方指定仓库地面交货"]
[null,"重庆市电力公司","国网重庆公司2017年营销类物资协议库存招标采购","专变III型远程通信单元（4G）","通信单元-通信单元类别:远程,适用终端/表类型:专变III型,通信方式:无线公网4G,频率范围/中心频率:无,调制方式:无","只","7500","2018-06-16","买方指定仓库地面交货"]
[null,"安徽省电力公司","","专变III型远程通信单元（4G）","通信单元-通信单元类别:远程,适用终端/表类型:专变III型,通信方式:无线公网4G,频率范围/中心频率:无,调制方式:无","只","13500","2017-07-10","买方指定仓库地面交货"]
["包Z11GW2","河南省电力公司","","专变III型远程通信单元（4G）","通信单元-通信单元类别:远程,适用终端/表类型:专变III型,通信方式:无线公网4G,频率范围/中心频率:无,调制方式:无","只","11000","2018-04-10","买方指定仓库地面交货"]
[null,"山西省电力公司","","专变采集终端III型（无线公网4G）","专变采集终端-设备类别:III型,远程通信:4G,交采功能:有,I/O配置:2,温度等级:C3","套","21588","2018-04-30","买方指定仓库地面交货"]
[null,"山西省电力公司","","专变III型远程通信单元（4G）","通信单元-通信单元类别:远程,适用终端/表类型:专变III型,通信方式:无线公网4G,频率范围/中心频率:无,调制方式:无","只","21588","2018-04-30","买方指定仓库地面交货"]
[null,"河南省电力公司","","专变采集终端III型（无线公网4G）","专变采集终端-设备类别:III型,远程通信:4G,交采功能:有,I/O配置:2,温度等级:C3","套","10000","2018-04-10","买方指定仓库地面交货"]
["包Z11GW3","辽宁省电力有限公司","","专变III型远程通信单元（4G）","通信单元-通信单元类别:远程,适用终端/表类型:专变III型,通信方式:无线公网4G,频率范围/中心频率:无,调制方式:无","只","2100","2017-09-22","买方指定仓库地面交货"]
[null,"辽宁省电力有限公司","","专变采集终端III型（无线公网4G）","专变采集终端-设备类别:III型,远程通信:4G,交采功能:有,I/O配置:2,温度等级:C3","套","550","2017-08-20","买方指定仓库地面交货"]
[null,"辽宁省电力有限公司","","专变采集终端III型（无线公网4G）","专变采集终端-设备类别:III型,远程通信:4G,交采功能:有,I/O配置:2,温度等级:C3","套","233","2017-07-24","买方指定仓库地面交货"]
[null,"辽宁省电力有限公司","","专变III型远程通信单元（4G）","通信单元-通信单元类别:远程,适用终端/表类型:专变III型,通信方式:无线公网4G,频率范围/中心频率:无,调制方式:无","只","233","2017-07-24","买方指定仓库地面交货"]
[null,"辽宁省电力有限公司","","专变III型远程通信单元（4G）","通信单元-通信单元类别:远程,适用终端/表类型:专变III型,通信方式:无线公网4G,频率范围/中心频率:无,调制方式:无","只","750","2017-08-22","买方指定仓库地面交货"]
[null,"辽宁省电力有限公司","","专变采集终端III型（无线公网4G）","专变采集终端-设备类别:III型,远程通信:4G,交采功能:有,I/O配置:2,温度等级:C3","套","500","2017-08-22","买方指定仓库地面交货"]
[null,"辽宁省电力有限公司","","专变采集终端III型（无线公网4G）","专变采集终端-设备类别:III型,远程通信:4G,交采功能:有,I/O配置:2,温度等级:C3","套","600","2017-07-25","买方指定仓库地面交货"]
[null,"辽宁省电力有限公司","","专变采集终端III型（无线公网4G）","专变采集终端-设备类别:III型,远程通信:4G,交采功能:有,I/O配置:2,温度等级:C3","套","300","2017-07-20","买方指定仓库地面交货"]
[null,"辽宁省电力有限公司","","专变III型远程通信单元（4G）","通信单元-通信单元类别:远程,适用终端/表类型:专变III型,通信方式:无线公网4G,频率范围/中心频率:无,调制方式:无","只","500","2017-08-20","买方指定仓库地面交货"]
[null,"辽宁省电力有限公司","","专变采集终端III型（无线公网4G）","专变采集终端-设备类别:III型,远程通信:4G,交采功能:有,I/O配置:2,温度等级:C3","套","249","2017-08-20","买方指定仓库地面交货"]
[null,"辽宁省电力有限公司","","专变III型远程通信单元（4G）","通信单元-通信单元类别:远程,适用终端/表类型:专变III型,通信方式:无线公网4G,频率范围/中心频率:无,调制方式:无","只","204","2017-08-20","买方指定仓库地面交货"]
[null,"辽宁省电力有限公司","","专变采集终端III型（无线公网4G）","专变采集终端-设备类别:III型,远程通信:4G,交采功能:有,I/O配置:2,温度等级:C3","套","500","2017-09-18","买方指定仓库地面交货"]
[null,"辽宁省电力有限公司","","专变III型远程通信单元（4G）","通信单元-通信单元类别:远程,适用终端/表类型:专变III型,通信方式:无线公网4G,频率范围/中心频率:无,调制方式:无","只","300","2017-07-20","买方指定仓库地面交货"]
[null,"辽宁省电力有限公司","","专变III型远程通信单元（4G）","通信单元-通信单元类别:远程,适用终端/表类型:专变III型,通信方式:无线公网4G,频率范围/中心频率:无,调制方式:无","只","600","2017-08-23","买方指定仓库地面交货"]
[null,"辽宁省电力有限公司","","专变采集终端III型（无线公网4G）","专变采集终端-设备类别:III型,远程通信:4G,交采功能:有,I/O配置:2,温度等级:C3","套","600","2017-08-23","买方指定仓库地面交货"]
[null,"辽宁省电力有限公司","","专变采集终端III型（无线公网4G）","专变采集终端-设备类别:III型,远程通信:4G,交采功能:有,I/O配置:2,温度等级:C3","套","1500","2017-09-15","买方指定仓库地面交货"]
[null,"辽宁省电力有限公司","","专变采集终端III型（无线公网4G）","专变采集终端-设备类别:III型,远程通信:4G,交采功能:有,I/O配置:2,温度等级:C3","套","96","2017-08-20","买方指定仓库地面交货"]
[null,"辽宁省电力有限公司","","专变III型远程通信单元（4G）","通信单元-通信单元类别:远程,适用终端/表类型:专变III型,通信方式:无线公网4G,频率范围/中心频率:无,调制方式:无","只","96","2017-08-25","买方指定仓库地面交货"]
[null,"辽宁省电力有限公司","","专变III型远程通信单元（4G）","通信单元-通信单元类别:远程,适用终端/表类型:专变III型,通信方式:无线公网4G,频率范围/中心频率:无,调制方式:无","只","500","2017-09-18","买方指定仓库地面交货"]
[null,"辽宁省电力有限公司","","专变采集终端III型（无线公网4G）","专变采集终端-设备类别:III型,远程通信:4G,交采功能:有,I/O配置:2,温度等级:C3","套","204","2017-08-20","买方指定仓库地面交货"]
[null,"内蒙古东部电力有限公司","","专变采集终端III型（无线公网4G）","专变采集终端-设备类别:III型,远程通信:4G,交采功能:有,I/O配置:2,温度等级:C3","套","48","2017-12-31","买方指定仓库地面交货"]
[null,"内蒙古东部电力有限公司","","专变采集终端III型（无线公网4G）","专变采集终端-设备类别:III型,远程通信:4G,交采功能:有,I/O配置:2,温度等级:C3","套","3","2017-12-31","买方指定仓库地面交货"]
[null,"内蒙古东部电力有限公司","","专变采集终端III型（无线公网4G）","专变采集终端-设备类别:III型,远程通信:4G,交采功能:有,I/O配置:2,温度等级:C3","套","21","2017-12-31","买方指定仓库地面交货"]
[null,"内蒙古东部电力有限公司","","专变采集终端III型（无线公网4G）","专变采集终端-设备类别:III型,远程通信:4G,交采功能:有,I/O配置:2,温度等级:C3","套","854","2017-12-31","买方指定仓库地面交货"]
[null,"内蒙古东部电力有限公司","","专变采集终端III型（无线公网4G）","专变采集终端-设备类别:III型,远程通信:4G,交采功能:有,I/O配置:2,温度等级:C3","套","1","2017-12-31","买方指定仓库地面交货"]
[null,"内蒙古东部电力有限公司","","专变采集终端III型（无线公网4G）","专变采集终端-设备类别:III型,远程通信:4G,交采功能:有,I/O配置:2,温度等级:C3","套","41","2017-12-31","买方指定仓库地面交货"]
[null,"内蒙古东部电力有限公司","","专变采集终端III型（无线公网4G）","专变采集终端-设备类别:III型,远程通信:4G,交采功能:有,I/O配置:2,温度等级:C3","套","67","2017-12-31","买方指定仓库地面交货"]
[null,"内蒙古东部电力有限公司","","专变采集终端III型（无线公网4G）","专变采集终端-设备类别:III型,远程通信:4G,交采功能:有,I/O配置:2,温度等级:C3","套","158","2017-12-31","买方指定仓库地面交货"]
[null,"内蒙古东部电力有限公司","","专变III型远程通信单元（4G）","通信单元-通信单元类别:远程,适用终端/表类型:专变III型,通信方式:无线公网4G,频率范围/中心频率:无,调制方式:无","只","897","2017-12-31","买方指定仓库地面交货"]
[null,"内蒙古东部电力有限公司","","专变III型远程通信单元（4G）","通信单元-通信单元类别:远程,适用终端/表类型:专变III型,通信方式:无线公网4G,频率范围/中心频率:无,调制方式:无","只","1","2017-12-31","买方指定仓库地面交货"]
[null,"辽宁省电力有限公司","","专变III型远程通信单元（4G）","通信单元-通信单元类别:远程,适用终端/表类型:专变III型,通信方式:无线公网4G,频率范围/中心频率:无,调制方式:无","只","600","2017-07-25","买方指定仓库地面交货"]
[null,"辽宁省电力有限公司","","专变III型远程通信单元（4G）","通信单元-通信单元类别:远程,适用终端/表类型:专变III型,通信方式:无线公网4G,频率范围/中心频率:无,调制方式:无","只","450","2017-09-21","买方指定仓库地面交货"]
[null,"辽宁省电力有限公司","","专变采集终端III型（无线公网4G）","专变采集终端-设备类别:III型,远程通信:4G,交采功能:有,I/O配置:2,温度等级:C3","套","500","2017-07-20","买方指定仓库地面交货"]
[null,"辽宁省电力有限公司","","专变III型远程通信单元（4G）","通信单元-通信单元类别:远程,适用终端/表类型:专变III型,通信方式:无线公网4G,频率范围/中心频率:无,调制方式:无","只","500","2017-07-20","买方指定仓库地面交货"]
[null,"辽宁省电力有限公司","","专变III型远程通信单元（4G）","通信单元-通信单元类别:远程,适用终端/表类型:专变III型,通信方式:无线公网4G,频率范围/中心频率:无,调制方式:无","只","1500","2017-09-15","买方指定仓库地面交货"]
[null,"内蒙古东部电力有限公司","","专变采集终端III型（无线公网4G）","专变采集终端-设备类别:III型,远程通信:4G,交采功能:有,I/O配置:2,温度等级:C3","套","423","2017-12-31","买方指定仓库地面交货"]
[null,"内蒙古东部电力有限公司","","专变采集终端III型（无线公网4G）","专变采集终端-设备类别:III型,远程通信:4G,交采功能:有,I/O配置:2,温度等级:C3","套","20","2017-12-31","买方指定仓库地面交货"]
[null,"内蒙古东部电力有限公司","","专变采集终端III型（无线公网4G）","专变采集终端-设备类别:III型,远程通信:4G,交采功能:有,I/O配置:2,温度等级:C3","套","4500","2017-12-31","买方指定仓库地面交货"]
[null,"内蒙古东部电力有限公司","","专变采集终端III型（无线公网4G）","专变采集终端-设备类别:III型,远程通信:4G,交采功能:有,I/O配置:2,温度等级:C3","套","4254","2017-12-31","买方指定仓库地面交货"]
[null,"内蒙古东部电力有限公司","","专变采集终端III型（无线公网4G）","专变采集终端-设备类别:III型,远程通信:4G,交采功能:有,I/O配置:2,温度等级:C3","套","11","2017-12-31","买方指定仓库地面交货"]
[null,"内蒙古东部电力有限公司","","专变采集终端III型（无线公网4G）","专变采集终端-设备类别:III型,远程通信:4G,交采功能:有,I/O配置:2,温度等级:C3","套","1459","2017-12-31","买方指定仓库地面交货"]
[null,"内蒙古东部电力有限公司","","专变采集终端III型（无线公网4G）","专变采集终端-设备类别:III型,远程通信:4G,交采功能:有,I/O配置:2,温度等级:C3","套","15","2017-12-31","买方指定仓库地面交货"]
[null,"内蒙古东部电力有限公司","","专变采集终端III型（无线公网4G）","专变采集终端-设备类别:III型,远程通信:4G,交采功能:有,I/O配置:2,温度等级:C3","套","164","2017-12-31","买方指定仓库地面交货"]
[null,"内蒙古东部电力有限公司","","专变采集终端III型（无线公网4G）","专变采集终端-设备类别:III型,远程通信:4G,交采功能:有,I/O配置:2,温度等级:C3","套","42","2017-12-31","买方指定仓库地面交货"]
[null,"内蒙古东部电力有限公司","","专变采集终端III型（无线公网4G）","专变采集终端-设备类别:III型,远程通信:4G,交采功能:有,I/O配置:2,温度等级:C3","套","12","2017-12-31","买方指定仓库地面交货"]
[null,"内蒙古东部电力有限公司","","专变采集终端III型（无线公网4G）","专变采集终端-设备类别:III型,远程通信:4G,交采功能:有,I/O配置:2,温度等级:C3","套","7","2017-12-31","买方指定仓库地面交货"]
[null,"内蒙古东部电力有限公司","","专变采集终端III型（无线公网4G）","专变采集终端-设备类别:III型,远程通信:4G,交采功能:有,I/O配置:2,温度等级:C3","套","4","2017-12-31","买方指定仓库地面交货"]
[null,"内蒙古东部电力有限公司","","专变III型远程通信单元（4G）","通信单元-通信单元类别:远程,适用终端/表类型:专变III型,通信方式:无线公网4G,频率范围/中心频率:无,调制方式:无","只","12","2017-12-31","买方指定仓库地面交货"]
[null,"内蒙古东部电力有限公司","","专变III型远程通信单元（4G）","通信单元-通信单元类别:远程,适用终端/表类型:专变III型,通信方式:无线公网4G,频率范围/中心频率:无,调制方式:无","只","200","2017-12-31","买方指定仓库地面交货"]
[null,"内蒙古东部电力有限公司","","专变III型远程通信单元（4G）","通信单元-通信单元类别:远程,适用终端/表类型:专变III型,通信方式:无线公网4G,频率范围/中心频率:无,调制方式:无","只","1532","2017-12-31","买方指定仓库地面交货"]
[null,"内蒙古东部电力有限公司","","专变III型远程通信单元（4G）","通信单元-通信单元类别:远程,适用终端/表类型:专变III型,通信方式:无线公网4G,频率范围/中心频率:无,调制方式:无","只","15","2017-12-31","买方指定仓库地面交货"]
[null,"内蒙古东部电力有限公司","","专变III型远程通信单元（4G）","通信单元-通信单元类别:远程,适用终端/表类型:专变III型,通信方式:无线公网4G,频率范围/中心频率:无,调制方式:无","只","164","2017-12-31","买方指定仓库地面交货"]
[null,"内蒙古东部电力有限公司","","专变III型远程通信单元（4G）","通信单元-通信单元类别:远程,适用终端/表类型:专变III型,通信方式:无线公网4G,频率范围/中心频率:无,调制方式:无","只","42","2017-12-31","买方指定仓库地面交货"]
[null,"内蒙古东部电力有限公司","","专变III型远程通信单元（4G）","通信单元-通信单元类别:远程,适用终端/表类型:专变III型,通信方式:无线公网4G,频率范围/中心频率:无,调制方式:无","只","200","2017-12-31","买方指定仓库地面交货"]
[null,"内蒙古东部电力有限公司","","专变III型远程通信单元（4G）","通信单元-通信单元类别:远程,适用终端/表类型:专变III型,通信方式:无线公网4G,频率范围/中心频率:无,调制方式:无","只","48","2017-12-31","买方指定仓库地面交货"]
[null,"内蒙古东部电力有限公司","","专变III型远程通信单元（4G）","通信单元-通信单元类别:远程,适用终端/表类型:专变III型,通信方式:无线公网4G,频率范围/中心频率:无,调制方式:无","只","50","2017-12-31","买方指定仓库地面交货"]
[null,"内蒙古东部电力有限公司","","专变III型远程通信单元（4G）","通信单元-通信单元类别:远程,适用终端/表类型:专变III型,通信方式:无线公网4G,频率范围/中心频率:无,调制方式:无","只","21","2017-12-31","买方指定仓库地面交货"]
[null,"内蒙古东部电力有限公司","","专变III型远程通信单元（4G）","通信单元-通信单元类别:远程,适用终端/表类型:专变III型,通信方式:无线公网4G,频率范围/中心频率:无,调制方式:无","只","200","2017-12-31","买方指定仓库地面交货"]
[null,"内蒙古东部电力有限公司","","专变III型远程通信单元（4G）","通信单元-通信单元类别:远程,适用终端/表类型:专变III型,通信方式:无线公网4G,频率范围/中心频率:无,调制方式:无","只","7","2017-12-31","买方指定仓库地面交货"]
[null,"内蒙古东部电力有限公司","","专变III型远程通信单元（4G）","通信单元-通信单元类别:远程,适用终端/表类型:专变III型,通信方式:无线公网4G,频率范围/中心频率:无,调制方式:无","只","4","2017-12-31","买方指定仓库地面交货"]
[null,"内蒙古东部电力有限公司","","专变III型远程通信单元（4G）","通信单元-通信单元类别:远程,适用终端/表类型:专变III型,通信方式:无线公网4G,频率范围/中心频率:无,调制方式:无","只","41","2017-12-31","买方指定仓库地面交货"]
[null,"内蒙古东部电力有限公司","","专变III型远程通信单元（4G）","通信单元-通信单元类别:远程,适用终端/表类型:专变III型,通信方式:无线公网4G,频率范围/中心频率:无,调制方式:无","只","67","2017-12-31","买方指定仓库地面交货"]
[null,"内蒙古东部电力有限公司","","专变III型远程通信单元（4G）","通信单元-通信单元类别:远程,适用终端/表类型:专变III型,通信方式:无线公网4G,频率范围/中心频率:无,调制方式:无","只","266","2017-12-31","买方指定仓库地面交货"]
[null,"内蒙古东部电力有限公司","","专变III型远程通信单元（4G）","通信单元-通信单元类别:远程,适用终端/表类型:专变III型,通信方式:无线公网4G,频率范围/中心频率:无,调制方式:无","只","50","2017-12-31","买方指定仓库地面交货"]
[null,"内蒙古东部电力有限公司","","专变III型远程通信单元（4G）","通信单元-通信单元类别:远程,适用终端/表类型:专变III型,通信方式:无线公网4G,频率范围/中心频率:无,调制方式:无","只","445","2017-12-31","买方指定仓库地面交货"]
[null,"内蒙古东部电力有限公司","","专变III型远程通信单元（4G）","通信单元-通信单元类别:远程,适用终端/表类型:专变III型,通信方式:无线公网4G,频率范围/中心频率:无,调制方式:无","只","20","2017-12-31","买方指定仓库地面交货"]
[null,"内蒙古东部电力有限公司","","专变III型远程通信单元（4G）","通信单元-通信单元类别:远程,适用终端/表类型:专变III型,通信方式:无线公网4G,频率范围/中心频率:无,调制方式:无","只","4725","2017-12-31","买方指定仓库地面交货"]
[null,"内蒙古东部电力有限公司","","专变III型远程通信单元（4G）","通信单元-通信单元类别:远程,适用终端/表类型:专变III型,通信方式:无线公网4G,频率范围/中心频率:无,调制方式:无","只","4470","2017-12-31","买方指定仓库地面交货"]
[null,"辽宁省电力有限公司","","专变III型远程通信单元（4G）","通信单元-通信单元类别:远程,适用终端/表类型:专变III型,通信方式:无线公网4G,频率范围/中心频率:无,调制方式:无","只","1207","2017-08-25","买方指定仓库地面交货"]
[null,"辽宁省电力有限公司","","专变采集终端III型（无线公网4G）","专变采集终端-设备类别:III型,远程通信:4G,交采功能:有,I/O配置:2,温度等级:C3","套","1207","2017-08-25","买方指定仓库地面交货"]
[null,"辽宁省电力有限公司","","专变采集终端III型（无线公网4G）","专变采集终端-设备类别:III型,远程通信:4G,交采功能:有,I/O配置:2,温度等级:C3","套","700","2017-08-21","买方指定仓库地面交货"]
["包Z11HE1","河北省电力公司","","专变III型远程通信单元（4G）","通信单元-通信单元类别:远程,适用终端/表类型:专变III型,通信方式:无线公网4G,频率范围/中心频率:无,调制方式:无","只","35000","2018-03-31","买方指定仓库地面交货"]
[null,"河北省电力公司","","专变采集终端III型（无线公网4G）","专变采集终端-设备类别:III型,远程通信:4G,交采功能:有,I/O配置:2,温度等级:C3","套","35000","2018-03-31","买方指定仓库地面交货"]